|  |  |
| --- | --- |
| 3GPP TS 29.537 V18.3.0 (2023-12) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Core Network and Terminals;  5G System; Multicast/Broadcast Policy Control Services;  Stage 3  (Release 18) | |
|  | |
|  | 3GPP-logo_web |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 6

1 Scope 8

2 References 8

3 Definitions, symbols and abbreviations 9

3.1 Definitions 9

3.2 Symbols 9

3.3 Abbreviations 9

4 Overview 9

5 Services offered by the PCF 10

5.1 Introduction 10

5.2 Npcf\_MBSPolicyControl Service 11

5.2.1 Service Description 11

5.2.2 Service Operations 11

5.2.2.1 Introduction 11

5.2.2.2 Npcf\_MBSPoliyControl\_Create 11

5.2.2.2.1 General 11

5.2.2.2.2 MBS Policy Association Establishment 11

5.2.2.3 Npcf\_MBSPolicyControl\_Update 14

5.2.2.3.1 General 14

5.2.2.3.2 MBS Policy Association Update 14

5.2.2.4 Npcf\_MBSPolicyControl\_Delete 16

5.2.2.4.1 General 16

5.2.2.4.2 MBS Policy Association Deletion 16

5.2.3 MBS Policy Decision Management 16

5.2.3.1 General 16

5.2.3.1.1 MBS PCC Rule definition 17

5.2.3.1.2 MBS QoS Decision 18

5.2.3.1.3 MBS QoS Characteristics 18

5.2.3.1.4 MBS Session-AMBR 18

5.2.3.1.5 MBS Policy Control Request Triggers 19

5.2.3.2 Provisioning and enforcement of MBS Policy Decisions 19

5.2.3.2.1 General 19

5.2.3.2.2 Provisioning and enforcement of MBS PCC rules 19

5.2.3.2.3 Provisioning and enforcement of authorized MBS QoS for an MBS service data flow 19

5.2.3.2.4 Provisioning and enforcement of authorized MBS Session-AMBR 20

5.2.3.2.5 Provisioning and enforcement of MBS Policy Control Request Triggers 20

5.2.4 MBS Policy Error Handling 21

5.2.4.1 MBS Policy Error Reporting 21

5.3 Npcf\_MBSPolicyAuthorization Service 22

5.3.1 Service Description 22

5.3.2 Service Operations 22

5.3.2.1 Introduction 22

5.3.2.2 Npcf\_MBSPoliyAuthorization\_Create 22

5.3.2.2.1 General 22

5.3.2.2.2 MBS Application Session Context Establishment 22

5.3.2.3 Npcf\_MBSPoliyAuthorization\_Update 24

5.3.2.3.1 General 24

5.3.2.3.2 MBS Application Session Context Update 24

5.3.2.4 Npcf\_MBSPoliyAuthorization\_Delete 25

5.3.2.4.1 General 25

5.3.2.4.2 MBS Application Session Context Deletion 26

6 API Definitions 27

6.1 Npcf\_MBSPolicyControl Service API 27

6.1.1 Introduction 27

6.1.2 Usage of HTTP 27

6.1.2.1 General 27

6.1.2.2 HTTP standard headers 27

6.1.2.2.1 General 27

6.1.2.2.2 Content type 27

6.1.2.3 HTTP custom headers 27

6.1.3 Resources 28

6.1.3.1 Overview 28

6.1.3.2 Resource: MBS Policies 28

6.1.3.2.1 Description 28

6.1.3.2.2 Resource Definition 28

6.1.3.2.3 Resource Standard Methods 29

6.1.3.2.3.1 POST 29

6.1.3.2.4 Resource Custom Operations 30

6.1.3.3 Resource: Individual MBS Policy 30

6.1.3.3.1 Description 30

6.1.3.3.2 Resource Definition 30

6.1.3.3.3 Resource Standard Methods 30

6.1.3.3.3.1 GET 30

6.1.3.3.3.2 DELETE 31

6.1.3.3.4 Resource Custom Operations 32

6.1.3.3.4.1 Overview 32

6.1.3.3.4.2 Operation: Update 33

6.1.4 Custom Operations without associated resources 34

6.1.5 Notifications 34

6.1.6 Data Model 34

6.1.6.1 General 34

6.1.6.2 Structured data types 35

6.1.6.2.1 Introduction 35

6.1.6.2.2 Type: MbsPolicyCtxtData 35

6.1.6.2.3 Type: MbsPolicyDecision 36

6.1.6.2.4 Type: MbsPolicyData 36

6.1.6.2.5 Void 37

6.1.6.2.6 Void 37

6.1.6.2.7 Type: MbsPccRule 37

6.1.6.2.8 Type: MbsQosDec 38

6.1.6.2.9 Type: MbsQosChar 39

6.1.6.2.10 Type: MbsErrorReport 39

6.1.6.2.11 Type: MbsPolicyCtxtDataUpdate 39

6.1.6.2.12 Type: MbsReport 40

6.1.6.3 Simple data types and enumerations 40

6.1.6.3.1 Introduction 40

6.1.6.3.2 Simple data types 40

6.1.6.3.3 Enumeration: MbsPcrt 40

6.1.6.3.4 Enumeration: MbsFailureCode 41

6.1.6.3.5 Enumeration: MbsPccRuleStatus 41

6.1.6.4 Data types describing alternative data types or combinations of data types 41

6.1.6.5 Binary data 42

6.1.6.5.1 Binary Data Types 42

6.1.7 Error Handling 42

6.1.7.1 General 42

6.1.7.2 Protocol Errors 42

6.1.7.3 Application Errors 42

6.1.8 Feature negotiation 43

6.1.9 Security 43

6.2 Npcf\_MBSPolicyAuthorization Service API 44

6.2.1 Introduction 44

6.2.2 Usage of HTTP 44

6.2.2.1 General 44

6.2.2.2 HTTP standard headers 44

6.2.2.2.1 General 44

6.2.2.2.2 Content type 44

6.2.2.3 HTTP custom headers 44

6.2.3 Resources 45

6.2.3.1 Overview 45

6.2.3.2 Resource: MBS Application Session Contexts 45

6.2.3.2.1 Description 45

6.2.3.2.2 Resource Definition 45

6.2.3.2.3 Resource Standard Methods 46

6.2.3.2.3.1 POST 46

6.2.3.2.4 Resource Custom Operations 46

6.2.3.3 Resource: Individual MBS Application Session Context 47

6.2.3.3.1 Description 47

6.2.3.3.2 Resource Definition 47

6.2.3.3.3 Resource Standard Methods 47

6.2.3.3.3.1 GET 47

6.2.3.3.3.2 PATCH 48

6.2.3.3.3.3 DELETE 49

6.2.3.3.4 Resource Custom Operations 51

6.2.4 Custom Operations without associated resources 51

6.2.5 Notifications 51

6.2.6 Data Model 51

6.2.6.1 General 51

6.2.6.2 Structured data types 51

6.2.6.2.1 Introduction 51

6.2.6.2.2 Type: MbsAppSessionCtxt 52

6.2.6.2.3 Type: MbsAppSessionCtxtPatch 53

6.2.6.2.4 Type: AcceptableMbsServInfo 53

6.2.6.3 Simple data types and enumerations 53

6.2.6.3.1 Introduction 53

6.2.6.3.2 Simple data types 53

6.2.6.4 Data types describing alternative data types or combinations of data types 54

6.2.6.4.1 Type: MbsExtProblemDetails 54

6.2.6.5 Binary data 54

6.2.6.5.1 Binary Data Types 54

6.2.7 Error Handling 54

6.2.7.1 General 54

6.2.7.2 Protocol Errors 54

6.2.7.3 Application Errors 54

6.2.8 Feature negotiation 55

6.2.9 Security 55

Annex A (normative): OpenAPI specification 56

A.1 General 56

A.2 Npcf\_MBSPolicyControl API 57

A.3 Npcf\_MBSPolicyAuthorization API 64

Annex B (informative): Withdrawn API versions 68

B.1 General 68

B.2 Npcf\_MBSPolicyControl API 68

B.3 Npcf\_MBSPolicyAuthorization API 68

Annex C (informative): Change history 69

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" are not substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The present document specifies the stage 3 protocol and data model for the Service Based Interfaces of the Multicast/Broadcast Policy Control Services. It provides stage 3 protocol definitions and message flows, and specifies the APIs of the Multicast/Broadcast Services provided by the PCF.

The 5G System stage 2 architecture and procedures are specified in 3GPP TS 23.501 [2] and 3GPP TS 23.502 [3]. The stage 2 architecture and procedures for 5G Multicast/Broadcast Services are specified in 3GPP TS 23.247 [14].

The Technical Realization of the Service Based Architecture and the Principles and Guidelines for Services Definition are specified in 3GPP TS 29.500 [4] and 3GPP TS 29.501 [5].

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[3] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[4] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[5] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[6] OpenAPI: "OpenAPI Specification Version 3.0.0", <https://spec.openapis.org/oas/v3.0.0>.

[7] 3GPP TR 21.900: "Technical Specification Group working methods".

[8] 3GPP TS 33.501: "Security architecture and procedures for 5G system".

[9] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[10] 3GPP TS 29.510: "5G System; Network Function Repository Services; Stage 3".

[11] IETF RFC 9113: "HTTP/2".

[12] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format".

[13] IETF RFC 9457: "Problem Details for HTTP APIs".

[14] 3GPP TS 23.247: "Architectural enhancements for 5G multicast-broadcast services; Stage 2".

[15] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[16] 3GPP TS 29.532: "5G System; 5G Multicast-Broadcast Session Management Services; Stage 3".

[17] 3GPP TS 29.514: "5G System; Policy Authorization Service; Stage 3".

[18] 3GPP TS 29.512: "5G System; Session Management Policy Control Service; Stage 3".

[19] 3GPP TS 29.214: "Policy and Charging Control over Rx reference point".

[20] 3GPP TS 29.519: "5G System; Usage of the Unified Data Repository service for Policy Data, Application Data and Structured Data for Exposure; Stage 3".

[21] 3GPP TS 29.521: "5G System; Binding Support Management Service; Stage 3".

[22] IETF RFC 7396: "JSON Merge Patch".

# 3 Definitions, symbols and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

For the purpose of the present document, the terms and definitions given in clause 3 of 3GPP TS 23.247 [14] also apply, including the ones referencing other specifications.

## 3.2 Symbols

None.

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

MBS Multicast/Broadcast Service

MB-SMF Multicast/Broadcast Session Management Function

MBSF Multicast/Broadcast Service Function

# 4 Overview

In the frame of supporting Multicast/Broadcast Services (MBS), the Policy Control Function (PCF) provides services to NF service consumers (e.g. MB-SMF) via the Npcf Service Based Interface. The PCF supports for this purpose the functionalities defined in 3GPP TS 23.247 [14], i.e. MBS related Policy and Charging Control procedures.

Figures°4-1 and 4.2 depict the Multicast/Broadcast related reference architecture of the PCF respectively in SBI representation and reference point representation.



Figure 4-1: Reference model for the MBS PCF Services – SBI representation



Figure 4-2: Reference Model for the MBS PCF Services – Reference point representation

# 5 Services offered by the PCF

## 5.1 Introduction

Table 5.1-1 summarizes the corresponding APIs defined for this specification.

Table 5.1-1: API Descriptions

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Service Name | Clause | Description | OpenAPI Specification File | apiName | Annex |
| Npcf\_MBSPolicyControl | 5.2 | MBS Policy Control Service | TS29537\_Npcf\_MBSPolicyControl.yaml | npcf-mbspolicycontrol | A.2 |
| Npcf\_MBSPolicyAuthorization | 5.3 | MBS Policy Authorization Service | TS29537\_Npcf\_MBSPolicyAuthorization.yaml | npcf-mbspolicyauth | A.3 |

## 5.2 Npcf\_MBSPolicyControl Service

### 5.2.1 Service Description

The MBS Session Policy Control Service enables the Policy Control Function (PCF) to provision, update and remove MBS session related policies to NF service consumers (e.g. MB-SMF), i.e.:

- enable an NF service consumer to request the creation, update and deletion of an MBS Policy Association for an MBS session; and

- enable the PCF to provision/update/remove MBS policies towards an NF service consumer.

### 5.2.2 Service Operations

#### 5.2.2.1 Introduction

The service operations defined for the Npcf\_MBSPolicyControl Service are shown in table 5.2.2.1-1.

Table 5.2.2.1-1: Npcf\_MBSPolicyControl Operations

|  |  |  |
| --- | --- | --- |
| Service Operation Name | Description | Initiated by |
| Npcf\_MBSPolicyControl\_Create | Request the creation of an MBS Policy Association at the PCF in order to receive MBS policies for an MBS session. | NF service consumer (e.g. MB-SMF) |
| Npcf\_MBSPolicyControl\_Update | Request the update of an existing MBS Policy Association at the PCF in order to receive the updated MBS policies for an MBS session. | NF service consumer (e.g. MB-SMF) |
| Npcf\_MBSPolicyControl\_Delete | Request the deletion of an existing MBS Policy Association. | NF service consumer (e.g. MB-SMF) |

#### 5.2.2.2 Npcf\_MBSPoliyControl\_Create

##### 5.2.2.2.1 General

The Npcf\_MBSPolicyControl\_Create service operation enables an NF service consumer (e.g. MB-SMF) to request the creation of an MBS Policy Association at the PCF and the provisioning of MBS policies for a multicast or a broadcast MBS session.

The following procedures using the Npcf\_MBSPolicyControl\_Create service operation are supported:

- MBS Policy Association Establishment.

##### 5.2.2.2.2 MBS Policy Association Establishment



Figure 5.2.2.2.2-1: Procedure for MBS Policy Association establishment

1. In order to request the creation of an MBS Policy Association, the NF service consumer (e.g. MB-SMF) shall send an HTTP POST request to the PCF targeting the URI of the "MBS Policies" collection resource, with the request body containing the MbsPolicyCtxtData data structure that shall contain:

- the identifier of the concerned MBS Session, within the "mbsSessionId" attribute;

- the MBS Service Information, if available, within the "mbsServInfo" attribute;

- the list of supported features, if feature negotiation needs to take place, within the "suppFeat" attribute; and

- the Area Session Policy ID within the "areaSessPolId" attribute, if the "AreaSessPolicy" feature is supported and the request corresponds to an MBS Session that is an instance of a location-dependent MBS service.

and may contain:

- the DNN of the MBS session, within the "dnn" attribute; and

- the S-NSSAI of the MBS session, within the "snssai" attribute.

2. Upon reception of the HTTP POST request from the NF service consumer:

- if MBS Service Information is present within the "mbsServInfo" attribute, the MBS session is an instance of a location-dependent MBS service, and if the "AreaSessPolicy" feature is supported, the Area Session Policy ID is present within the "areaSessPolId" attribute, and the PCF is not already serving this location-dependent MBS service (i.e., there is no MBS Policy Association at the PCF for the MBS Session ID provided within "mbsSessionId" attribute), or if the MBS Service Information is not present, the PCF may interact with the BSF by invoking the Nbsf\_Management\_Register service operation, as specified in clause 4.2.2.4 of 3GPP TS 29.521 [21], to check whether there is already a PCF serving the MBS Session, and if it is not the case, register itself as the PCF serving the MBS session;

NOTE 1: Interacting with the BSF is not necessary in a deployment with a single PCF.

- if MBS Service Information is present within the "mbsServInfo" attribute, then:

- the PCF may interact with the UDR to retrieve MBS Session policy control data for the MBS session, as specified in 3GPP TS 29.519 [20];

NOTE 2: Interacting with the UDR for MBS Session policy control data retrieval is not necessary in a deployment where MBS Policy Session policy control data is stored locally at the PCF.

- the PCF shall then perform MBS policy authorization based on the received MBS Service Information, the operator policies that are pre-configured at the PCF and the MBS Session policy control data retrieved from the UDR, if any;

- if MBS policy authorization is successful, the PCF shall derive the required MBS policies (e.g. QoS parameters) and determine whether they are allowed or not;

- if the required MBS policies are allowed:

- the PCF shall store the generated MBS policies for the MBS session together with the corresponding MBS session ID, and if the "AreaSessPolicy" feature is supported and the MBS session is an instance of a location-dependent MBS service, the corresponding Area Session Policy ID; and

- if MBS policy authorization is not successful or the required MBS policies are not allowed, the PCF shall reject the request with an appropriate error response as specified below in this clause;

- otherwise, when MBS Service Information is not present within the "mbsServInfo" attribute and the PCF has previously derived the necessary MBS policies for the MBS session using the procedure defined in clause 5.3.2.2, the PCF shall provide these MBS policies in the response message returned to the NF service consumer (MB-SMF) as described below;

- upon success, the PCF shall:

- create a new "Individual MBS Policy" resource; and

- respond to the NF service consumer with an HTTP "201 Created" status code including a Location header field containing the URI of the created "Individual MBS Policy" resource, and the response body including the MbsPolicyData data structure that shall contain:

- the received input parameters within the corresponding request body, within the "mbsPolicyCtxtData" attribute;

- the provisioned MBS Policy Decision containing the MBS policies derived by the PCF as defined above in this clause, within the "mbsPolicies" attribute; and

- the list of supported features, if feature negotiation is taking place, within the "suppFeat" attribute;

- if errors occur when processing the HTTP POST request, the PCF shall apply the error handling procedures specified in clause 6.1.7;

NOTE 3: The PCF also deregisters at the BSF from being the PCF serving the MBS Session using the procedure defined in clause 4.2.3.4 of 3GPP TS 29.521 [21], if the PCF created such MBS Session binding as defined above in this clause. Interacting with the BSF to deregister from being the PCF serving the MBS Session is not necessary in a deployment with a single PCF.

NOTE 4: For a location-dependent MBS service, the PCF deregisters at the BSF from being the PCF serving the MBS Session as indicated in NOTE 3 above only if it is the last MBS Policy Association associated to the location-dependent MBS service (i.e., associated to the corresponding MBS Session ID).

- if MBS Service Information is provided but is invalid, incorrect or insufficient for the PCF to perform MBS policy authorization, the PCF shall reject the request with an HTTP "400 Bad Request" response message including the ProblemDetails data structure with the "cause" attribute set to "INVALID\_MBS\_SERVICE\_INFO";

- if MBS Service Information is provided, but the MBS IP flow(s) description provided within the MBS Service Information cannot be handled by the PCF because the restrictions defined in clause 5.3.8 of 3GPP TS 29.214 [19] are not respected, the PCF shall reject the request with an HTTP "400 Bad Request" status code including the ProblemDetails data structure with the "cause" attribute set to "FILTER\_RESTRICTIONS\_NOT\_RESPECTED";

- if from an application level point of view, the provided set of input parameters is incomplete, erroneous or missing necessary information for the PCF to perform MBS policy control, the PCF shall reject the request with an HTTP "400 Bad Request" response message including the ProblemDetails data structure with the "cause" attribute set to "ERROR\_INPUT\_PARAMETERS";

- if MBS Service Information is provided but is not authorized, the PCF shall reject the request with an HTTP "403 Forbidden" status code including the MbsExtProblemDetails data structure that shall contain:

- the ProblemDetails data structure with the "cause" attribute set to "MBS\_SERVICE\_INFO\_NOT\_AUTHORIZED";

and may contain:

- the AcceptableMbsServInfo data structure including the MBS Service Information that is acceptable for the PCF;

and

- if the PCF denies the creation of the "Individual MBS Policy" resource based on local configuration and/or operator policies, the PCF shall reject the request within an HTTP "403 Forbidden" status code including the "cause" attribute of the ProblemDetails data structure set to "MBS\_POLICY\_CONTEXT\_DENIED". At the reception of this error code and based on the internally configured failure actions, the NF service consumer may reject or allow, by applying local policies, the establishment of the corresponding MBS session.

#### 5.2.2.3 Npcf\_MBSPolicyControl\_Update

##### 5.2.2.3.1 General

The Npcf\_MBSPolicyControl\_Update service operation enables the NF service consumer (e.g. MB-SMF) to request the update of an existing "Individual MBS Policy" resource for a multicast or a broadcast MBS session and/or report MBS Policy Decision installation and/or enforcement failure(s) to the PCF.

The following procedures using the Npcf\_MBSPolicyControl\_Update service operation are supported:

- MBS Policy Association Update.

##### 5.2.2.3.2 MBS Policy Association Update



Figure 5.2.2.3.2-1: Procedure for MBS Policy Association Update

1. In order to request the update of an existing MBS Policy Association, the NF service consumer shall invoke the "Update" resource custom operation by sending an HTTP POST request to the PCF targeting the URI of the corresponding "Individual MBS Policy" resource custom operation, i.e. "{apiRoot}/npcf-mbspolicycontrol/<apiVersion>/mbs-policies/{mbsPolicyId}/update", with the request body including the MbsPolicyCtxtDataUpdate data structure that may contain:

- the updated MBS Service Information, within the "mbsServInfo" attribute;

- the MBS Policy Control Request Triggers that are met, within the "mbsPcrts" attribute, and/or

- the MBS Error reporting containing the MBS Policy Decision installation and/or enforcement failure(s), within the "mbsErrorReport" attribute.

If the PCF determines that the received HTTP POST request needs to be redirected, the PCF shall respond with an HTTP redirect response, as specified in clause 6.10.9 of 3GPP TS 29.500 [4].

2. Upon reception of the HTTP POST request from the NF service consumer:

- if the MBS Policy Control Request Trigger "MBS\_SESSION\_UPDATE" is triggered and updated MBS Service Information is present within the "mbsServInfo" attribute, then the PCF shall perform MBS policy authorization for the received updated MBS Service Information taking into account the operator policies pre-configured at the PCF and/or the MBS Session policy control data retrieved from the UDR. Then:

- if MBS policy authorization is successful, the PCF shall determine whether updated MBS policies (e.g. QoS parameters) need to be derived and provisioned. If it is the case, the PCF shall derive these required updated MBS policies (e.g. QoS parameters) and determine whether they are allowed or not;

- if updated MBS policies are derived and allowed, the PCF shall store the generated updated MBS policies for the MBS session together with the corresponding MBS session ID; and

- if MBS policy authorization is not successful or the required updated MBS policies, if any, are not allowed, the PCF shall reject the request with an appropriate error response as specified below in this clause;

- if the MBS Policy Control Request Trigger "MBS\_SESSION\_UPDATE" is triggered and no updated MBS Service Information is provided, then the PCF may identify whether there are any updated MBS policies that need to be applied as per the procedure defined in clause 5.3.2.3 and/or based on local configuration;

NOTE: If updated MBS Service Information is not present in the received request, then the PCF has previously determined and generated the required updated MBS policies for the MBS session as specified in clause 5.3.

- if MBS error reporting is present in the request and contains a set of MBS Policy Decision installation and/or enforcement failure(s), the PCF may take it into account when deriving the required updated MBS policies as specified in clause 5.2.4.1;

- upon success, the PCF shall:

- update the corresponding "Individual MBS Policy" resource accordingly; and

- respond to the NF service consumer with an HTTP "200 OK" status code with the response body including the MbsPolicyData data structure that shall contain:

- the updated complete list of input parameters, within the "mbsPolicyCtxtData" attribute;

and may contain:

- the updated MBS Policy Decision containing the updated, deleted and/or newly provisioned MBS policies, within the "mbsPolicies" attribute;

- if errors occur when processing the HTTP POST request, the PCF shall apply the error handling procedures specified in clause 6.1.7;

- if updated MBS Service Information is provided but is invalid, incorrect or insufficient for the PCF to perform MBS policy authorization, the PCF shall reject the request with an HTTP "400 Bad Request" response message including the ProblemDetails data structure with the "cause" attribute set to "INVALID\_MBS\_SERVICE\_INFO";

- if updated MBS Service Information is provided, but the MBS IP flow(s) description provided within the MBS Service Information cannot be handled by the PCF because the restrictions defined in clause 5.3.8 of 3GPP TS 29.214 [19] are not respected, the PCF shall reject the request with an HTTP "400 Bad Request" status code including the ProblemDetails data structure with the "cause" attribute set to "FILTER\_RESTRICTIONS\_NOT\_RESPECTED";

- if from an application level point of view, the provided set of input parameters is incomplete, erroneous or missing necessary information for the PCF to perform MBS policy control, the PCF shall reject the request with an HTTP "400 Bad Request" response message including the ProblemDetails data structure with the "cause" attribute set to "ERROR\_INPUT\_PARAMETERS";

- if updated MBS Service Information is provided but is not authorized, the PCF shall reject the request with an HTTP "403 Forbidden" status code including the MbsExtProblemDetails data structure that shall contain:

- the ProblemDetails data structure with the "cause" attribute set to "MBS\_SERVICE\_INFO\_NOT\_AUTHORIZED";

and may contain:

- the AcceptableMbsServInfo data structure including the MBS Service Information that is acceptable for the PCF;

- if the PCF denies the update of the "Individual MBS Policy" resource based on local configuration and/or operator policies, the PCF shall reject the request within an HTTP "403 Forbidden" status code including the ProblemDetails data structure with the "cause" attribute set to "MBS\_POLICY\_CONTEXT\_DENIED". At the reception of this error code and based on the internally configured failure actions, the NF service consumer (MB-SMF) may reject or allow, by applying local policies, the update of the corresponding MBS session; and

- if the targeted "Individual MBS Policy" resource does not exist, the PCF shall reject the request with an HTTP "404 Not Found" status code including the ProblemDetails data structure with the "cause" attribute set to "MBS\_POLICY\_ASSOCIATION\_NOT\_FOUND".

#### 5.2.2.4 Npcf\_MBSPolicyControl\_Delete

##### 5.2.2.4.1 General

The Npcf\_MBSPolicyControl\_Delete service operation enables the NF service consumer (e.g. MB-SMF) to request the deletion of an existing "Individual MBS Policy" resource.

The following procedures using the Npcf\_MBSPolicyControl\_Delete service operation are supported:

- MBS Policy Association Deletion.

##### 5.2.2.4.2 MBS Policy Association Deletion



Figure 5.2.2.4.2-1: MBS Policy Association Deletion procedure

1. In order to request the deletion of an existing MBS Policy Association, the NF service consumer shall send an HTTP DELETE request to the PCF, targeting the URI of the corresponding "Individual MBS Policy" resource.

If the PCF determines that the received HTTP DELETE request needs to be redirected, the PCF shall respond with an HTTP redirect response, as specified in clause 6.10.9 of 3GPP TS 29.500 [4].

2. On successful deletion of the targeted MBS Policy Association:

- the PCF may deregister at the BSF from being the PCF serving the MBS Session using the procedure defined in clause 4.2.3.4 of 3GPP TS 29.521 [21], if the PCF created such MBS Session binding during the creation of the MBS Policy Association, and for a location-dependent MBS service, this is the last MBS Policy Association associated to the location-dependent MBS service (i.e., associated to the corresponding MBS Session ID), as specified in clause 5.2.2.2; and

- the PCF shall respond to the NF service consumer (MB-SMF) with an HTTP "204 No Content" status code.

If errors occur when processing the HTTP DELETE request, the PCF shall apply the error handling procedures specified in clause 6.1.7.

If the targeted "Individual MBS Policy" resource does not exist, the PCF shall reject the request with an HTTP "404 Not Found" status code including the ProblemDetails data structure with the "cause" attribute set to "MBS\_POLICY\_ASSOCIATION\_NOT\_FOUND".

### 5.2.3 MBS Policy Decision Management

#### 5.2.3.1 General

An MBS Policy Decision enables to provide the necessary MBS policies for controlling an MBS Session. An MBS Policy Decision is encoded via the MbsPolicyDecision data structure defined in clause 6.1.6.2.3 and composed of the following information:

- MBS PCC rule(s), within the "mbsPccRules" attribute.

- MBS QoS decision(s), which can be referred by MBS PCC rules, within the "mbsQosDecs" attribute.

- Set(s) of MBS QoS characteristics for non-standardized and non-preconfigured 5QIs, within the "mbsQosChars" attribute.

- The authorized MBS Session-AMBR, within the "authMbsSessAmbr" attribute.

- The MBS Policy Control Request Trigger(s), within the "mbsPcrts" attribute.

The following clauses describe the above components of an MBS Policy Decision.

##### 5.2.3.1.1 MBS PCC Rule definition

An MBS PCC rule enables to provide MBS policy control for an MBS service data flow. It is composed of the following information, as defined in table 5.2.3.1.1-1.

- Information enabling the detection of the MBS service data flow.

- A set of MBS Policy Control parameters to be enforced for the MBS service data flow.

Table 5.2.3.1.1-1: Content of an MBS PCC rule

|  |  |  |
| --- | --- | --- |
| Name | Description | Category |
| MBS PCC Rule identifier | Uniquely identifies the MBS PCC rule, within an MBS Session.  It is used between the PCF and the MB-SMF for referencing the MBS PCC rules of an MBS Session. | Mandatory |
|  | MBS service data flow detection |  |
| Precedence | Determines the order in which the MBS service data flow template of the MBS PCC rule is applied relative to the MBS service data flow templates of the other MBS PCC rules of the MBS session, during MBS service data flow detection and policy enforcement. | Mandatory |
| MBS Service Data Flow Template | The list of MBS service data flow filter(s) for the detection of the MBS service data flow. | Mandatory |
|  | MBS policy control parameters |  |
| 5QI | Identifier of the authorized set of QoS parameters for the MBS service data flow. | Mandatory |
| ARP | The authorized Allocation and Retention Priority for the MBS service data flow, consisting of the priority level, the pre-emption capability and the pre-emption vulnerability. | Mandatory |
| MBR – Maximum BitRate (DL) | The downlink maximum bitrate authorized for the MBS service data flow. | Optional |
| GBR – Guaranteed BitRate (DL) | The downlink guaranteed bitrate authorized for the MBS service data flow. | Optional |
| Averaging Window | Represents the duration over which the guaranteed and maximum bitrates shall be calculated. | Optional |
| Priority Level | Indicates the level of priority in scheduling resources among MBS QoS flows. | Optional |
| Maximum Data Burst Volume | Denotes the largest amount of data that is required to be transferred within a period of 5G-AN PDB. | Optional |

NOTE: If the user plane towards the MB-UPF uses a unicast tunnel, the MBS Service Data Flow Template relates to the inner IP layer within the unicast tunnel.

An MBS PCC rule is encoded via the MbsPccRule data structure defined in clause 6.1.6.2.7 and is composed of the following information:

- An MBS PCC rule identifier that uniquely identifies the MBS PCC rule within the related MBS Session, within the "mbsPccRuleId" attribute.

- The MBS service data flow template for MBS service data flow detection, within the "mbsDlIpFlowInfo" attribute.

- The precedence information, i.e. the order in which the MBS service data flow template of the MBS PCC rule is applied relative to the MBS service data flow templates of the other MBS PCC rules of the MBS session, during MBS service data flow detection and policy enforcement, within the "precedence" attribute.

- The MBS authorized QoS to be applied for the MBS service data flow corresponding to the MBS PCC rule, i.e. a reference to an MBS QoS decision instance provisioned by the PCF at MBS Policy Decision level, within the "refMbsQosDec" attribute.

The following operations are allowed on MBS PCC rule(s):

- Installation, i.e. to provision MBS PCC rule(s).

- Modification, i.e. to modify MBS PCC rule(s).

- Removal, i.e. to remove MBS PCC rule(s).

##### 5.2.3.1.2 MBS QoS Decision

An MBS Policy Decision based on MBS QoS contains the QoS parameters to be applied for an MBS service data flow. It defines the QoS parameters (e.g. 5QI, ARP, maximum/guaranteed bitrates, etc.) to be applied for the corresponding MBS PCC rule. An MBS QoS decision is encoded via the MbsQosDec data structure defined in clause 6.1.6.2.8 and composed of the following information:

- An identifier of the MBS QoS Decision that uniquely identifies the MBS QoS Decision within the related MBS Session, within the "mbsQosId" attribute.

- The 5QI information, i.e. an identifier of the set of QoS parameters to be applied to an MBS service data flow, within the "5qi" attribute;

- The 5QI Priority Level, within the "priorityLevel" attribute.

- The Allocation and Retention Priority information to be applied for an MBS service data flow, within the "arp" attribute.

- The Maximum Downlink Bit Rate for to be applied for an MBS service data flow, within the "mbrDl" attribute.

- The Guaranteed Downlink Bit Rate to be applied for an MBS service data flow, within the "gbrDl" attribute.

- The averaging window, i.e. the duration over which the guaranteed and maximum bitrates shall be calculated, within the "averWindow" attribute.

- The MBS Maximum Data Burst Volume to be applied for an MBS service data flow, within the "mbsMaxDataBurstVol" attribute.

##### 5.2.3.1.3 MBS QoS Characteristics

A set of MBS QoS Characteristics contains the QoS parameters for a non-standardized and non-preconfigured 5QI. It defines the QoS parameters (e.g. 5QI, ARP, maximum/guaranteed bitrates, etc.) to be applied for an MBS PCC rule and the corresponding MBS service data flow. A set of MBS QoS Characteristics is encoded via the MbsQosChars data structure defined in clause 6.1.6.2.9 and composed of the following information:

- The 5QI information, i.e. an identifier of the set of non-standardized and non-preconfigured QoS parameters for an MBS service data flow, within the "5qi" attribute. It applies at MBS PCC rule level and MBS session level.

- The resource type (i.e. GBR, delay critical GBR or non-GBR), within the "resourceType" attribute.

- The 5QI priority level, within the "priorityLevel" attribute.

- The Packet Delay Budget, within the "packetDelayBudget" attribute.

- The Packet Error Rate, within the "packetErrorRate" attribute.

- The averaging window, within the "averWindow" attribute.

- The MBS Maximum Data Burst Volume, within the "mbsMaxDataBurstVol" attribute.

##### 5.2.3.1.4 MBS Session-AMBR

The MBS Session-AMBR contains the Aggregated Maximum Bit Rate to be applied for an MBS session.

##### 5.2.3.1.5 MBS Policy Control Request Triggers

The MBS Policy Control Request Triggers identify the conditions based on which the NF service consumer (MB-SMF) shall trigger the MBS Policy Association Update procedure defined in clause 5.2.2.3. They can be either pre-configured at the NF service consumer (MB-SMF), i.e. implicitly subscribed by default by the PCF, or explicitly provisioned by the PCF to the NF service consumer (MB-SMF) during the MBS Policy Association Creation/Update procedures defined in clause 5.2.2.

The MBS Policy Control Request Triggers are encoded using the MbsPcrt Enumeration data type defined in clause 6.1.6.3.3. The possible values are the following:

- "MBS\_SESSION\_UPDATE", i.e. MBS Session Update: the MBS policies may need to be updated due to updated MBS Session information. This MBS Policy Control Request Trigger is pre-configured at the NF service consumer (MB-SMF), i.e. implicitly subscribed by the PCF.

#### 5.2.3.2 Provisioning and enforcement of MBS Policy Decisions

##### 5.2.3.2.1 General

MBS Policy Decisions are provided by the PCF to the NF service consumer (MB-SMF) as part of the following service operations:

- the Npcf\_MBSPolicyControl\_Create service operation defined in clause 5.2.2.2; and

- the Npcf\_MBSPolicyControl\_Update service operation defined in clause 5.2.2.3.

For the Npcf\_MbsPolicyControl\_Create service operation, the MbsPolicyDecision data structure shall contain the MBS Policy Decision containing a full description of all the MBS policies provisioned by the PCF for the MBS Policy Association.

For the Npcf\_MBSPolicyControl\_Update service operation for, the MbsPolicyDecision data structure shall contain the updated MBS Policy Decision containing a full description of all the updated MBS policies (if any) provisioned for the MBS Policy Association.

##### 5.2.3.2.2 Provisioning and enforcement of MBS PCC rules

The PCF provisions/updates/removes MBS PCC rule(s) via the "mbsPccRules" attribute of the MbsPolicyDecision data structure as part of the provisioning/update/removal of an MBS Policy Decision (cf. clause 5.2.3.2.1).

- For provisioning or modifying a dynamic PCF-provisioned MBS PCC rule, the corresponding MbsPccRule data structure shall be provided as a map entry value of the "mbsPccRules" attribute within the MbsPolicyDecision data structure representing the related MBS Policy Decision. The corresponding map key shall be set to the value of the "mbsPccRuleId" attribute of the MbsPccRule data structure.

- For removing a previously provisioned MBS PCC rule, the corresponding map entry value shall be set to "NULL" and map key to the value of the "mbsPccRuleId" attribute of the MbsPccRule data structure representing the targeted MBS PCC rule.

##### 5.2.3.2.3 Provisioning and enforcement of authorized MBS QoS for an MBS service data flow

The authorized MBS QoS for an MBS service data flow is provisioned along with the corresponding MBS PCC rule, as specified in the clause 5.2.3.2.2.

The MBS authorized QoS per MBS service data flow shall be provisioned within the MbsQosDec data structure representing the MBS QoS Decision to be applied for the MBS service data flow. For this purpose:

- the PCF shall include this MBS QoS Decision instance as a map entry within the "mbsQosDecs" attribute of the MbsPolicyDecision data structure of the corresponding MBS Policy Decision, as specified in clause 5.2.3.1.2, and include the reference to this MBS QoS Decision instance within the "refMbsQosDec" attribute of the MbsPccRule data structure representing the corresponding MBS PCC rule;

- when the PCF provisions a standardized 5QI value, but the Priority Level, the Averaging Window and/or the Maximum Data Burst Volume shall be different from the standardized values defined in the table 5.7.4-1 of 3GPP TS 23.501 [2], the PCF shall include within the corresponding MbsQosDec data structure the required Priority Level within the "priorityLevel" attribute, the Averaging Window within the "averWindow" attribute and/or the MBS Maximum Data Burst Volume within the "mbsMaxDataBurstVol" attribute;

- if the PCF needs to provision dynamically assigned 5QI value(s) (from the non-standardized and non-preconfigured value range) and the associated set(s) of MBS QoS Characteristics, the PCF shall include within the MbsPolicyDecision data structure representing the related MBS Policy Decision the "mbsQosChars" map attribute containing one or more set(s) of MBS QoS Characteristics, with each one of them encoded using the MbsQosChar data structure as specified in clause 5.2.3.1.3. The PCF shall not update nor remove previously provisioned set(s) of MBS QoS Characteristics during the lifetime of the concerned MBS Policy Association;

- when the PCF provisions a dynamically assigned 5QI value (from the non-standardized and non-preconfigured value range) for the MBS PCC rule within the referred MBS QoS Decision instance, then the "5qi" attribute of the corresponding MbsQosDec data structure shall be set to the value of the dynamically assigned 5QI which points to the MBS QoS Characteristics instance containing the related QoS parameters;

NOTE: Operator configuration is assumed to ensure that a dynamically assigned 5QI value is unique and references at a given time the same set of MBS QoS characteristics within the whole PLMN.

Upon reception of an MBS PCC rule provisioning including the corresponding authorized MBS QoS information from the PCF, the NF service consumer (MB-SMF) shall perform MBS QoS flow binding as specified in clause 6.10 of 3GPP TS 23.247 [14]. The NF service consumer (MB-SMF) shall also reserve the necessary resources for the guaranteed bitrate of the MBS PCC rule, if provided. For GBR MBS QoS flows, the NF service consumer (MB-SMF) should set the MBS QoS flow's GBR to the sum of the GBR(s) of all the MBS PCC rule(s) that are active/installed and bound to that GBR MBS QoS flow, and the MBS QoS flow's MBR to the sum of the MBR(s) of all the MBS PCC rule(s) that are active/installed and bound to that GBR MBS QoS flow.

The NF service consumer (MB-SMF) shall assign a new MBS QFI if a new MBS QoS flow needs to be established and derive the MBS QoS profile required towards the Access Network, if applicable, and the MBS QoS information with PDRs towards the MB-UPF.

During an MBS session policy association update procedure that results in updating all the MBS PCC rule(s) bound to a certain MBS QoS flow, if all these MBS PCC rule(s) are updated with the same values of the QoS parameters (e.g. 5QI, ARP, Priority level, Averaging Window and Maximum Data Burst Volume), the NF service consumer (MB-SMF) should not perform a new MBS QoS flow binding and simply modify this MBS QoS flow with the updated QoS parameters.

##### 5.2.3.2.4 Provisioning and enforcement of authorized MBS Session-AMBR

The Provisioning of the authorized MBS Session-AMBR for an MBS session is part of the provisioning of the corresponding MBS Policy Decision, as specified in the clause 5.2.3.2.1.

Upon reception of the authorized MBS Session-AMBR from the PCF, the NF service consumer (MB-SMF) shall trigger the necessary procedures towards the MB-UPF for the provisioning and enforcement of the MBS Session-AMBR for the concerned MBS session.

NOTE: For an MBS session, the authorized MBS Session-AMBR is not propagated to neither the access network nor the UE.

##### 5.2.3.2.5 Provisioning and enforcement of MBS Policy Control Request Triggers

The PCF may provision one or more MBS Policy Control Request Triggers(s) to the NF service consumer (MB-SMF). In order to do so, the PCF shall include the "mbsPcrts" attribute containing one or more MBS Policy Control Request Triggers(s) within the MbsPolicyDecision data structure.

During the lifetime of the MBS Policy Association, the PCF may update and/or remove previously provisioned MBS Policy Control Request Triggers(s):

- In order to update a previously subscribed set of MBS Policy Control Request Triggers(s), the PCF shall provide the complete list of the subscribed MBS Policy Control Request Triggers(s) within the "mbsPcrts" attribute of the MbsPolicyDecision data structure.

- In order to remove all the previously subscribed MBS Policy Control Request Triggers(s), the PCF shall provide the "mbsPcrts" attribute set to the value "NULL" within the MbsPolicyDecision data structure. Upon reception of a "NULL" value within the "mbsPcrts" attribute, the NF service consumer (MB-SMF) shall only trigger the MBS Policy Association Update procedure for the pre-configured MBS Policy Control Request Triggers(s), i.e. the ones implicitly subscribed by the PCF.

MBS Policy Control Request Triggers(s) may also be pre-configured at the NF service consumer as specified in clause 5.2.3.1.5. In such case, the PCF is implicitly subscribed and does not need to explicitly subscribe to these MBS Policy Control Request Triggers(s) towards the NF service consumer (MB-SMF). A combination of pre-configured MBS Policy Control Request Triggers(s) and explicitly subscribed MBS Policy Control Request Triggers(s) may be present for an MBS Policy Association.

### 5.2.4 MBS Policy Error Handling

#### 5.2.4.1 MBS Policy Error Reporting

Following an MBS Policy Association Creation or Update procedure, as defined in clause 5.2.2.2.2 or 5.2.2.3.2, the NF service consumer (MB-SMF) may report the potentially encountered failure(s) during the installation and/or enforcement of the provisioned MBS Policy Decision, both for MBS Policy Decision level failure(s) (e.g. MBS QoS Decision failure) and MBS PCC rule level failure(s) (e.g. the installation of one or more MBS PCC rule(s) fails or the PCF installed or modified one or more MBS PCC rules but resource allocation for these MBS PCC rule(s) was unsuccessful).

In order to do so, the NF service consumer (MB-SMF) shall trigger the MBS Policy Association Update procedure defined in clause 5.2.2.3.2 and include within the "mbsErrorReport" attribute of the MbsPolicyCtxtDataUpdate data structure the necessary information on the failure(s) that occurred within one or more MBS Report instance(s), each one of them encoded using the MbsReport data structure that shall include:

- the failure reason, if available, within the "failureCode" attribute;

- the affected MBS PCC rule(s), if the reported failure is at MBS PCC rule level, within the "mbsPccRuleIds" attribute; and

- the MBS PCC rule status, if the reported failure is at MBS PCC rule level, within the "mbsPccRuleStatus" attribute.

Depending on the value of the "failureCode" attribute, the PCF may decide on the necessary updates to be applied to the MBS Policy Decision, if any, including whether to retain, re-install, modify or remove the existing MBS PCC rule(s), or any other action applies.

For MBS PCC rule level failure(s), the following handling shall apply:

- if the installation of one or more new MBS PCC rule(s) (i.e. MBS PCC rule(s) which were not successfully installed previously) fails, the NF service consumer (MB-SMF) shall set the "mbsPccRuleStatus" attribute to the value "INACTIVE";

- if one or more MBS PCC rule(s) were successfully installed but can no longer be enforced by the NF service consumer (MB-SMF), the MB-SMF shall set the "mbsPccRuleStatus" attribute to "INACTIVE";

NOTE: When the PCF receives the "mbsPccRuleStatus" set to the value "INACTIVE", the PCF does not need to request the MB-SMF to remove the concerned MBS PCC rule(s) within the "mbsPccRuleIds" attribute.

- if the requested modifications to currently active MBS PCC rule(s) fails, the NF service consumer (MB-SMF) shall:

- retain the targeted existing MBS PCC rule(s) active in their current version (i.e. without any modification), unless the failure reason also impacts the current version of these existing MBS PCC rule(s); and

- report the modification failure to the PCF;

and

- the removal of MBS PCC rule(s) shall not fail. The NF service consumer (MB-SMF) shall retain the MBS PCC rule(s) removal request and perform the related necessary actions/procedures in the network when it is possible.

## 5.3 Npcf\_MBSPolicyAuthorization Service

### 5.3.1 Service Description

The MBS Policy Authorization Service enables the Policy Control Function (PCF) to authorize the MBS Service Information provided by an NF service consumer (e.g. AF, NEF, MBSF) and derive the related MBS policies, i.e.:

- enable an NF service consumer (e.g. AF, NEF, MBSF) to request the creation, update or removal of an MBS Application Session Context, based on the provisioning of MBS Service Information; and

- enable the PCF to authorize the provided MBS Service Information and derive the MBS policies related to the targeted MBS session.

### 5.3.2 Service Operations

#### 5.3.2.1 Introduction

The service operations defined for the Npcf\_MBSPolicyAuthorization Service are shown in table 5.3.2.1-1.

Table 5.3.2.1-1: Npcf\_MBSPolicyAuthorization Service Operations

|  |  |  |
| --- | --- | --- |
| Service Operation Name | Description | Initiated by |
| Npcf\_MBSPolicyAuthorization\_Create | Request the creation of an MBS Application Session Context at the PCF, to enable MBS policy authorization for the provided MBS Service Information. | NF service consumer (e.g. NEF, MBSF, AF) |
| Npcf\_MBSPolicyAuthorization\_Update | Update an existing MBS Application Session Context at the PCF, to enable MBS policy authorization for the provided updated MBS Service Information. | NF service consumer (e.g. NEF, MBSF, AF) |
| Npcf\_MBSPolicyAuthorization\_Delete | Delete an existing MBS Application Session Context at the PCF. | NF service consumer (e.g. NEF, MBSF, AF) |

#### 5.3.2.2 Npcf\_MBSPoliyAuthorization\_Create

##### 5.3.2.2.1 General

The Npcf\_MBSPolicyAuthorization\_Create service operation enables an NF service consumer (e.g. AF, NEF, MBSF) to request the creation of an MBS Application Session Context at the PCF, for the purpose of requesting MBS policy authorization for a multicast or a broadcast MBS session.

The following procedures using the Npcf\_MBSPolicyAuthorization\_Create service operation are supported:

- MBS Application Session Context Establishment.

##### 5.3.2.2.2 MBS Application Session Context Establishment



Figure 5.3.2.2.2-1: MBS Application Session Context establishment procedure

1. In order to request the creation of a new MBS Application Session Context, the NF service consumer (e.g. AF, NEF, MBSF) shall send an HTTP POST request to the PCF, targeting the URI of the "MBS Application Session Contexts" collection resource, with the request body containing the MbsAppSessionCtxt data structure that shall contain:

- the MBS session identifier, within the "mbsSessionId" attribute;

- the MBS Service Information, if available, within the "mbsServInfo" attribute; and

- the list of supported features, if feature negotiation needs to take place, within the "suppFeat" attribute;

and may contain:

- the DNN of the MBS session, within the "dnn" attribute;

- the S-NSSAI of the MBS session, within the "snssai" attribute; and

- the "request for location-dependent MBS session" indication within the "reqForLocDepMbs" attribute, if the "AreaSessPolicy" feature is supported and the request corresponds to an MBS Session that is an instance of a location-dependent MBS service.

2. Upon reception of the HTTP POST request from the NF service consumer:

- the PCF may interact with the UDR to retrieve MBS Session policy control data for the MBS session, as specified in clause 5.2.16 of 3GPP TS 29.519 [20];

NOTE 1: Interacting with the UDR for MBS Session policy control data retrieval is not necessary in a deployment where MBS Policy Session policy control data is stored locally at the PCF.

- the PCF shall perform MBS policy authorization based on the MBS Service Information received from the NF service consumer and the operator policies that are pre-configured at the PCF and/or the MBS Session policy control data retrieved from the UDR. Then:

- if MBS policy authorization is successful, the PCF shall derive the required MBS policies (e.g. QoS parameters) and determine whether they are allowed or not;

- if the required MBS policies are allowed:

- if the "AreaSessPolicy" feature is supported and the "request for location dependent MBS session" indication was present within the "reqForLocDepMbs" attribute and set to "true", the PCF shall assign an Area Session Policy ID within the "areaSessPolId" attribute for this MBS Session as an instance of a location-dependent MBS service;

- the PCF shall store the generated MBS policies for the MBS session together with the corresponding MBS session ID, and if applicable and the "AreaSessPolicy" feature is supported, the corresponding Area Session Policy ID for an MBS Session that is an instance of a location-dependent MBS service;

- the PCF shall create a new "Individual MBS Application Session Context" resource and respond to the NF service consumer with an HTTP "201 Created" status code, including an HTTP Location header field containing the URI of the created "Individual MBS Application Session Context" resource and the response body containing a representation of the created resource within the MbsAppSessionCtxt data structure; and

- the PCF may register itself at the BSF as the PCF handling the MBS session as specified in clause 4.2.2.4 of 3GPP TS 29.521 [21];

NOTE 2: Registering at the BSF as the PCF serving the MBS Session is not necessary in a deployment with a single PCF.

- otherwise, when MBS policy authorization is not successful or the required MBS policies are not allowed, the PCF shall reject the request with an appropriate error response as specified below in this clause;

- if errors occur when processing the HTTP POST request, the PCF shall apply the error handling procedures specified in clause 6.2.7;

- if the provided MBS Service Information is invalid, incorrect or insufficient for the PCF to perform MBS policy authorization, the PCF shall reject the request with an HTTP "400 Bad Request" status code including the ProblemDetails data structure with the "cause" attribute set to "INVALID\_MBS\_SERVICE\_INFO";

- if the MBS IP flow(s) description provided within the MBS Service Information cannot be handled by the PCF because the restrictions defined in clause 5.3.8 of 3GPP TS 29.214 [19] are not respected, the PCF shall reject the request with an HTTP "400 Bad Request" status code including the ProblemDetails data structure with the "cause" attribute set to "FILTER\_RESTRICTIONS\_NOT\_RESPECTED"; and

- if the provided MBS Service Information are not authorized, the PCF shall reject the request with an HTTP "403 Forbidden" status code including the MbsExtProblemDetails data structure that shall contain:

- the ProblemDetails data structure with the "cause" attribute set to "MBS\_SERVICE\_INFO\_NOT\_AUTHORIZED";

and may contain:

- the AcceptableMbsServInfo data structure including the MBS Service Information that is acceptable for the PCF.

#### 5.3.2.3 Npcf\_MBSPoliyAuthorization\_Update

##### 5.3.2.3.1 General

The Npcf\_MBSPolicyAuthorization\_Update service operation enables an NF service consumer (e.g. AF, NEF, MBSF) to request the update of an existing MBS Application Session Context, for the purpose of requesting the authorization of updated MBS Service Information.

The following procedures using the Npcf\_MBSPolicyAuthorization\_Update service operation are supported:

- MBS Application Session Context Update.

##### 5.3.2.3.2 MBS Application Session Context Update



Figure 5.3.2.3.2-1: MBS Application Session Context update procedure

1. In order to request the modification of an existing MBS Application Session Context, the NF service consumer (e.g. AF, NEF, MBSF) shall send an HTTP PATCH request to the PCF, targeting the URI of the corresponding "Individual MBS Application Session Context" resource, with the request body containing the MbsAppSessionCtxtPatch data structure that may contain:

- the requested modifications to the MBS Service Information, within the "mbsServInfo" attribute.

2. Upon reception of the HTTP PATCH request from the NF service consumer:

- the PCF may interact with the UDR to retrieve MBS Session policy control data for the MBS session, as specified in 3GPP TS 29.519 [20];

- the PCF shall perform MBS policy authorization based on the requested modifications to the MBS Service Information received from the NF service consumer and the operator policies that are pre-configured at the PCF and/or the MBS session policy control data retrieved from the UDR. Then:

- if MBS policy authorization of the requested modifications to the MBS Service Information is successful, the PCF shall derive the required updated MBS policies (e.g. QoS parameters), if any, and determine whether they are allowed or not;

- if the required updated MBS policies are allowed:

- the PCF shall store the generated updated MBS policies for the MBS session, if any, together with the corresponding MBS session ID;

- the PCF shall update the associated "Individual MBS Application Session Context" resource accordingly and respond to the NF service consumer with either an HTTP "200 OK" status code with the response body containing a representation of the updated resource within the MbsAppSessionCtxt data structure, or an HTTP "204 No Content" status code; and

- if the authorized MBS policies have been changed, the PCF shall include the "contactPcfInd" attribute set to "true" within the returned MbsAppSessionCtxt data structure to indicate that the PCF shall be contacted, i.e. to indicate to the NF service consumer (MB-SMF) that it needs to trigger the MBS Policy Association Update procedure, as defined in clause 5.2.2.3, to receive updated MBS policies from the PCF;

- otherwise, when MBS policy authorization is not successful or the required updated MBS policies are not allowed, the PCF shall reject the request with an appropriate error response as specified below in this clause;

- if errors occur when processing the HTTP PATCH request, the PCF shall apply the error handling procedures specified in clause 6.2.7;

- if the targeted "Individual MBS Application Session Context" resource does not exist, the PCF shall reject the request with an HTTP "404 Not Found" status code including the ProblemDetails data structure with the "cause" attribute set to "MBS\_SESSION\_POL\_AUTH\_CTXT\_NOT\_FOUND";

- if the provided MBS Service Information is invalid, incorrect or insufficient for the PCF to perform MBS policy authorization, the PCF shall reject the request with an HTTP "400 Bad Request" status code including the ProblemDetails data structure with the "cause" attribute set to "INVALID\_MBS\_SERVICE\_INFO";

- if the MBS IP flow(s) description provided within the MBS Service Information cannot be handled by the PCF because the restrictions defined in clause 5.3.8 of 3GPP TS 29.214 [19] are not respected, the PCF shall reject the request with an HTTP "400 Bad Request" status code including the ProblemDetails data structure with the "cause" attribute set to "FILTER\_RESTRICTIONS\_NOT\_RESPECTED"; and

- if the provided MBS Service Information is not authorized, the PCF shall reject the request with an HTTP "403 Forbidden" status code including the MbsExtProblemDetails data structure that shall contain:

- the ProblemDetails data structure with the "cause" attribute set to "MBS\_SERVICE\_INFO\_NOT\_AUTHORIZED";

and may contain:

- the AcceptableMbsServInfo data structure including the MBS Service Information that is acceptable for the PCF.

#### 5.3.2.4 Npcf\_MBSPoliyAuthorization\_Delete

##### 5.3.2.4.1 General

The Npcf\_MBSPolicyAuthorization\_Delete service operation enables an NF service consumer (e.g. AF, NEF, MBSF) to request the deletion of an existing MBS Application Session Context at the PCF.

The following procedures using the Npcf\_MBSPolicyAuthorization\_Delete service operation are supported:

- MBS Application Session Context Deletion.

##### 5.3.2.4.2 MBS Application Session Context Deletion



Figure 5.3.2.4.2-1: MBS Application Session Context deletion procedure

1. In order to request the deletion of an existing MBS Application Session Context, the NF service consumer (e.g. AF, NEF, MBSF) shall send an HTTP DELETE request to the PCF targeting the URI of the corresponding "Individual MBS Application Session Context" resource.

2. Upon success, the PCF shall respond with an HTTP "204 No Content" status code.

If errors occur when processing the HTTP DELETE request, the PCF shall apply the error handling procedures specified in clause 6.2.7.

If the targeted Individual MBS Application Session Context does not exist, the PCF shall reject the request with an HTTP "404 Not Found" status code including the ProblemDetails data structure with the "cause" attribute set to "MBS\_SESSION\_POL\_AUTH\_CTXT\_NOT\_FOUND".

# 6 API Definitions

## 6.1 Npcf\_MBSPolicyControl Service API

### 6.1.1 Introduction

The Npcf\_MBSPolicyControl Service shall use the Npcf\_MBSPolicyControl API.

The API URI of the Npcf\_MBSPolicyControl Service shall be:

**{apiRoot}/<apiName>/<apiVersion>**

The request URIs used in HTTP requests from the NF service consumer towards the NF service producer shall have the Resource URI structure defined in clause 4.4.1 of 3GPP TS 29.501 [5], i.e.:

**{apiRoot}/<apiName>/<apiVersion>/<apiSpecificResourceUriPart>**

with the following components:

- The {apiRoot} shall be set as described in 3GPP TS 29.501 [5].

- The <apiName>shall be "npcf-mbspolicycontrol".

- The <apiVersion> shall be "v1".

- The <apiSpecificResourceUriPart> shall be set as described in clause 6.1.3.

### 6.1.2 Usage of HTTP

#### 6.1.2.1 General

HTTP/2, IETF RFC 9113 [11], shall be used as specified in clause 5 of 3GPP TS 29.500 [4].

HTTP/2 shall be transported as specified in clause 5.3 of 3GPP TS 29.500 [4].

The OpenAPI [6] specification of HTTP messages and content bodies for the Npcf\_MBSPolicyControl API is contained in Annex A.2.

#### 6.1.2.2 HTTP standard headers

##### 6.1.2.2.1 General

See clause 5.2.2 of 3GPP TS 29.500 [4] for the usage of HTTP standard headers.

##### 6.1.2.2.2 Content type

JSON, IETF RFC 8259 [12], shall be used as content type of the HTTP bodies specified in the present specification as specified in clause 5.4 of 3GPP TS 29.500 [4]. The use of the JSON format shall be signalled by the content type "application/json".

The "Problem Details" JSON object shall be used to indicate additional details of the error in a HTTP response body and shall be signalled by the content type "application/problem+json", as defined in IETF RFC 9754 [13].

#### 6.1.2.3 HTTP custom headers

The mandatory HTTP custom header fields specified in clause 5.2.3.2 of 3GPP TS 29.500 [4] shall be supported, and the optional HTTP custom header fields specified in clause 5.2.3.3 of 3GPP TS 29.500 [4] may be supported.

### 6.1.3 Resources

#### 6.1.3.1 Overview

This clause describes the structure for the resource URIs and the resources and methods used for the Npcf\_MBSPolicyControl service.

Figure 6.1.3.1-1 depicts the resource URIs structure for the Npcf\_MBSPolicyControl API.



Figure 6.1.3.1-1: Resource URI structure of the Npcf\_MBSPolicyControl API

Table 6.1.3.1-1 provides an overview of the resources and applicable HTTP methods.

Table 6.1.3.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource purpose/name | Resource URI (relative path after API URI) | HTTP method or custom operation | Description (service operation) |
| MBS Policies | /mbs-policies | POST | Request the creation of a new Individual MBS Policy resource. |
| Individual MBS Policy | /mbs-policies/{mbsPolicyId} | GET | Request the retrieval of an existing Individual MBS Policy resource. |
| DELETE | Request the deletion of an existing Individual MBS Policy resource. |
| Update  (POST) | Request the update of an existing Individual MBS Policy resource. |

#### 6.1.3.2 Resource: MBS Policies

##### 6.1.3.2.1 Description

This resource represents the collection of "Individual MBS Policy" resources managed by the PCF.

##### 6.1.3.2.2 Resource Definition

Resource URI: **{apiRoot}/npcf-mbspolicycontrol/<apiVersion>/mbs-policies**

This resource shall support the resource URI variables defined in table 6.1.3.2.2-1.

Table 6.1.3.2.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 6.1.1. |

##### 6.1.3.2.3 Resource Standard Methods

###### 6.1.3.2.3.1 POST

This method enables an NF service consumer (e.g. MB-SMF) to request the creation of an MBS Policy Association at the PCF.

This method shall support the URI query parameters specified in table 6.1.3.2.3.1-1.

Table 6.1.3.2.3.1-1: URI query parameters supported by the POST method on this resource

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description | Applicability |
| n/a |  |  |  |  |  |

This method shall support the request data structures specified in table 6.1.3.2.3.1-2 and the response data structures and response codes specified in table 6.1.3.2.3.1-3.

Table 6.1.3.2.3.1-2: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| MbsPolicyCtxtData | M | 1 | Contains the parameters to request the creation of an MBS Policy Association. |

Table 6.1.3.2.3.1-3: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| MbsPolicyData | M | 1 | 201 Created | Successful case. An Individual MBS Policy resource is successfully created. |
| n/a |  |  | 308 Permanent Redirect | Permanent Redirection. Another PCF already serves the MBS Session. |
| ProblemDetails | O | 0..1 | 400 Bad Request | (NOTE 2) |
| ProblemDetails | O | 0..1 | 403 Forbidden | (NOTE 2) |
| MbsExtProblemDetails | O | 0..1 | 403 Forbidden | (NOTE 2) |
| NOTE 1: The mandatory HTTP error status codes for the POST method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] also apply.  NOTE 2: Failure cases are described in clause 6.1.7. | | | | |

Table 6.1.3.2.3.1-4: Headers supported by the 201 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains the URI of the newly created resource, according to the structure:  {apiRoot}/npcf-mbspolicycontrol/<apiVersion>/mbs-policies/{mbsPolicyId} |

Table 6.1.3.2.3.1-5: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains the URI (i.e. "apiRoot") of the PCF currently handling the MBS Session and towards which the request is redirected. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Contains the identifier of the PCF (service) instance towards which the request is redirected. |

##### 6.1.3.2.4 Resource Custom Operations

There are no resource custom operations defined for this resource in this release of the specification.

#### 6.1.3.3 Resource: Individual MBS Policy

##### 6.1.3.3.1 Description

This resource represents an "Individual MBS Policy" resource managed by the PCF.

##### 6.1.3.3.2 Resource Definition

Resource URI: **{apiRoot}/npcf-mbspolicycontrol/<apiVersion>/mbs-policies/{mbsPolicyId}**

This resource shall support the resource URI variables defined in table 6.1.3.3.2-1.

Table 6.1.3.3.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 6.1.1. |
| mbsPolicyId | string | Represents the unique identifier of the "Individual MBS Policy" resource. |

##### 6.1.3.3.3 Resource Standard Methods

###### 6.1.3.3.3.1 GET

This method enables an NF service consumer (e.g. MB-SMF) to retrieve an existing "Individual MBS Policy" resource at the PCF.

This method shall support the URI query parameters specified in table 6.1.3.3.3.1-1.

Table 6.1.3.3.3.1-1: URI query parameters supported by the GET method on this resource

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description | Applicability |
| n/a |  |  |  |  |  |

This method shall support the request data structures specified in table 6.1.3.3.3.1-2 and the response data structures and response codes specified in table 6.1.3.3.3.1-3.

Table 6.1.3.3.3.1-2: Data structures supported by the GET Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| n/a |  |  |  |

Table 6.1.3.3.3.1-3: Data structures supported by the GET Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| MbsPolicyData | M | 1 | 200 OK | Successful case. The requested Individual MBS Policy resource is successfully returned in the response body. |
| RedirectResponse | O | 0..1 | 307 Temporary Redirect | Temporary redirection.  (NOTE 2) |
| RedirectResponse | O | 0..1 | 308 Permanent Redirect | Permanent redirection.  (NOTE 2) |
| NOTE 1: The mandatory HTTP error status codes for the GET method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] also apply.  NOTE 2: The RedirectResponse data structure may be provided by an SCP (cf. clause 6.10.9.1 of 3GPP TS 29.500 [4]). | | | | |

Table 6.1.3.3.3.1-4: Headers supported by the 307 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI of the resource located in an alternative PCF (service) instance towards which the request is redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target PCF (service) instance towards which the request is redirected. |

Table 6.1.3.3.3.1-5: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI of the resource located in an alternative PCF (service) instance towards which the request is redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target PCF (service) instance towards which the request is redirected. |

###### 6.1.3.3.3.2 DELETE

This method enables an NF service consumer (e.g. MB-SMF) to request the deletion of an existing "Individual MBS Policy" resource at the PCF.

This method shall support the URI query parameters specified in table 6.1.3.3.3.2-1.

Table 6.1.3.3.3.2-1: URI query parameters supported by the DELETE method on this resource

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description | Applicability |
| n/a |  |  |  |  |  |

This method shall support the request data structures specified in table 6.1.3.3.3.2-2 and the response data structures and response codes specified in table 6.1.3.3.3.2-3.

Table 6.1.3.3.3.2-2: Data structures supported by the DELETE Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| n/a |  |  |  |

Table 6.1.3.3.3.2-3: Data structures supported by the DELETE Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  Codes | Description |
| n/a |  |  | 204 No Content | Successful response. The Individual MBS Policy resource was successfully deleted. |
| RedirectResponse | O | 0..1 | 307 Temporary Redirect | Temporary redirection.  (NOTE 3) |
| RedirectResponse | O | 0..1 | 308 Permanent Redirect | Permanent redirection.  (NOTE 3) |
| ProblemDetails | O | 0..1 | 404 Not Found | (NOTE 2) |
| NOTE 1: The mandatory HTTP error status codes for the DELETE method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] also apply.  NOTE 2: Failure cases are described in clause 6.1.7.  NOTE 3: The RedirectResponse data structure may be provided by an SCP (cf. clause 6.10.9.1 of 3GPP TS 29.500 [4]). | | | | |

Table 6.1.3.3.3.2-4: Headers supported by the 307 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI of the resource located in an alternative PCF (service) instance towards which the request is redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target PCF (service) instance towards which the request is redirected. |

Table 6.1.3.3.3.2-5: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI of the resource located in an alternative PCF (service) instance towards which the request is redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target PCF (service) instance towards which the request is redirected. |

##### 6.1.3.3.4 Resource Custom Operations

###### 6.1.3.3.4.1 Overview

Table 6.1.3.3.4.1-1: Custom operations

|  |  |  |  |
| --- | --- | --- | --- |
| Operation name | Custom operaration URI | Mapped HTTP method | Description |
| Update | /mbs-policies/{mbsPolicyId}/update | Update  (POST) | Request the update of an existing MBS Policy Association. |

###### 6.1.3.3.4.2 Operation: Update

6.1.3.3.4.2.1 Description

This resource custom operation enables an NF service consumer (e.g. MB-SMF) to request the update of an existing MBS Policy Association at the PCF.

6.1.3.3.4.2.2 Operation Definition

This operation shall support the request data structures specified in table 6.1.3.3.4.2.2-1 and the response data structure and response codes specified in table 6.1.3.3.4.2.2-2.

Table 6.1.3.3.4.2.2-1: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| MbsPolicyCtxtDataUpdate | M | 1 | Contains the parameters to request the update of the Individual MBS Policy resource. |

Table 6.1.3.3.4.2.2-2: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| MbsPolicyData | M | 1 | 200 OK | Successful case. The targeted Individual MBS Policy resource is successfully updated. |
| RedirectResponse | O | 0..1 | 307 Temporary Redirect | Temporary redirection.  (NOTE 3) |
| RedirectResponse | O | 0..1 | 308 Permanent Redirect | Permanent redirection.  (NOTE 3) |
| ProblemDetails | O | 0..1 | 400 Bad Request | (NOTE 2) |
| ProblemDetails | O | 0..1 | 403 Forbidden | (NOTE 2) |
| MbsExtProblemDetails | O | 0..1 | 403 Forbidden | (NOTE 2) |
| ProblemDetails | O | 0..1 | 404 Not Found | (NOTE 2) |
| NOTE 1: The mandatory HTTP error status codes for the POST method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] also apply.  NOTE 2: Failure cases are described in clause 6.1.7.  NOTE 3: The RedirectResponse data structure may be provided by an SCP (cf. clause 6.10.9.1 of 3GPP TS 29.500 [4]). | | | | |

Table 6.1.3.3.4.2.2-3: Headers supported by the 307 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI of the resource located in an alternative PCF (service) instance towards which the request is redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target PCF (service) instance towards which the request is redirected. |

Table 6.1.3.3.4.2.2-4: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI of the resource located in an alternative PCF (service) instance towards which the request is redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target PCF (service) instance towards which the request is redirected. |

### 6.1.4 Custom Operations without associated resources

There are no custom operations without associated resources defined for this API in this release of the specification.

### 6.1.5 Notifications

There are no notifications defined for this API in this release of the specification.

### 6.1.6 Data Model

#### 6.1.6.1 General

This clause specifies the application data model supported by the API.

Table 6.1.6.1-1 specifies the data types defined for the Npcf\_MBSPolicyControl service based interface protocol.

Table 6.1.6.1-1: Npcf\_MBSPolicyControl specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Clause defined | Description | Applicability |
| MbsErrorReport | 6.1.6.2.10 | Contains the reporting of MBS Policy decision level failure(s) and/or MBS PCC rule level failure(s). |  |
| MbsFailureCode | 6.1.6.3.4 | Represents the reason behind the MBS Policy Decision(s) enforcement failure or the MBS PCC rule(s) installation failure. |  |
| MbsMaxDataBurstVol | 6.1.6.3.2 | Represents the maximum MBS data burst volume. |  |
| MbsPccRule | 6.1.6.2.7 | Represents the parameters constituting an MBS PCC rule. |  |
| MbsPcrt | 6.1.6.3.3 | Represents an MBS Policy Control Request Trigger. |  |
| MbsPolicyCtxtData | 6.1.6.2.2 | Contains the parameters used to request the creation of an Individual MBS Policy resource. |  |
| MbsPolicyCtxtDataUpdate | 6.1.6.2.11 | Contains the parameters to update an existing MBS Policy Association. |  |
| MbsPolicyData | 6.1.6.2.4 | Contains the MBS policy data of an Individual MBS Policy resource. |  |
| MbsPolicyDecision | 6.1.6.2.3 | Contains the parameters constituting an MBS Policy Decision. |  |
| MbsPccRuleStatus | 6.1.6.3.5 | Represents the status of an MBS PCC rule. |  |
| MbsQosChar | 6.1.6.2.9 | Represents the parameters constituting a set of explicitly signalled QoS Characteristics. |  |
| MbsQosDec | 6.1.6.2.8 | Represents the parameters constituting an MBS QoS Decision. |  |
| MbsReport | 6.1.6.2.12 | Includes the information about the MBS Policy Decision level failure(s) and/or the MBS PCC rule level failure(s). |  |

Table 6.1.6.1-2 specifies data types re-used by the Npcf\_MBSPolicyControl service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Npcf\_MBSPolicyControl service based interface.

Table 6.1.6.1-2: Npcf\_MBSPolicyControl re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| 5Qi | 3GPP TS 29.571 [15] | Indicates the 5G QoS Identifier. |  |
| 5QiPriorityLevel | 3GPP TS 29.571 [15] | Indicates the 5QI Priority Level. |  |
| AreaSessionPolicyId | 3GPP TS 29.571 [15] | Indicates the Area Session Policy Identifier. | AreaSessPolicy |
| Arp | 3GPP TS 29.571 [15] | Indicates the allocation and retention priority. |  |
| AverWindow | 3GPP TS 29.571 [15] | Indicates the Averaging Window. |  |
| BitRate | 3GPP TS 29.571 [15] | Indicates the Bit Rate. |  |
| Dnn | 3GPP TS 29.571 [15] | Identifies a DNN. |  |
| FlowDescription | 3GPP TS 29.512 [18] | Represents packet filtering information for an IP flow. |  |
| MbsExtProblemDetails | Clause 6.2.6.4.1 | Identifies the MBS related extensions to the ProblemDetails data structure. |  |
| MbsServiceInfo | 3GPP TS 29.571 [15] | Represents MBS Service Information. |  |
| MbsSessionId | 3GPP TS 29.571 [15] | Represents an MBS Session Identifier. |  |
| PacketDelBudget | 3GPP TS 29.571 [15] | Indicates the Packet Delay Budget. |  |
| PacketErrRate | 3GPP TS 29.571 [15] | Indicates the Packet Error Rate. |  |
| ProblemDetails | 3GPP TS 29.571 [15] | Contains error related additional information. |  |
| QosResourceType | 3GPP TS 29.571 [15] | Indicates the QoS resource type. |  |
| RedirectResponse | 3GPP TS 29.571 [15] | Contains redirection related information. |  |
| Snssai | 3GPP TS 29.571 [15] | Identifies an S-NSSAI. |  |
| SupportedFeatures | 3GPP TS 29.571 [15] | Represents the list of supported features. It is used to negotiate the applicability of the optional features. |  |
| Uinteger | 3GPP TS 29.571 [15] | Represents an unsigned integer. |  |

#### 6.1.6.2 Structured data types

##### 6.1.6.2.1 Introduction

This clause defines the structures to be used in resource representations.

##### 6.1.6.2.2 Type: MbsPolicyCtxtData

Table 6.1.6.2.2-1: Definition of type MbsPolicyCtxtData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| mbsSessionId | MbsSessionId | M | 1 | Represents the identifier of the MBS Session. |  |
| dnn | Dnn | O | 0..1 | Represents the DNN of the MBS session. |  |
| snssai | Snssai | O | 0..1 | Represents the S-NSSAI of the MBS session. |  |
| areaSessPolId | AreaSessionPolicyId | C | 0..1 | Represents the Area Session Policy ID.  This attribute shall be present if available. | AreaSessPolicy |
| mbsServInfo | MbsServiceInfo | O | 0..1 | Represents the MBS Service Information.  This attribute shall be provided, if available. |  |
| suppFeat | SupportedFeatures | C | 0..1 | Contains the list of the supported features among the ones defined in clause 6.1.8.  This attribute shall be present when feature negotiation needs to take place. |  |

##### 6.1.6.2.3 Type: MbsPolicyDecision

Table 6.1.6.2.3-1: Definition of type MbsPolicyDecision

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| mbsPccRules | map(MbsPccRule) | O | 1..N | A map of MBS PCC rule(s) with the content being the MbsPccRule as described in clause 6.1.6.2.7. The key used in this map for each entry is the "mbsPccRuleId" attribute of the corresponding MbsPccRule instance. |  |
| mbsQosDecs | map(MbsQosDec) | O | 1..N | Map of MBS QoS Decision(s). The key used in this map for each entry is the "mbsQosId" attribute of the corresponding MbsQosDec instance.  (NOTE) |  |
| mbsQosChars | map(MbsQosChar) | O | 1..N | Map of QoS characteristics for non-standard 5QIs and non-preconfigured 5QIs. The key of the map is the 5QI value within the "5qi" attribute of the corresponding MbsQosChar instance.  (NOTE) |  |
| authMbsSessAmbr | BitRate | O | 0..1 | The Authorized MBS Session-AMBR. |  |
| mbsPcrts | array(MbsPcrt) | O | 1..N | The MBS Policy Control Request Triggers(s) that the PCF requests to subscribe to. |  |
| NOTE: This attribute shall not be removed if it was provisioned. | | | | | |

##### 6.1.6.2.4 Type: MbsPolicyData

Table 6.1.6.2.4-1: Definition of type MbsPolicyData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| mbsPolicyCtxtData | MbsPolicyCtxtData | M | 1 | Contains the parameters used to request MBS Policy Association creation/update. |  |
| mbsPolicies | MbsPolicyDecision | C | 0..1 | Contains the provisioned MBS Policy Decision containing the MBS policies authorized by the PCF.  This attribute shall be present in the response to a request to create an MBS Policy Association or a request to retrieve the properties of an existing MBS Policy Association, and may be present in the response to a request to update an existing MBS Policy Association. |  |
| suppFeat | SupportedFeatures | C | 0..1 | Contains the list of negotiated supported features.  This parameter shall be provided by the PCF in the response to a request in which the NF service consumer provided the list of features that it supports. |  |

##### 6.1.6.2.5 Void

##### 6.1.6.2.6 Void

##### 6.1.6.2.7 Type: MbsPccRule

Table 6.1.6.2.7-1: Definition of type MbsPccRule

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| mbsPccRuleId | string | M | 1 | Univocally identifies the MBS PCC rule within the related MBS session. |  |
| mbsDlIpFlowInfo | array(FlowDescription) | C | 1..N | Contains the MBS downlink IP flow packet filter(s) information.  (NOTE 3) |  |
| precedence | Uinteger | O | 0..1 | Determines the order in which this MBS PCC rule is applied relative to other MBS PCC rules within the same MBS session.  (NOTE 1) |  |
| refMbsQosDec | array(string) | C | 1..N | A reference to the MbsQosDec policy decision type. It contains the value of the "mbsQosId" attribute of the referred MbsQosDec policy decision defined in clause 6.1.6.2.8.  (NOTE 2, NOTE 3) |  |
| NOTE 1: The "precedence" attribute is used to specify the precedence of the MBS PCC rule among all MBS PCC rules associated to an MBS session. It includes an integer value in the range of 0 to 255 (decimal). The higher the value of the "precedence" attribute, the lower the precedence of the MBS PCC rule to which it applies.  NOTE 2: Arrays are only introduced for future compatibility. In this release of the specification, the maximum number of elements in the array is 1.  NOTE 3: This attribute shall be present in the response to an MBS Policy Association Creation request and may be present in the response to an MBS Policy Association Update request. | | | | | |

##### 6.1.6.2.8 Type: MbsQosDec

Table 6.1.6.2.8-1: Definition of type MbsQosDec

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| mbsQosId | string | M | 1 | Univocally identifies the MBS QoS Decision within the related MBS session. |  |
| 5qi | 5Qi | O | 0..1 | Contains the identifier of the authorized QoS parameters for the MBS service data flow.  (NOTE 2) |  |
| priorityLevel | 5QiPriorityLevel | O | 0..1 | Indicates a priority in scheduling resources among MBS QoS flows.  (NOTE 1) |  |
| mbrDl | BitRate | O | 0..1 | Indicates the maximum bandwidth in downlink. |  |
| gbrDl | BitRate | O | 0..1 | Indicates the guaranteed bandwidth in downlink. |  |
| arp | Arp | O | 0..1 | Indicates the allocation and retention priority. |  |
| averWindow | AverWindow | O | 0..1 | Represents the duration over which the guaranteed and maximum bitrates shall be calculated.  (NOTE 1) |  |
| mbsMaxDataBurstVol | MbsMaxDataBurstVol | O | 0..1 | Denotes the largest amount of data that is required to be transferred within a period.  (NOTE 1) |  |
| NOTE 1: This attribute is applicable only when a value different from the standardized 5QI values, defined in table 5.7.4-1 3GPP TS 23.501 [2], is provided.  NOTE 2: When the provided 5QI value is a dynamically assigned 5QI (i.e. from the non-standardized and non-preconfigured value range), the corresponding QoS parameters (e.g. Packet Delay Budget, Packet Error Rate, etc.) are provided in the corresponding MbsQosChar data structure. | | | | | |

##### 6.1.6.2.9 Type: MbsQosChar

Table 6.1.6.2.9-1: Definition of type MbsQosChar

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| 5qi | 5Qi | M | 1 | Represents the identifier of the set of non-standardized and non-preconfigured MBS QoS parameters for an MBS service data flow. |  |
| resourceType | QosResourceType | M | 1 | Indicates whether the MBS QoS resource type is GBR, delay critical GBR or non-GBR. |  |
| priorityLevel | 5QiPriorityLevel | M | 1 | Indicates the 5QI Priority Level within a range of 1 to 127 and encoded as an unsigned integer. |  |
| packetDelayBudget | PacketDelBudget | M | 1 | Indicates the packet delay budget expressed in milliseconds and encoded as an unsigned integer. |  |
| packetErrorRate | PacketErrRate | M | 1 | Indicates the packet error rate encoded as a string.  Examples:  - A Packer Error Rate of 4x10-6 shall be encoded as "4E-6".  - A Packer Error Rate of 10-2 shall be encoded as"1E-2". |  |
| averWindow | AverWindow | C | 0..1 | Indicates the averaging window.  This attribute shall be present only for a GBR QoS flow or a Delay Critical GBR QoS flow. |  |
| mbsMaxDataBurstVol | MbsMaxDataBurstVol | M | 1 | Indicates the maximum data burst volume, encoded as an unsigned integer. |  |

##### 6.1.6.2.10 Type: MbsErrorReport

Table 6.1.6.2.11-1: Definition of type MbsErrorReport

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| mbsReports | array(MbsReport) | O | 1..N | Contains the reporting of MBS Policy decision level failure(s) and/or MBS PCC rule level failure(s). |  |

##### 6.1.6.2.11 Type: MbsPolicyCtxtDataUpdate

Table 6.1.6.2.11-1: Definition of type MbsPolicyCtxtDataUpdate

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| mbsServInfo | MbsServiceInfo | O | 0..1 | Represents the updated MBS Service Information. |  |
| mbsPcrts | array(MbsPcrt) | O | 1..N | Represents the list of MBS Policy Control Request Triggers that are met. |  |
| mbsErrorReport | MbsErrorReport | O | 0..1 | Contains the reporting of MBS Policy decision level failure(s) and/or MBS PCC rule level failure(s). |  |

##### 6.1.6.2.12 Type: MbsReport

Table 6.1.6.2.12-1: Definition of type MbsReport

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| mbsPccRuleIds | array(string) | C | 1..N | Contains the identifier(s) of the affected MBS PCC rule(s).  This attribute shall be present if the reported failure is related to the MBS PCC rule(s) installation.  (NOTE) |  |
| mbsPccRuleStatus | MbsPccRuleStatus | C | 0..1 | Indicates the status of the MBS PCC rule(s) identified by the "mbsPccRuleIds" attribute.  This attribute shall be present only if the "mbsPccRuleIds" attribute is present. |  |
| failureCode | MbsFailureCode | C | 0..1 | Indicates the reason of the failure of the MBS Policy Decision or the MBS PCC rule(s) identified by the "mbsPccRuleIds" attribute.  This attribute shall be present when available.  (NOTE) |  |
| NOTE: If the reported failure is due to MBS Policy Decision failure, then the "mbsPccRuleIds" attribute shall not be present and the "failureCode" attribute indicates the appropriate failure cause illustrating the MBS Policy Decision failure that occurred. | | | | | |

#### 6.1.6.3 Simple data types and enumerations

##### 6.1.6.3.1 Introduction

This clause defines simple data types and enumerations that can be referenced from data structures defined in the previous clauses.

##### 6.1.6.3.2 Simple data types

The simple data types defined in table 6.1.6.3.2-1 shall be supported.

Table 6.1.6.3.2-1: Simple data types

|  |  |  |  |
| --- | --- | --- | --- |
| Type Name | Type Definition | Description | Applicability |
| MbsMaxDataBurstVol | Integer | Represents MBS Maximum Data Burst Volume expressed in Bytes.  Minimum = 1. Maximum = 2000000. |  |

##### 6.1.6.3.3 Enumeration: MbsPcrt

The enumeration MbsPcrt represents the MBS Policy Control Request Triggers. It shall comply with the provisions defined in table 6.1.6.3.3-1.

Table 6.1.6.3.3-1: Enumeration MbsPcrt

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| MBS\_SESSION\_UPDATE | Indicates the MBS Session Update policy control request trigger.  This MBS Policy Control Request Trigger is implicitly subscribed by the PCF, i.e. pre-configured at the NF service consumer (MB-SMF). |  |

##### 6.1.6.3.4 Enumeration: MbsFailureCode

The enumeration MbsFailureCode represents the reason behind the MBS Policy Decision failure. It shall comply with the provisions of table 6.1.6.3.4-1.

Table 6.1.6.3.4-1: Enumeration MbsFailureCode

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| NF\_MALFUNCTION | Indicates that the MBS PCC rule could not be successfully installed due to MB-SMF/MB-UPF malfunction. |  |
| NF\_RESOURCES\_UNAVAILABLE | Indicates that the MBS PCC rule could not be successfully installed due to resources unavailable at the MB-SMF/MB-UPF. |  |
| RESOURCE\_ALLOCATION\_FAILURE | Indicates that the MBS PCC rule could not be successfully installed or maintained since the associated MBS QoS flow establishment/modification failed or the associated MBS QoS flow was released. |  |
| MBS\_QOS\_VALIDATION\_FAILURE | Indicate that MBS QoS validation has failed. |  |
| NO\_MBS\_QOS\_FLOW | Indicates that there is no MBS QoS flow to which the MB-SMF can bind the MBS PCC rule(s). |  |
| MBS\_QOS\_DECISION\_ERROR | Indicates failure in the provisioning of MBS QoS Decision data. |  |
| MBS\_POLICY\_PARAM\_ERROR | Indicates that the information related to the provisioned MBS policy parameter(s) is incorrect, incomplete or inconsistent. |  |

##### 6.1.6.3.5 Enumeration: MbsPccRuleStatus

The enumeration MbsPccRuleStatus represents the status of an MBS PCC rule. It shall comply with the provisions of table 6.1.6.3.5-1.

Table 6.1.6.3.5-1: Enumeration MbsPccRuleStatus

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| ACTIVE | Indicates that the MBS PCC rule(s) are successfully installed. |  |
| INACTIVE | Indicates that the MBS PCC rule(s) are removed. |  |

#### 6.1.6.4 Data types describing alternative data types or combinations of data types

There are no data types describing alternative data types or combinations of data types defined for this API in this release of the specification.

#### 6.1.6.5 Binary data

##### 6.1.6.5.1 Binary Data Types

Table 6.1.6.5.1-1: Binary Data Types

|  |  |  |
| --- | --- | --- |
| Name | Clause defined | Content type |
|  |  |  |

### 6.1.7 Error Handling

#### 6.1.7.1 General

For the Npcf\_MBSPolicyControl API, HTTP error responses shall be supported as specified in clause 4.8 of 3GPP TS 29.501 [5]. Protocol errors and application errors specified in table 5.2.7.2-1 of 3GPP TS 29.500 [4] shall be supported for an HTTP method if the corresponding HTTP status codes are specified as mandatory for that HTTP method in table 5.2.7.1-1 of 3GPP TS 29.500 [4].

In addition, the requirements in the following clauses are applicable for the Npcf\_MBSPolicyControl API.

#### 6.1.7.2 Protocol Errors

No specific procedures for the Npcf\_MBSPolicyControl service are specified.

#### 6.1.7.3 Application Errors

The application errors defined for the Npcf\_MBSPolicyControl service are listed in Table 6.1.7.3-1.

Table 6.1.7.3-1: Application errors

|  |  |  |
| --- | --- | --- |
| Application Error | HTTP status code | Description |
| INVALID\_MBS\_SERVICE\_INFO | 400 Bad Request | The HTTP request is rejected because the provided MBS Service Information is invalid (e.g. invalid QoS reference), incorrect or insufficient for the PCF to perform MBS policy authorization. |
| FILTER\_RESTRICTIONS\_NOT\_RESPECTED | 400 Bad Request | The HTTP request is rejected because the MBS IP flow(s) description provided within the MBS Service Information cannot be handled due to the restrictions defined in clause 5.3.8 of 3GPP TS 29.214 [19] not being respected. |
| ERROR\_INPUT\_PARAMETERS | 400 Bad Request | The HTTP request is rejected because the provided set of input parameters are incomplete, erroneous or missing necessary information for the PCF to perform MBS policy control. |
| MBS\_SERVICE\_INFO\_NOT\_AUTHORIZED | 403 Forbidden | The HTTP request is rejected because the provided MBS Service Information is not authorized by the PCF. |
| MBS\_POLICY\_CONTEXT\_DENIED | 403 Forbidden | The HTTP request is rejected because the PCF does not accept the NF service consumer request due to operator policies and/or local configuration. |
| MBS\_POLICY\_ASSOCIATION\_NOT\_FOUND | 404 Not Found | The HTTP request is rejected because the targeted MBS Policy Association does not exist at the PCF. |

### 6.1.8 Feature negotiation

The optional features listed in table 6.1.8-1 are defined for the Npcf\_MBSPolicyControl API. They shall be negotiated using the extensibility mechanism defined in clause 6.6 of 3GPP TS 29.500 [4].

Table 6.1.8-1: Supported Features

|  |  |  |
| --- | --- | --- |
| Feature number | Feature Name | Description |
| 1 | AreaSessPolicy | This feature indicates the support of the Area Session Policy ID related handling for location-dependent MBS services.  The following functionalities are supported:  - Support the provisioning of the Area Session Policy ID to the PCF for MBS Sessions that are instances of a location-dependent MBS service. |

### 6.1.9 Security

As indicated in 3GPP TS 33.501 [8] and 3GPP TS 29.500 [4], the access to the Npcf\_MBSPolicyControl API may be authorized by means of the OAuth2 protocol (see IETF RFC 6749 [9]), based on local configuration, using the "Client Credentials" authorization grant, where the NRF (see 3GPP TS 29.510 [10]) plays the role of the authorization server.

If OAuth2 is used, an NF Service Consumer, prior to consuming services offered by the Npcf\_MBSPolicyControl API, shall obtain a "token" from the authorization server, by invoking the Access Token Request service, as described in 3GPP TS 29.510 [10], clause 5.4.2.2.

NOTE: When multiple NRFs are deployed in a network, the NRF used as authorization server is the same NRF that the NF Service Consumer used for discovering the Npcf\_MBSPolicyControl service.

The Npcf\_MBSPolicyControl API defines a single scope "npcf-mbspolicycontrol" for the entire service, and it does not define any additional scopes at resource or operation level.

## 6.2 Npcf\_MBSPolicyAuthorization Service API

### 6.2.1 Introduction

The Npcf\_MBSPolicyAuthorization Service shall use the Npcf\_MBSPolicyAuthorization API.

The API URI of the Npcf\_MBSPolicyAuthorization Service shall be:

**{apiRoot}/<apiName>/<apiVersion>**

The request URIs used in HTTP requests from the NF service consumer towards the NF service producer shall have the Resource URI structure defined in clause 4.4.1 of 3GPP TS 29.501 [5], i.e.:

**{apiRoot}/<apiName>/<apiVersion>/<apiSpecificResourceUriPart>**

with the following components:

- The {apiRoot} shall be set as described in 3GPP TS 29.501 [5].

- The <apiName>shall be "npcf-mbspolicyauth".

- The <apiVersion> shall be "v1".

- The <apiSpecificResourceUriPart> shall be set as described in clause 6.2.3.

### 6.2.2 Usage of HTTP

#### 6.2.2.1 General

HTTP/2, IETF RFC 9113 [11], shall be used as specified in clause 5 of 3GPP TS 29.500 [4].

HTTP/2 shall be transported as specified in clause 5.3 of 3GPP TS 29.500 [4].

The OpenAPI [6] specification of HTTP messages and content bodies for the Npcf\_MBSPolicyAuthorization API is contained in Annex A.2.

#### 6.2.2.2 HTTP standard headers

##### 6.2.2.2.1 General

See clause 5.2.2 of 3GPP TS 29.500 [4] for the usage of HTTP standard headers.

##### 6.2.2.2.2 Content type

JSON, IETF RFC 8259 [12], shall be used as content type of the HTTP bodies specified in the present specification as specified in clause 5.4 of 3GPP TS 29.500 [4]. The use of the JSON format shall be signalled by the content type "application/json".

JSON object used in the HTTP PATCH request shall be encoded according to "JSON Merge Patch" and shall be signalled by the content type "application/merge-patch+json", as defined in IETF RFC 7396 [22].

The "Problem Details" JSON object shall be used to indicate additional details of the error in a HTTP response body and shall be signalled by the content type "application/problem+json", as defined in IETF RFC 9754 [13].

#### 6.2.2.3 HTTP custom headers

The mandatory HTTP custom header fields specified in clause 5.2.3.2 of 3GPP TS 29.500 [4] shall be supported, and the optional HTTP custom header fields specified in clause 5.2.3.3 of 3GPP TS 29.500 [4] may be supported.

### 6.2.3 Resources

#### 6.2.3.1 Overview

This clause describes the structure of the resource URIs and the resources and methods used for the Npcf\_MBSPolicyAuthorization service.

Figure 6.2.3.1-1 depicts the resource URIs structure for the Npcf\_MBSPolicyAuthorization API.



Figure 6.2.3.1-1: Resource URI structure of the Npcf\_MBSPolicyAuthorization API

Table 6.2.3.1-1 provides an overview of the resources and applicable HTTP methods.

Table 6.2.3.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource purpose/name | Resource URI (relative path after API URI) | HTTP method or custom operation | Description (service operation) |
| MBS Application Session Contexts | /contexts | POST | Create a new MBS Application Session Context. |
| Individual MBS Application Session Context | /contexts/{contextId} | GET | Retrieve an existing Individual MBS Application Session Context resource. |
| PATCH | Modify an existing Individual MBS Application Session Context resource. |
| DELETE | Delete an existing Individual MBS Application Session Context resource. |

#### 6.2.3.2 Resource: MBS Application Session Contexts

##### 6.2.3.2.1 Description

This resource represents the collection of "Individual MBS Application Session Context" resources managed by the PCF.

##### 6.2.3.2.2 Resource Definition

Resource URI: **{apiRoot}/npcf-mbspolicyauth/<apiVersion>/contexts**

This resource shall support the resource URI variables defined in table 6.2.3.2.2-1.

Table 6.2.3.2.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 6.2.1. |

##### 6.2.3.2.3 Resource Standard Methods

###### 6.2.3.2.3.1 POST

This method enables an NF service consumer (e.g. NEF, MBSF, AF) to request the creation of an MBS Application Session Context at the PCF.

This method shall support the URI query parameters specified in table 6.2.3.2.3.1-1.

Table 6.2.3.2.3.1-1: URI query parameters supported by the POST method on this resource

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description | Applicability |
| n/a |  |  |  |  |  |

This method shall support the request data structures specified in table 6.2.3.2.3.1-2 and the response data structures and response codes specified in table 6.2.3.2.3.1-3.

Table 6.2.3.2.3.1-2: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| MbsAppSessionCtxt | M | 1 | Contains the parameters to create an Individual MBS Application Session Context for MBS policy authorization. |

Table 6.2.3.2.3.1-3: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| MbsAppSessionCtxt | M | 1 | 201 Created | Successful case. An Individual MBS Application Session Context resource is successfully created and a representation of the created resource is returned in the response body.  A Location header field containing the URI of the created resource is also included. |
| ProblemDetails | O | 0..1 | 400 Bad Request | (NOTE 2) |
| MbsExtProblemDetails | O | 0..1 | 403 Forbidden | (NOTE 2) |
| NOTE 1: The mandatory HTTP error status codes for the HTTP POST method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] also apply.  NOTE 2: Failure cases are described in clause 6.2.7. | | | | |

Table 6.2.3.2.3.1-4: Headers supported by the POST method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains the URI of the newly created resource, according to the structure: {apiRoot}/npcf-mbspolicyauth/<apiVersion>/contexts/{contextId} |

##### 6.2.3.2.4 Resource Custom Operations

There are no resource custom operations defined for this resource in this release of the specification.

#### 6.2.3.3 Resource: Individual MBS Application Session Context

##### 6.2.3.3.1 Description

This resource represents an "Individual MBS Application Session Context" resource managed by the PCF.

##### 6.2.3.3.2 Resource Definition

Resource URI: **{apiRoot}/npcf-mbspolicyauth/<apiVersion>/contexts/{contextId}**

This resource shall support the resource URI variables defined in table 6.2.3.3.2-1.

Table 6.2.3.3.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 6.2.1. |
| contextId | string | Represents the unique identifier of the "Individual MBS Application Session Context" resource. |

##### 6.2.3.3.3 Resource Standard Methods

###### 6.2.3.3.3.1 GET

This method enables an NF service consumer (e.g. NEF, MBSF, AF) to retrieve an existing "Individual MBS Application Session Context" resource at the PCF.

This method shall support the URI query parameters specified in table 6.2.3.3.3.1-1.

Table 6.2.3.3.3.1-1: URI query parameters supported by the GET method on this resource

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description | Applicability |
| n/a |  |  |  |  |  |

This method shall support the request data structures specified in table 6.2.3.3.3.1-2 and the response data structures and response codes specified in table 6.2.3.3.3.1-3.

Table 6.2.3.3.3.1-2: Data structures supported by the GET Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| n/a |  |  |  |

Table 6.2.3.3.3.1-3: Data structures supported by the GET Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| MbsAppSessionCtxt | M | 1 | 200 OK | Successful case. The requested Individual MBS Application Session Context resource is successfully returned. |
| RedirectResponse | O | 0..1 | 307 Temporary Redirect | Temporary redirection.  (NOTE 2) |
| RedirectResponse | O | 0..1 | 308 Permanent Redirect | Permanent redirection.  (NOTE 2) |
| NOTE 1: The mandatory HTTP error status codes for the HTTP GET method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] also apply.  NOTE 2: The RedirectResponse data structure may be provided by an SCP (cf. clause 6.10.9.1 of 3GPP TS 29.500 [4]). | | | | |

Table 6.2.3.3.3.1-4: Headers supported by the 307 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI of the resource located in an alternative PCF (service) instance towards which the request is redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target PCF (service) instance towards which the request is redirected. |

Table 6.2.3.3.3.1-5: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI of the resource located in an alternative PCF (service) instance towards which the request is redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target PCF (service) instance towards which the request is redirected. |

###### 6.2.3.3.3.2 PATCH

This method enables an NF service consumer (e.g. NEF, MBSF, AF) to request the modification of an existing "Individual MBS Application Session Context" resource at the PCF.

This method shall support the URI query parameters specified in table 6.2.3.3.3.2-1.

Table 6.2.3.3.3.2-1: URI query parameters supported by the PATCH method on this resource

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description | Applicability |
| n/a |  |  |  |  |  |

This method shall support the request data structures specified in table 6.2.3.3.3.2-2 and the response data structures and response codes specified in table 6.2.3.3.3.2-3.

Table 6.2.3.3.3.2-2: Data structures supported by the PATCH Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| MbsAppSessionCtxtPatch | M | 1 | Contains the parameters to request the modification of an existing Individual MBS Application Session Context resource. |

Table 6.2.3.3.3.2-3: Data structures supported by the PATCH Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| MbsAppSessionCtxt | M | 1 | 200 OK | Successful case. The corresponding Individual MBS Application Session Context resource is successfully modified and a representation of the updated resource is returned in the response body. |
| n/a |  |  | 204 No Content | Successful case. The corresponding Individual MBS Application Session Context resource is successfully modified and no content is returned in the response body. |
| RedirectResponse | O | 0..1 | 307 Temporary Redirect | Temporary redirection.  (NOTE 3) |
| RedirectResponse | O | 0..1 | 308 Permanent Redirect | Permanent redirection.  (NOTE 3) |
| ProblemDetails | O | 0..1 | 400 Bad Request | (NOTE 2) |
| MbsExtProblemDetails | O | 0..1 | 403 Forbidden | (NOTE 2) |
| ProblemDetails | O | 0..1 | 404 Not Found | (NOTE 2) |
| NOTE 1: The mandatory HTTP error status codes for the HTTP PATCH method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] also apply.  NOTE 2: Failure cases are described in clause 6.2.7.  NOTE 3: The RedirectResponse data structure may be provided by an SCP (cf. clause 6.10.9.1 of 3GPP TS 29.500 [4]). | | | | |

Table 6.2.3.3.3.2-4: Headers supported by the 307 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI of the resource located in an alternative PCF (service) instance towards which the request is redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target PCF (service) instance towards which the request is redirected. |

Table 6.2.3.3.3.2-5: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI of the resource located in an alternative PCF (service) instance towards which the request is redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target PCF (service) instance towards which the request is redirected. |

###### 6.2.3.3.3.3 DELETE

This method enables an NF service consumer (e.g. NEF, MBSF, AF) to request the deletion of an existing "Individual MBS Application Session Context" resource at the PCF.

This method shall support the URI query parameters specified in table 6.2.3.3.3.3-1.

Table 6.2.3.3.3.3-1: URI query parameters supported by the DELETE method on this resource

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description | Applicability |
| n/a |  |  |  |  |  |

This method shall support the request data structures specified in table 6.2.3.3.3.3-2 and the response data structures and response codes specified in table 6.2.3.3.3.3-3.

Table 6.2.3.3.3.3-2: Data structures supported by the DELETE Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| n/a |  |  |  |

Table 6.2.3.3.3.3-3: Data structures supported by the DELETE Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| n/a |  |  | 204 No Content | Successful case. The corresponding Individual MBS Application Session Context resource is successfully deleted. |
| RedirectResponse | O | 0..1 | 307 Temporary Redirect | Temporary redirection.  (NOTE 3) |
| RedirectResponse | O | 0..1 | 308 Permanent Redirect | Permanent redirection.  (NOTE 3) |
| ProblemDetails | O | 0..1 | 404 Not Found | (NOTE 2) |
| NOTE 1: The mandatory HTTP error status codes for the HTTP DELETE method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] also apply.  NOTE 2: Failure cases are described in clause 6.2.7.  NOTE 3: The RedirectResponse data structure may be provided by an SCP (cf. clause 6.10.9.1 of 3GPP TS 29.500 [4]). | | | | |

Table 6.2.3.3.3.3-4: Headers supported by the 307 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI of the resource located in an alternative PCF (service) instance towards which the request is redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target PCF (service) instance towards which the request is redirected. |

Table 6.2.3.3.3.3-5: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI of the resource located in an alternative PCF (service) instance towards which the request is redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target PCF (service) instance towards which the request is redirected. |

##### 6.2.3.3.4 Resource Custom Operations

There are no resource custom operations defined for this resource in this release of the specification.

### 6.2.4 Custom Operations without associated resources

There are no custom operations without associated resources defined for this API in this release of the specification.

### 6.2.5 Notifications

There are no notifications defined for this API in this release of the specification.

### 6.2.6 Data Model

#### 6.2.6.1 General

This clause specifies the application data model supported by the API.

Table 6.2.6.1-1 specifies the data types defined for the Npcf\_MBSPolicyAuthorization service based interface protocol.

Table 6.2.6.1-1: Npcf\_MBSPolicyAuthorization specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Clause defined | Description | Applicability |
| AcceptableMbsServInfo | 6.2.6.2.4 | Contains the MBS Service Information that can be accepted by the PCF. |  |
| MbsExtProblemDetails | 6.2.6.4.1 | Identifies the MBS related extensions to the ProblemDetails data structure. |  |
| MbsAppSessionCtxt | 6.2.6.2.2 | Represents the parameters of an MBS Application Session Context. |  |
| MbsAppSessionCtxtPatch | 6.2.6.2.3 | Represents the modifications to an existing MBS Application Session Context. |  |

Table 6.2.6.1-2 specifies data types re-used by the Npcf\_MBSPolicyAuthorization service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Npcf\_MBSPolicyAuthorization service based interface.

Table 6.2.6.1-2: Npcf\_MBSPolicyAuthorization re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| AreaSessionPolicyId | 3GPP TS 29.571 [15] | Indicates the Area Session Policy Identifier. | AreaSessPolicy |
| BitRate | 3GPP TS 29.571 [15] | Represents a bit rate. |  |
| Dnn | 3GPP TS 29.571 [15] | Identifies a DNN. |  |
| MbsMediaComp | 3GPP TS 29.571 [15] | Represents an MBS Media Component. |  |
| MbsServiceInfo | 3GPP TS 29.571 [15] | Represents MBS Service Information. |  |
| MbsSessionId | 3GPP TS 29.571 [15] | Represents an MBS Session Identifier. |  |
| ProblemDetails | 3GPP TS 29.571 [15] | Contains error related additional information. |  |
| RedirectResponse | 3GPP TS 29.571 [15] | Contains redirection related information. |  |
| Snssai | 3GPP TS 29.571 [15] | Identifies an S-NSSAI. |  |
| SupportedFeatures | 3GPP TS 29.571 [15] | Represents the list of supported features. It is used to negotiate the applicability of the optional features. |  |

#### 6.2.6.2 Structured data types

##### 6.2.6.2.1 Introduction

This clause defines the structures to be used in resource representations.

##### 6.2.6.2.2 Type: MbsAppSessionCtxt

Table 6.2.6.2.2-1: Definition of type MbsAppSessionCtxt

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| mbsSessionId | MbsSessionId | M | 1 | Represents the identifier of the corresponding MBS Session. |  |
| mbsServInfo | MbsServiceInfo | C | 0..1 | Represents the MBS Service Information.  This attribute shall be provided, if available. |  |
| dnn | Dnn | O | 0..1 | Represents the DNN of the MBS session. |  |
| snssai | Snssai | O | 0..1 | Represents the S-NSSAI of the MBS session. |  |
| areaSessPolId | AreaSessionPolicyId | C | 0..1 | Contains the Area Session Policy ID.  This attribute may be present only in the response to an MBS Application Session Context creation request.  This attribute shall be present if the "reqForLocDepMbs" attribute was present and set to "true" in the corresponding request. | AreaSessPolicy |
| reqForLocDepMbs | boolean | O | 0..1 | Indicates whether the request corresponds to a location-dependent MBS service, i.e.:  - "true" means that the request corresponds to a location-dependent MBS service.  - "false" means that the request does not correspond to a location-dependent MBS service.  - When this attribute is not present, the default value is "false".  This attribute may be present only in a request to create an MBS Application Session Context. It shall not be present otherwise. | AreaSessPolicy |
| contactPcfInd | boolean | O | 0..1 | Indicates whether the PCF shall be contacted or not, i.e.:  - "true" means that the PCF shall be contacted.  - "false" means that the PCF shall not be contacted.  - When this attribute is not present, the default value is "false".  This attribute may be present only in the response to an MBS Application Session Context update request. |  |
| suppFeat | SupportedFeatures | C | 0..1 | Contains the list of the supported features (among the ones defined in clause 6.2.8).  This parameter shall be provided if feature negotiation needs to take place. |  |

##### 6.2.6.2.3 Type: MbsAppSessionCtxtPatch

Table 6.2.6.2.3-1: Definition of type MbsAppSessionCtxtPatch

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| mbsServInfo | MbsServiceInfo | O | 0..1 | Represents the updated MBS Service Information. |  |

##### 6.2.6.2.4 Type: AcceptableMbsServInfo

Table 6.2.6.2.4-1: Definition of type AcceptableMbsServInfo

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| accMbsServInfo | map(MbsMediaComp) | C | 1..N | Contains the maximum acceptable bandwidth per media component that can be accepted and authorized by the PCF.  Each map entry encoded using the MbsMediaComp data structure shall only include the "mbsMedCompNum" attribute and the "maxReqMbsBwDl" attribute indicating the maximum acceptable bandwidth.  The key of the map is the "medCompN" attribute of the corresponding MbsMediaComp data structure provided as a map entry.  (NOTE) |  |
| accMaxMbsBw | BitRate | C | 0..1 | Contains the maximum acceptable bandwidth.  (NOTE) |  |
| NOTE: When the acceptable MBS bandwidth is per MBS media component, only the "accMbsServInfo" attribute shall be present. When the acceptable MBS bandwidth applies to all the MBS media components, only the "accMaxMbsBw" attribute shall be present. | | | | | |

#### 6.2.6.3 Simple data types and enumerations

##### 6.2.6.3.1 Introduction

This clause defines simple data types and enumerations that can be referenced from data structures defined in the previous clauses.

##### 6.2.6.3.2 Simple data types

The simple data types defined in table 6.2.6.3.2-1 shall be supported.

Table 6.2.6.3.2-1: Simple data types

|  |  |  |  |
| --- | --- | --- | --- |
| Type Name | Type Definition | Description | Applicability |
|  |  |  |  |

#### 6.2.6.4 Data types describing alternative data types or combinations of data types

##### 6.2.6.4.1 Type: MbsExtProblemDetails

Table 6.2.6.4.1-1: Definition of type MbsExtProblemDetails as a list of to be combined data types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Cardinality | Description | Applicability |
| ProblemDetails | 1 | Contains the details of the encountered problem, as defined in 3GPP TS 29.571 [15]. |  |
| AcceptableMbsServInfo | 0..1 | Contains the MBS Service Information that can be accepted by the PCF. |  |

#### 6.2.6.5 Binary data

##### 6.2.6.5.1 Binary Data Types

Table 6.2.6.5.1-1: Binary Data Types

|  |  |  |
| --- | --- | --- |
| Name | Clause defined | Content type |
|  |  |  |

### 6.2.7 Error Handling

#### 6.2.7.1 General

For the Npcf\_MBSPolicyAuthorization API, HTTP error responses shall be supported as specified in clause 4.8 of 3GPP TS 29.501 [5]. Protocol errors and application errors specified in table 5.2.7.2-1 of 3GPP TS 29.500 [4] shall be supported for an HTTP method if the corresponding HTTP status codes are specified as mandatory for that HTTP method in table 5.2.7.1-1 of 3GPP TS 29.500 [4].

In addition, the requirements in the following clauses are applicable for the Npcf\_MBSPolicyAuthorization API.

#### 6.2.7.2 Protocol Errors

No specific procedures for the Npcf\_MBSPolicyAuthorization service are specified.

#### 6.2.7.3 Application Errors

The application errors defined for the Npcf\_MBSPolicyAuthorization service are listed in table 6.2.7.3-1.

Table 6.2.7.3-1: Application errors

|  |  |  |
| --- | --- | --- |
| Application Error | HTTP status code | Description |
| INVALID\_MBS\_SERVICE\_INFO | 400 Bad Request | The HTTP request is rejected because the provided MBS Service Information is invalid (e.g. invalid QoS reference), incorrect or insufficient for the PCF to perform MBS policy authorization. |
| FILTER\_RESTRICTIONS\_NOT\_RESPECTED | 400 Bad Request | The HTTP request is rejected because the MBS IP flow(s) description provided within the MBS Service Information cannot be handled due to the restrictions defined in clause 5.3.8 of 3GPP TS 29.214 [19] not being respected. |
| MBS\_SERVICE\_INFO\_NOT\_AUTHORIZED | 403 Forbidden | The HTTP request is rejected because the provided MBS Service Information is not authorized by the PCF. |
| MBS\_SESSION\_POL\_AUTH\_CTXT\_NOT\_FOUND | 404 Not Found | The HTTP request is rejected because the targeted Individual MBS Application Session Context does not exist at the PCF. |

### 6.2.8 Feature negotiation

The optional features listed in table 6.2.8-1 are defined for the Npcf\_MBSPolicyAuthorization API. They shall be negotiated using the extensibility mechanism defined in clause 6.6 of 3GPP TS 29.500 [4].

Table 6.2.8-1: Supported Features

|  |  |  |
| --- | --- | --- |
| Feature number | Feature Name | Description |
| 1 | AreaSessPolicy | This feature indicates the support of the Area Session Policy ID related handling for location-dependent MBS services.  The following functionalities are supported:  - Support the provisioning of the "request for location dependent MBS session" indication to the PCF for MBS Sessions that are instances of a location-dependent MBS service.  - Support that the PCF assigns and returns to the NF service consumer an Area Session Policy ID for an MBS Session that is an instance of a location-dependent MBS service. |

### 6.2.9 Security

As indicated in 3GPP TS 33.501 [8] and 3GPP TS 29.500 [4], the access to the Npcf\_MBSPolicyAuthorization API may be authorized by means of the OAuth2 protocol (see IETF RFC 6749 [9]), based on local configuration, using the "Client Credentials" authorization grant, where the NRF (see 3GPP TS 29.510 [10]) plays the role of the authorization server.

If OAuth2 is used, an NF Service Consumer, prior to consuming services offered by the Npcf\_MBSPolicyAuthorization API, shall obtain a "token" from the authorization server, by invoking the Access Token Request service, as described in 3GPP TS 29.510 [10], clause 5.4.2.2.

NOTE: When multiple NRFs are deployed in a network, the NRF used as authorization server is the same NRF that the NF Service Consumer used for discovering the Npcf\_MBSPolicyAuthorization service.

The Npcf\_MBSPolicyAuthorization API defines a single scope "npcf-mbspolicyauth" for the entire service, and it does not define any additional scopes at resource or operation level.

Annex A (normative):  
OpenAPI specification

# A.1 General

This Annex specifies the formal definition of the API(s) defined in the present specification. It consists of OpenAPI specifications in YAML format.

This Annex takes precedence when being discrepant to other parts of the specification with respect to the encoding of information elements and methods within the API(s).

NOTE 1: The semantics and procedures, as well as conditions, e.g. for the applicability and allowed combinations of attributes or values, not expressed in the OpenAPI definitions but defined in other parts of the specification also apply.

Informative copies of the OpenAPI specification files contained in this 3GPP Technical Specification are available on a Git-based repository that uses the GitLab software version control system (see clause 5.3.1 of 3GPP TS 29.501 [5] and clause 5B of 3GPP TR 21.900 [7]).

# A.2 Npcf\_MBSPolicyControl API

openapi: 3.0.0

info:

title: Npcf\_MBSPolicyControl API

version: 1.1.0-alpha.3

description: |

MBS Policy Control Service

© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 29.537 V18.3.0; 5G System; Multicast/Broadcast Policy Control Services.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.537/'

security:

- {}

- oAuth2ClientCredentials:

- npcf-mbspolicycontrol

servers:

- url: '{apiRoot}/npcf-mbspolicycontrol/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501.

paths:

/mbs-policies:

post:

summary: Request the creation of a new MBS Policy Association.

operationId: CreateMBSPolicy

tags:

- MBS Policies (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MbsPolicyCtxtData'

responses:

'201':

description: >

Created. An Individual MBS Policy resource is successfully created.

content:

application/json:

schema:

$ref: '#/components/schemas/MbsPolicyData'

headers:

Location:

description: >

Contains the URI of the newly created Individual MBS Policy resource.

required: true

schema:

type: string

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden.

content:

application/problem+json:

schema:

$ref: 'TS29537\_Npcf\_MBSPolicyAuthorization.yaml#/components/schemas/MbsExtProblemDetails'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/mbs-policies/{mbsPolicyId}:

parameters:

- name: mbsPolicyId

in: path

description: >

Contains the identifier of the concerned Individual MBS Policy resource.

required: true

schema:

type: string

get:

summary: Read an Individual MBS Policy resource.

operationId: GetIndMBSPolicy

tags:

- Individual MBS Policy (Document)

responses:

'200':

description: >

OK. The requested Individual MBS Policy resource is successfully returned.

content:

application/json:

schema:

$ref: '#/components/schemas/MbsPolicyData'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Deletes an existing Individual MBS Policy resource.

operationId: DeleteIndMBSPolicy

tags:

- Individual MBS Policy (Document)

parameters:

- name: mbsPolicyId

in: path

description: >

Contains the identifier of the concerned Individual MBS Policy resource.

required: true

schema:

type: string

responses:

'204':

description: >

No Content. The concerned Individual MBS Policy resource is successfully deleted.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/mbs-policies/{mbsPolicyId}/update:

post:

summary: Request the update of an existing MBS Policy Association.

operationId: UpdateIndMBSPolicy

tags:

- Individual MBS Policy (Document)

parameters:

- name: mbsPolicyId

in: path

description: >

Contains the identifier of the concerned Individual MBS Policy resource.

required: true

schema:

type: string

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MbsPolicyCtxtDataUpdate'

responses:

'200':

description: >

OK. The targeted Individual MBS Policy resource is successfully updated.

content:

application/json:

schema:

$ref: '#/components/schemas/MbsPolicyData'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden.

content:

application/problem+json:

schema:

$ref: 'TS29537\_Npcf\_MBSPolicyAuthorization.yaml#/components/schemas/MbsExtProblemDetails'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

npcf-mbspolicycontrol: Access to the Npcf\_MBSPolicyControl API

schemas:

MbsPolicyCtxtData:

description: >

Contains the parameters used to request the creation of an MBS Policy

Association.

type: object

properties:

mbsSessionId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsSessionId'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

areaSessPolId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AreaSessionPolicyId'

mbsServInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsServiceInfo'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- mbsSessionId

MbsPolicyDecision:

description: >

Represents the parameters constituting an MBS Policy Decision.

type: object

properties:

mbsPccRules:

type: object

additionalProperties:

$ref: '#/components/schemas/MbsPccRule'

minProperties: 1

description: >

A map of MBS PCC rule(s) with each map entry containing the MbsPccRule data structure.

The key of the map for each entry is the mbsPccRuleId attribute of the corresponding

MbsPccRule data structure.

nullable: true

mbsQosDecs:

type: object

additionalProperties:

$ref: '#/components/schemas/MbsQosDec'

minProperties: 1

description: >

A map of MBS QoS Decision(s) with each map entry containing the MbsQosDec data structure.

The key of the map for each entry is the mbsQosId attribute of the corresponding

MbsQosDec data structure.

mbsQosChars:

type: object

additionalProperties:

$ref: '#/components/schemas/MbsQosChar'

minProperties: 1

description: >

A map of MBS QoS Characteristics set(s) with each map entry containing the MbsQosChar data

structure. The key of the map for each entry is the 5QI attribute of the corresponding

MbsQosDec data structure.

authMbsSessAmbr:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

mbsPcrts:

type: array

items:

$ref: '#/components/schemas/MbsPcrt'

minItems: 1

nullable: true

MbsPolicyData:

description: >

Contains the MBS policy data provisioned as part of an MBS Policy Association.

type: object

properties:

mbsPolicyCtxtData:

$ref: '#/components/schemas/MbsPolicyCtxtData'

mbsPolicies:

$ref: '#/components/schemas/MbsPolicyDecision'

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- mbsPolicyCtxtData

MbsPccRule:

description: Represents the parameters constituting an MBS PCC rule.

type: object

properties:

mbsPccRuleId:

type: string

mbsDlIpFlowInfo:

type: array

items:

$ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/FlowDescription'

minItems: 1

precedence:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uinteger'

refMbsQosDec:

type: array

items:

type: string

minItems: 1

maxItems: 1

required:

- mbsPccRuleId

MbsQosDec:

description: Represents the parameters constituting an MBS QoS Decision.

type: object

properties:

mbsQosId:

type: string

5qi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5Qi'

priorityLevel:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5QiPriorityLevel'

mbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

gbrDl:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

arp:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Arp'

averWindow:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AverWindow'

mbsMaxDataBurstVol:

$ref: '#/components/schemas/MbsMaxDataBurstVol'

required:

- mbsQosId

MbsQosChar:

description: >

Represents the parameters constituting a set of explicitly signalled QoS characteristics.

type: object

properties:

5qi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5Qi'

priorityLevel:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/5QiPriorityLevel'

resourceType:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/QosResourceType'

packetDelayBudget:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketDelBudget'

packetErrorRate:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/PacketErrRate'

averWindow:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AverWindow'

mbsMaxDataBurstVol:

$ref: '#/components/schemas/MbsMaxDataBurstVol'

required:

- 5qi

- resourceType

- priorityLevel

- packetDelayBudget

- packetErrorRate

- mbsMaxDataBurstVol

MbsPolicyCtxtDataUpdate:

description: >

Contains the parameters to request the modification of an existing MBS Policy Association.

type: object

properties:

mbsServInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsServiceInfo'

mbsPcrts:

type: array

items:

$ref: '#/components/schemas/MbsPcrt'

minItems: 1

mbsErrorReport:

$ref: '#/components/schemas/MbsErrorReport'

MbsErrorReport:

description: >

Represents the reporting of MBS Policy decision level failure(s) and/or MBS PCC rule level

failure(s).

type: object

properties:

mbsReports:

type: array

items:

$ref: '#/components/schemas/MbsReport'

minItems: 1

MbsReport:

description: >

Contains information about the MBS Policy Decision level failure(s) and/or the MBS PCC

rule level failure(s).

type: object

properties:

mbsPccRuleIds:

type: array

items:

type: string

minItems: 1

mbsPccRuleStatus:

$ref: '#/components/schemas/MbsPccRuleStatus'

failureCode:

$ref: '#/components/schemas/MbsFailureCode'

# Simple data types:

MbsMaxDataBurstVol:

description: Represents the MBS Maximum Data Burst Volume expressed in Bytes.

type: integer

minimum: 1

maximum: 2000000

# ENUMS:

MbsPcrt:

anyOf:

- type: string

enum:

- MBS\_SESSION\_UPDATE

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Represents the MBS Policy Control Request Trigger.

Possible values are:

- MBS\_SESSION\_UPDATE: Indicates the MBS Session Update policy control request trigger.

MbsPccRuleStatus:

anyOf:

- type: string

enum:

- ACTIVE

- INACTIVE

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Represents the MBS PCC rule status.

Possible values are:

- ACTIVE: Indicates that the MBS PCC rule(s) are successfully installed.

- INACTIVE: Indicates that the MBS PCC rule(s) are removed.

MbsFailureCode:

anyOf:

- type: string

enum:

- NF\_MALFUNCTION

- NF\_RESOURCES\_UNAVAILABLE

- RESOURCE\_ALLOCATION\_FAILURE

- MBS\_QOS\_VALIDATION\_FAILURE

- NO\_MBS\_QOS\_FLOW

- MBS\_QOS\_DECISION\_ERROR

- MBS\_POLICY\_PARAM\_ERROR

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Represents the reason for the MBS Policy Decision(s) enforcement failure or

the MBS PCC rule(s) installation failure.

Possible values are:

- NF\_MALFUNCTION: Indicates that the MBS PCC rule could not be successfully installed due

to MB-SMF/MB-UPF malfunction.

- NF\_RESOURCES\_UNAVAILABLE: Indicates that the MBS PCC rule could not be successfully

installed due to resources unavailable at the MB-SMF/MB-UPF.

- RESOURCE\_ALLOCATION\_FAILURE: Indicates that the MBS PCC rule could not be successfully

installed or maintained since the associated MBS QoS flow establishment/modification

failed or the associated MBS QoS flow was released.

- MBS\_QOS\_VALIDATION\_FAILURE: Indicates that MBS QoS validation has failed.

- NO\_MBS\_QOS\_FLOW: Indicates that there is no MBS QoS flow to which the MB-SMF can bind

the MBS PCC rule(s).

- MBS\_QOS\_DECISION\_ERROR: Indicates failure in the provisioning of MBS QoS Decision data.

- MBS\_POLICY\_PARAM\_ERROR: Indicates that the information related to the provisioned MBS

policy parameter(s) is incorrect, incomplete or inconsistent.

# A.3 Npcf\_MBSPolicyAuthorization API

openapi: 3.0.0

info:

title: Npcf\_MBSPolicyAuthorization API

version: 1.1.0-alpha.2

description: |

MBS Policy Authorization Service.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: >

3GPP TS 29.537 V18.3.0; 5G System; Multicast/Broadcast Policy Control Services.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.537/'

security:

- {}

- oAuth2ClientCredentials:

- npcf-mbspolicyauth

servers:

- url: '{apiRoot}/npcf-mbspolicyauth/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501.

paths:

/contexts:

post:

summary: Request the creation of a new Individual MBS Application Session Context resource.

operationId: CreateMBSAppSessionCtxt

tags:

- MBS Application Session Contexts (Collection)

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/MbsAppSessionCtxt'

responses:

'201':

description: >

Created. An Individual MBS Application Session Context resource is successfully created

and a representation of the created resource is returned.

content:

application/json:

schema:

$ref: '#/components/schemas/MbsAppSessionCtxt'

headers:

Location:

description: >

Contains the URI of the newly created Individual MBS Application Session Context

resource.

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden.

content:

application/problem+json:

schema:

$ref: '#/components/schemas/MbsExtProblemDetails'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/contexts/{contextId}:

parameters:

- name: contextId

in: path

description: >

Contains the identifier of the Individual MBS Application Session Context resource.

required: true

schema:

type: string

get:

summary: Read an existing Individual MBS Application Session Context resource.

operationId: GetMBSAppSessionCtxt

tags:

- Individual MBS Application Session Context (Document)

responses:

'200':

description: >

OK. The requested Individual MBS Application Session Context resource is successfully

returned.

content:

application/json:

schema:

$ref: '#/components/schemas/MbsAppSessionCtxt'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

patch:

summary: Request the modification of an existing Individual MBS Application Session Context resource.

operationId: ModifyMBSAppSessionCtxt

tags:

- Individual MBS Application Session Context (Document)

requestBody:

required: true

content:

application/merge-patch+json:

schema:

$ref: '#/components/schemas/MbsAppSessionCtxtPatch'

responses:

'200':

description: >

OK. The requested Individual MBS Application Session Context resource is successfully

modified and a representation of the updated resource is returned in the response body.

content:

application/json:

schema:

$ref: '#/components/schemas/MbsAppSessionCtxt'

'204':

description: >

No Content. The corresponding Individual MBS Application Session Context resource is

successfully modified and no content is returned in the response body.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

description: Forbidden.

content:

application/problem+json:

schema:

$ref: '#/components/schemas/MbsExtProblemDetails'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

summary: Request the deletion of an existing Individual MBS Application Session Context resource.

operationId: DeleteMBSAppSessionCtxt

tags:

- Individual MBS Application Session Context (Document)

responses:

'204':

description: >

No Content. The corresponding Individual MBS Application Session Context resource is

successfully deleted.

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'406':

$ref: 'TS29571\_CommonData.yaml#/components/responses/406'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

npcf-mbspolicyauth: Access to the Npcf\_MBSPolicyAuthorization API

schemas:

MbsAppSessionCtxt:

description: >

Represents the parameter of an MBS Application Session Context.

type: object

properties:

mbsSessionId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsSessionId'

mbsServInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsServiceInfo'

dnn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

snssai:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

areaSessPolId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/AreaSessionPolicyId'

reqForLocDepMbs:

type: boolean

default: false

contactPcfInd:

type: boolean

default: false

suppFeat:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

required:

- mbsSessionId

MbsAppSessionCtxtPatch:

description: >

Represents the modifications to an existing MBS Application Session Context resource.

type: object

properties:

mbsServInfo:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsServiceInfo'

AcceptableMbsServInfo:

description: >

Contains the MBS Service Information that can be accepted by the PCF.

type: object

properties:

accMbsServInfo:

type: object

additionalProperties:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/MbsMediaComp'

minProperties: 1

accMaxMbsBw:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'

oneOf:

- required: [accMbsServInfo]

- required: [accMaxMbsBw]

# Data types describing alternative data types or combinations of data types:

MbsExtProblemDetails:

description: Identifies the MBS related extensions to the ProblemDetails data structure.

allOf:

- $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

- $ref: '#/components/schemas/AcceptableMbsServInfo'

Annex B (informative):  
Withdrawn API versions

# B.1 General

This Annex lists withdrawn API versions of the APIs defined in the present specification. Clause 4.3.1.6 of 3GPP TS 29.501 [5] describes the withdrawal of API versions.

# B.2 Npcf\_MBSPolicyControl API

The API versions listed in table B.2-1 are withdrawn for the Npcf\_MBSPolicyControl API.

Table B.2-1: Withdrawn API versions of the Npcf\_MBSPolicyControl service

|  |  |
| --- | --- |
| API version number | Remarks |
|  |  |

# B.3 Npcf\_MBSPolicyAuthorization API

The API versions listed in table B.3-1 are withdrawn for the Npcf\_MBSPolicyAuthorization API.

Table B.3-1: Withdrawn API versions of the Npcf\_MBSPolicyAuthorization service

|  |  |
| --- | --- |
| API version number | Remarks |
|  |  |

Annex C (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2022-01 | CT3#119bis-e | C3-220401 |  |  |  | TS Skeleton | 0.0.0 |
| 2022-01 | CT3#119bis-e | C3-220457 |  |  |  | Inclusion of C3-220113, C3-220114, C3-220115,  C3-220116, C3-220402, C3-220403, C3-220404 C3-220491, C3-220492, C3-220493 | 0.1.0 |
| 2022-04 | CT3#121-e | C3-222483 |  |  |  | Inclusion of C3-222056, C3-222124, C3-222127,  C3-222403, C3-222404, C3-222405, C3-222406 C3-222407, C3-222462 | 0.2.0 |
| 2022-05 | CT3#122-e | C3-223506 |  |  |  | Inclusion of C3-223561, C3-223574, C3-223562,  C3-223563, C3-223564, C3-223568, C3-223565 C3-223566, C3-223573, C3-223308 | 0.3.0 |
| 2022-06 | CT#96 | CP-221097 |  |  |  | Presentation to TSG CT for information | 1.0.0 |
| 2022-06 |  |  |  |  |  | Update of info and externalDocs fields in OpenAPI specs by MCC | 1.0.1 |
| 2022-09 | CT3#123-e |  |  |  |  | Inclusion of C3-224644, C3-224645, C3-224646, C3-224709, C3-224710, C3-224711 | 1.0.2 |
| 2022-09 | CT#97e | CP-222129 |  |  |  | Presentation to TSG CT for approval | 2.0.0 |
| 2022-09 | CT#97e | CP-222129 |  |  |  | Approved by TSG CT | 17.0.0 |
| 2022-12 | CT#98e | CP-223167 | 0001 | 1 | F | Attribute corrections in the description and data model clause in Npcf\_MBSPolicyControl Service | 17.1.0 |
| 2022-12 | CT#98e | CP-223166 | 0005 | - | F | Wrong data type for MBS QoS information | 17.1.0 |
| 2022-12 | CT#98e | CP-223167 | 0006 | 1 | F | Add 404 NOT FOUND for the Npcf\_MBSPolicyauthorization update and delete service | 17.1.0 |
| 2022-12 | CT#98e | CP-223166 | 0007 | - | F | Correction to architecture figure | 17.1.0 |
| 2022-12 | CT#98e | CP-223167 | 0008 | 1 | F | Correction to content type of Npcf\_MBSPolicyAuthorization API | 17.1.0 |
| 2022-12 | CT#98e | CP-223166 | 0009 | - | F | Correction to Individual MBS Policy | 17.1.0 |
| 2022-12 | CT#98e | CP-223166 | 0010 | - | F | Correction to MbsAppSessionCtxt | 17.1.0 |
| 2022-12 | CT#98e | CP-223167 | 0011 | 1 | F | Correction to Npcf\_MBSPoliyControl\_Create operation | 17.1.0 |
| 2022-12 | CT#98e | CP-223167 | 0012 | 1 | F | Correction to reponse of create operation | 17.1.0 |
| 2022-12 | CT#98e | CP-223166 | 0013 | - | F | Correction to the indication that the PCF has to be contacted | 17.1.0 |
| 2022-12 | CT#98e | CP-223167 | 0014 | 1 | F | Corrections for Npcf\_MBSPolicyControl service | 17.1.0 |
| 2022-12 | CT#98e | CP-223188 | 0015 | - | F | Update of info and externalDocs fields | 17.1.0 |
| 2022-12 | CT#98e | CP-223192 | 0003 | - | F | Adding the mandatory error code 502 Bad Gateway | 18.0.0 |
| 2022-12 | CT#98e | CP-223192 | 0004 | 1 | F | Npcf\_MBSPolicyControl API: enumeration definitions in the OpenAPI file | 18.0.0 |
| 2022-12 | CT#98e | CP-223189 | 0016 | - | F | Update of info and externalDocs fields | 18.0.0 |
| 2023-03 | CT#99 | CP-230166 | 0017 | - | F | Correction of the description fields in enumerations | 18.1.0 |
| 2023-03 | CT#99 | CP-230131 | 0019 | 1 | A | Miscellaneous essential corrections to the MBS PCF APIs | 18.1.0 |
| 2023-03 | CT#99 | CP-230161 | 0021 | - | F | Update of info and externalDocs fields | 18.1.0 |
| 2023-06 | CT#100 | CP-231131 | 0020 | 3 | F | Corrections to the redirection mechanism description | 18.2.0 |
| 2023-12 | CT#102 | CP-233228 | 0022 |  | F | Updating the obsoleted IETF HTTP RFCs | 18.3.0 |
| 2023-12 | CT#102 | CP-233229 | 0023 | 1 | F | Updating the obsoleted ProblemDetails IETF HTTP RFC | 18.3.0 |
| 2023-12 | CT#102 | CP-233247 | 0026 | 1 | F | Clarification regarding the MBS service flow template | 18.3.0 |
| 2023-12 | CT#102 | CP-233123 | 0028 | 2 | A | Correction to Npcf\_MBSPolicyControl API for location dependent MBS service | 18.3.0 |
| 2023-12 | CT#102 | CP-233238 | 0030 |  | F | Update of info and externalDocs fields | 18.3.0 |