|  |  |
| --- | --- |
| 3GPP TS 29.577 V18.2.0 (2023-12) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Core Network and Terminals;  5G System; IP Short Message Gateway and SMS Router  For Short Message Services;  Stage 3  (Release 18) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 6

1 Scope 8

2 References 8

3 Definitions and abbreviations 9

3.1 Definitions 9

3.2 Abbreviations 9

4 Overview 9

4.1 Introduction 9

5 Services offered by the IP-SM-GW and SMS Router 10

5.1 Introduction 10

5.2 Nipsmgw\_SMService Service 10

5.2.1 Service Description 10

5.2.2 Service Operations 11

5.2.2.1 Introduction 11

5.2.2.2 RoutingInfo 11

5.2.2.2.1 General 11

5.2.2.3 MtForwardSm 12

5.2.2.3.1 General 12

5.3 Nrouter\_SMService Service 12

5.3.1 Service Description 12

5.3.2 Service Operations 13

5.3.2.1 Introduction 13

5.3.2.2 RoutingInfo 13

5.3.2.2.1 General 13

5.3.2.3 MtForwardSm 14

5.3.2.3.1 General 14

6 API Definitions 14

6.1 Nipsmgw\_SMService Service API 14

6.1.1 Introduction 14

6.1.2 Usage of HTTP 15

6.1.2.1 General 15

6.1.2.2 HTTP standard headers 15

6.1.2.2.1 General 15

6.1.2.2.2 Content type 15

6.1.2.3 HTTP custom headers 16

6.1.2.4 HTTP multipart messages 16

6.1.3 Resources 16

6.1.3.1 Overview 16

6.1.3.2 Resource: MtSmInfos (Collection) 17

6.1.3.2.1 Description 17

6.1.3.2.2 Resource Definition 17

6.1.3.2.3 Resource Standard Methods 17

6.1.3.3 Resource: MtSmInfo (Document) 17

6.1.3.3.1 Description 17

6.1.3.3.2 Resource Definition 17

6.1.3.3.3 Resource Standard Methods 18

6.1.3.3.4 Resource Custom Operations 19

6.1.4 Custom Operations without associated resources 21

6.1.5 Notifications 21

6.1.6 Data Model 21

6.1.6.1 General 21

6.1.6.2 Structured data types 22

6.1.6.2.1 Introduction 22

6.1.6.2.2 Type: CreateRoutingData 22

6.1.6.2.3 Type: CreatedRoutingData 23

6.1.6.2.4 Type: SmsData 23

6.1.6.2.5 Type: SmsDeliveryData 23

6.1.6.3 Simple data types and enumerations 23

6.1.6.3.1 Introduction 23

6.1.6.3.2 Simple data types 23

6.1.6.4 Data types describing alternative data types or combinations of data types 24

6.1.6.5 Binary data 24

6.1.6.5.1 Binary Data Types 24

6.1.6.5.2 SMS Payload Information 24

6.1.7 Error Handling 24

6.1.7.1 General 24

6.1.7.2 Protocol Errors 24

6.1.7.3 Application Errors 24

6.1.8 Feature negotiation 25

6.1.9 Security 25

6.1.10 HTTP redirection 25

6.2 Nrouter\_SMService Service API 25

6.2.1 Introduction 25

6.2.2 Usage of HTTP 26

6.2.2.1 General 26

6.2.2.2 HTTP standard headers 26

6.2.2.2.1 General 26

6.2.2.2.2 Content type 26

6.2.2.3 HTTP custom headers 27

6.2.2.4 HTTP multipart messages 27

6.2.3 Resources 27

6.2.3.1 Overview 27

6.2.3.2 Resource: MtSmInfos (Store) 28

6.2.3.2.1 Description 28

6.2.3.2.2 Resource Definition 28

6.2.3.2.3 Resource Standard Methods 28

6.2.3.3 Resource: MtSmInfo (Document) 28

6.2.3.3.1 Description 28

6.2.3.3.2 Resource Definition 28

6.2.3.3.3 Resource Standard Methods 29

6.2.3.3.4 Resource Custom Operations 30

6.2.4 Custom Operations without associated resources 32

6.2.5 Notifications 32

6.2.6 Data Model 32

6.2.6.1 General 32

6.2.6.2 Structured data types 33

6.2.6.2.1 Introduction 33

6.2.6.2.2 Type: CreatedRoutingData 33

6.2.6.3 Simple data types and enumerations 34

6.2.6.3.1 Introduction 34

6.2.6.3.2 Simple data types 34

6.2.6.3.3 Enumeration: <EnumType1> 34

6.2.6.4 Data types describing alternative data types or combinations of data types 34

6.2.6.5 Binary data 34

6.2.7 Error Handling 34

6.2.7.1 General 34

6.2.7.2 Protocol Errors 34

6.2.7.3 Application Errors 34

6.2.8 Feature negotiation 35

6.2.9 Security 35

6.2.10 HTTP redirection 35

Annex A (normative): OpenAPI specification 36

A.1 General 36

A.2 Nipsmgw\_SMService API 36

A.3 Nrouter\_SMService API 39

Annex B (Informative): HTTP Multipart Messages 42

B.1 Example of HTTP multipart message 42

B.2 Example HTTP multipart message with SMS binary data 43

Annex C (informative): Change history 44

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" are not substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The present document specifies the stage 3 protocol and data model for the Nipsmgw and Nrouter Service Based Interface. It provides stage 3 protocol definitions and message flows, and specifies the API for each service offered by the IP-SM-GW and SMS Router.

The 5G System stage 2 architecture and procedures are specified in 3GPP TS 23.501 [2] and 3GPP TS 23.502 [3].

The Technical Realization of the Service Based Architecture and the Principles and Guidelines for Services Definition are specified in TS 29.500 [4] and TS 29.501 [5].

The Stage 2 architecture, procedures and services to support service based short message service (SMS) in 5G system (5GS) is specified in 3GPP TS 23.540 [14].

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[3] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[4] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[5] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[6] OpenAPI: "OpenAPI Specification Version 3.0.0", <https://spec.openapis.org/oas/v3.0.0>.

[7] 3GPP TR 21.900: "Technical Specification Group working methods".

[8] 3GPP TS 33.501: "Security architecture and procedures for 5G system".

[9] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[10] 3GPP TS 29.510: "5G System; Network Function Repository Services; Stage 3".

[11] IETF RFC 9113: "HTTP/2".

[12] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format".

[13] IETF RFC 9457: "Problem Details for HTTP APIs".

[14] 3GPP TS 23.540: "5G System; Technical realization of Service Based Short Message Service; Stage 2".

[15] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[16] 3GPP TS 23.040: "Technical realization of the Short Message Service (SMS)".

[17] 3GPP TS 24.011: "Point-to-Point (PP) Short Message Service (SMS) support on mobile radio interface".

[18] IETF RFC 2387: "The MIME Multipart/Related Content-type".

[19] IETF RFC 2045: "Multipurpose Internet Mail Extensions (MIME) Part One: Format of Internet Message Bodies".

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**Gateway MSC For Short Message Service (SMS‑GMSC):** function of an MSC capable of receiving a short message from an SC, interrogating an HLR/HSS/UDM for routing information and SMS info, and delivering the short message to the VMSC/SGSN/MME/SMSF of the recipient MS/UE.

**IP-Short-Message-Gateway (IP-SM-GW):** function responsible for protocol interworking between the IP-based UE and the SC.

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

IP-SM-GW IP Short Message Gateway

SM MO Short Message Mobile Originated

SM MT Short Message Mobile Terminated

SMSF Short Message Service Function

# 4 Overview

## 4.1 Introduction

Within the 5GC, the IP-SM-GW offers services to the UDM or SMS-GMSC via the Nipsmgw service based interface, the SMS Router offers services to the UDM or SMS-GMSC via the Nrouter service based interface (see 3GPP TS 23.540 [14], 3GPP TS 23.501 [2] and 3GPP TS 23.502 [3]).

Figure 4.1-1 and Figure 4.1-2 provide the reference model (in service based interface representation and in reference point representation), with focus on the IP-SM-GW and SMS Router and the scope of the present specification.



Figure 4.1-1: Reference model – IP-SM-GW



Figure 4.1-2: Reference model – SMS Router

The functionalities supported by the IP-SM-GW and SMS Router are listed in 3GPP TS 23.540 [14].

# 5 Services offered by the IP-SM-GW and SMS Router

## 5.1 Introduction

The IP-SM-GW offers to other NFs the following service:

- Nipsmgw\_SMService

The SMS Router offers to other NFs the following service:

- Nrouter\_SMService

The Nipsmgw\_SMService service and Nrouter\_SMService service are specified in 3GPP TS 23.540 [14].

Table 5.1-1 summarizes the corresponding APIs defined for this specification.

Table 5.1-1: API Descriptions

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Service Name | Clause | Description | OpenAPI Specification File | apiName | Annex |
| Nipsmgw\_SMService | 6.1 | IP-SM-GW SMService Service | TS29577\_Nipsmgw\_SMService.yaml | nipsmgw-smservice | A.2 |
| Nrouter\_SMService | 6.2 | SMS Router SMService Service | TS29577\_Nrouter\_SMService.yaml | nrouter-smservice | A.3 |

## 5.2 Nipsmgw\_SMService Service

### 5.2.1 Service Description

The Nipsmgw\_SMService service provides SBI-based MT SM transmit through IP-SM-GW. The IP-SM-GW is acting as NF Service Producer, while the UDM or SMS-GMSC is the NF Service Consumer.

Following functionalities are provided by the Nipsmgw\_SMService service:

- Provide Routing Information;

- Transmit downlink SMS message.

The Nipsmgw\_SMService service supports the following service operations.

Table 5.2.1-1: Service operations supported by the Nipsmgw\_SMService service

|  |  |  |  |
| --- | --- | --- | --- |
| Service Operations | Description | Operation  Semantics | Example Consumer(s) |
| RoutingInfo | Provide Routing Information. | Request/Response | UDM |
| MtForwardSm | Transmit downlink SMS message. | Request/Response | SMS-GMSC |

### 5.2.2 Service Operations

#### 5.2.2.1 Introduction

See Table 5.2.1-1 for an overview of the service operations supported by the Nipsmgw\_SMService service.

#### 5.2.2.2 RoutingInfo

##### 5.2.2.2.1 General

The RoutingInfo service operation shall be used to provide the SMSF Instance Id to the IP-SM-GW.

It is used in the following procedures:

- Successful Mobile Terminated short message transfer via IP-SM-GW (see clause 5.1.4 of 3GPP TS 23.540 [14]).

- Unsuccessful Mobile Terminated short message transfer via IP-SM-GW (see clause 5.1.6 of 3GPP TS 23.540 [14]).

The NF Service Consumer (e.g. UDM) shall provide the SMSF Instance Id to the IP-SM-GW by using the HTTP PUT method as shown in Figure 5.2.2.2.1-1.



Figure 5.2.2.2.1-1: Routing Information creation

1. The NF Service Consumer shall send a PUT request to the resource representing the UE's Mobile Terminated Short Message Information resource (i.e. …/mt-sms/{gpsi}) of the IP-SM-GW to update or create the routing information for a given UE. The content of the PUT request shall contain:

- SMSF Instance Id.

2a. If the resource does not exist (there is no previous routing information stored in IP-SM-GW for that user), IP-SM-GW stores the received routing data and returns a "201 Created" response with the "Location" header containing the URI of the created resource.

The PUT response body shall include:

- the IP address of the IP-SM-GW (to be sent by the UDM to the SMS-GMSC); and/or

- the FQDN of the IP-SM-GW (to be sent by the UDM to the SMS-GMSC).

2b. If the resource exists (there is previous routing information stored in IP-SM-GW for that user), the IP-SM-GW updates the routing data by replacing it with the received information, and responds with "200 OK" or "204 No Content".

2c. On failure, or redirection, one of the HTTP status code listed in Table 6.1.3.3.3.1-3 shall be returned.

#### 5.2.2.3 MtForwardSm

##### 5.2.2.3.1 General

The MtForwardSm service operation shall be used to transmit downlink SMS message via IP-SM-GW.

It is used in the following procedures:

- Successful Mobile Terminated short message transfer via IP-SM-GW (see clause 5.1.4 of 3GPP TS 23.540 [14]).

- Unsuccessful Mobile Terminated short message transfer via IP-SM-GW (see clause 5.1.6 of 3GPP TS 23.540 [14]).

The NF Service Consumer (e.g. SMS-GMSC) shall transmit downlink SMS message to the IP-SM-GW by using the HTTP POST method as shown in Figure 5.2.2.3.1-1.



Figure 5.2.2.3.1-1: Transmit downlink SMS message

1. The NF Service Consumer shall send a POST request to the resource representing the UE's Mobile Terminated Short Message Information resource (i.e. …/mt-sms/{gpsi}/sendsms) of the IP-SM-GW. The content of the POST request shall contain the SMS message to be sent.

2a. On success, "200 OK" shall be returned with "SmsDeliveryData" object contains the MT SMS Delivery Report in the response body.

2b. On failure, or redirection, one of the HTTP status code listed in Table 6.1.3.3.4.2.2-2 shall be returned.

## 5.3 Nrouter\_SMService Service

### 5.3.1 Service Description

The Nrouter\_SMService service provides SBI-based MT SM transmit through SMS Router. The SMS Router is acting as NF Service Producer, while the UDM or SMS-GMSC is the NF Service Consumer.

Following functionalities are provided by the Nrouter\_SMService service:

- Provide Routing Information;

- Transmit downlink SMS message.

The Nrouter\_SMService service supports the following service operations.

Table 5.3.1-1: Service operations supported by the Nrouter\_SMService service

|  |  |  |  |
| --- | --- | --- | --- |
| Service Operations | Description | Operation  Semantics | Example Consumer(s) |
| RoutingInfo | Provide Routing Information. | Request/Response | UDM |
| MtForwardSm | Transmit downlink SMS message. | Request/Response | SMS-GMSC |

### 5.3.2 Service Operations

#### 5.3.2.1 Introduction

See Table 5.3.1-1 for an overview of the service operations supported by the Nrouter\_SMService service.

#### 5.3.2.2 RoutingInfo

##### 5.3.2.2.1 General

The RoutingInfo service operation shall be used to provide the SMSF Instance Id to the SMS Router.

It is used in the following procedures:

- Successful Mobile Terminated short message transfer via SMS Router (see clause 5.1.3 of 3GPP TS 23.540 [14]).

- Unsuccessful Mobile Terminated short message transfer via SMS Router (see clause 5.1.9 of 3GPP TS 23.540 [14]).

The NF Service Consumer (e.g. UDM) shall provide the SMSF Instance Id to the SMS Router by using the HTTP PUT method as shown in Figure 5.3.2.2.1-1.



Figure 5.3.2.2.1-1: Routing Information creation

1. The NF Service Consumer shall send a PUT request to the resource representing the UE's Mobile Terminated Short Message Information resource (i.e. …/mt-sms/{gpsi}) of the SMS Router to update or create the routing information for a given UE. The content of the PUT request shall contain:

- SMSF Instance Id.

2a. If the resource does not exist (there is no previous routing information stored in SMS Router for that user), SMS Router stores the received routing data and returns a "201 Created" response with the "Location" header containing the URI of the created resource.

The PUT response body shall include:

- the IP address of the SMS Router (to be sent by the UDM to the SMS-GMSC); and/or

- the FQDN of the SMS Router (to be sent by the UDM to the SMS-GMSC).

2b. If the resource exists (there is previous routing information stored in SMS Router for that user), the SMS Router updates the routing data by replacing it with the received information, and responds with "200 OK" or "204 No Content".

2c. On failure, or redirection, one of the HTTP status code listed in Table 6.2.3.3.3.1-3 shall be returned.

#### 5.3.2.3 MtForwardSm

##### 5.3.2.3.1 General

The MtForwardSm service operation shall be used to transmit downlink SMS message via SMS Router.

It is used in the following procedures:

- Successful Mobile Terminated short message transfer via SMS Router (see clause 5.1.3 of 3GPP TS 23.540 [14]).

- Unsuccessful Mobile Terminated short message transfer via SMS Router (see clause 5.1.9 of 3GPP TS 23.540 [14]).

The NF Service Consumer (e.g. SMS-GMSC) shall transmit downlink SMS message to the SMS Router by using the HTTP POST method as shown in Figure 5.3.2.3.1-1.



Figure 5.3.2.3.1-1: Transmit downlink SMS message

1. The NF Service Consumer shall send a POST request to the resource representing the UE's Mobile Terminated Short Message Information resource (i.e. …/mt-sms/{gpsi}/sendsms) of the SMS Router. The content of the POST request shall contain the SMS message to be sent.

2a. On success, "200 OK" shall be returned with "SmsDeliveryData" object contains the MT SMS Delivery Report in the response body.

2b. On failure, or redirection, one of the HTTP status code listed in Table 6.2.3.3.4.2.2-2 shall be returned.

# 6 API Definitions

## 6.1 Nipsmgw\_SMService Service API

### 6.1.1 Introduction

The Nipsmgw\_SMService shall use the Nipsmgw\_SMService API.

The API URI of the Nipsmgw\_SMService API shall be:

**{apiRoot}/<apiName>/<apiVersion>**

The request URIs used in HTTP requests from the NF service consumer towards the NF service producer shall have the Resource URI structure defined in clause 4.4.1 of 3GPP TS 29.501 [5], i.e.:

**{apiRoot}/<apiName>/<apiVersion>/<apiSpecificResourceUriPart>**

with the following components:

- The {apiRoot} shall be set as described in 3GPP TS 29.501 [5].

- The <apiName>shall be "nipsmgw-smservice".

- The <apiVersion> shall be "v1".

- The <apiSpecificResourceUriPart> shall be set as described in clause 6.1.3.

### 6.1.2 Usage of HTTP

#### 6.1.2.1 General

HTTP/2, IETF RFC 9113 [11], shall be used as specified in clause 5 of 3GPP TS 29.500 [4].

HTTP/2 shall be transported as specified in clause 5.3 of 3GPP TS 29.500 [4].

The OpenAPI [6] specification of HTTP messages and content bodies for the Nipsmgw\_SMService API is contained in Annex A.

#### 6.1.2.2 HTTP standard headers

##### 6.1.2.2.1 General

See clause 5.2.2 of 3GPP TS 29.500 [4] for the usage of HTTP standard headers.

##### 6.1.2.2.2 Content type

JSON, IETF RFC 8259 [12], shall be used as content type of the HTTP bodies specified in the present specification as specified in clause 5.4 of 3GPP TS 29.500 [4]. The use of the JSON format shall be signalled by the content type "application/json".

"Problem Details" JSON object shall be used to indicate additional details of the error in a HTTP response body and shall be signalled by the content type "application/problem+json", as defined in IETF RFC 9457 [13].

Multipart messages shall also be supported (see clause 6.1.2.4) using the content type "multipart/related", comprising:

- one JSON body part with the "application/json" content type; and

- one binary body part with 3gpp vendor specific content subtypes.

The 3gpp vendor specific content subtypes defined in Table 6.1.2.2.2-1 shall be supported.

Table 6.1.2.2.2-1: 3GPP vendor specific content subtypes

|  |  |
| --- | --- |
| content subtype | Description |
| vnd.3gpp.sms | Binary encoded payload, encoding SMS payload, as specified in 3GPP TS 23.040 [16] and 3GPP TS 24.011 [17]. |
| NOTE: Using 3GPP vendor content subtypes allows to describe the nature of the opaque payload (e.g. SMS payload) without having to rely on metadata in the JSON payload. | |

See clause 6.1.2.4 for the binary payloads supported in the binary body part of multipart messages.

#### 6.1.2.3 HTTP custom headers

The mandatory HTTP custom header fields specified in clause 5.2.3.2 of 3GPP TS 29.500 [4] shall be supported, and the optional HTTP custom header fields specified in clause 5.2.3.3 of 3GPP TS 29.500 [4] may be supported.

#### 6.1.2.4 HTTP multipart messages

HTTP multipart messages shall be supported, to transfer opaque SMS payload (e.g. SMS message, CP Ack, etc.), in the following service operations (and HTTP messages):

- MtForwardSm service operation;

HTTP multipart messages shall include one JSON body part and one binary body part comprising content of SMS payload content (see clause 6.1.6.5).

The JSON body part shall be the "root" body part of the multipart message. It shall be encoded as the first body part of the multipart message. The "Start" parameter does not need to be included.

The multipart message shall include a "type" parameter (see IETF RFC 2387 [18]) specifying the media type of the root body part, i.e. "application/json".

NOTE: The "root" body part (or "root" object) is the first body part the application processes when receiving a multipart/related message, see IETF RFC 2387 [18]. The default root is the first body within the multipart/related message. The "Start" parameter indicates the root body part, e.g. when this is not the first body part in the message.

A binary body part shall include a Content-ID header (see IETF RFC 2045 [19]), and the JSON body part shall make a reference to the binary body part using the Content-ID header field.

Examples of multipart/related messages can be found in Annex B.

### 6.1.3 Resources

#### 6.1.3.1 Overview

This clause describes the structure for the Resource URIs and the resources and methods used for the service.

Figure 6.1.3.1-1 depicts the resource URIs structure for the Nipsmgw\_SMService API.



Figure 6.1.3.1-1: Resource URI structure of the Nipsmgw\_SMService API

Table 6.1.3.1-1 provides an overview of the resources and applicable HTTP methods.

Table 6.1.3.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource purpose/name | Resource URI (relative path after API URI) | HTTP method or custom operation | Description (service operation) |
| MtSmInfos  (Collection) | /mt-sm-infos |  |  |
| MtSmInfo  (Document) | /mt-sm-infos/{gpsi} | PUT | Create Routing Information for MT SMS. |
| /mt-sm-infos/{gpsi}/sendsms | sendsms  (POST) | It is used for the MtForwardSm service operation, to allow NF Service Consumer to send SMS payload in downlink direction. |

#### 6.1.3.2 Resource: MtSmInfos (Collection)

##### 6.1.3.2.1 Description

This resource represents the collection of Mobile Terminated Short Message Information in IP-SM-GW.

This resource is modelled with the Collection resource archetype (see clause C.2 of 3GPP TS 29.501 [5]).

No HTTP method has been defined for this resource.

##### 6.1.3.2.2 Resource Definition

Resource URI: **{apiRoot}/nipsmgw-smsevice/<apiVersion>/mt-sm-infos**

This resource shall support the resource URI variables defined in table 6.1.3.2.2-1.

Table 6.1.3.2.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 6.1.1 |

##### 6.1.3.2.3 Resource Standard Methods

No HTTP method has been defined for the Mobile Terminated Short Message Information collection resource.

#### 6.1.3.3 Resource: MtSmInfo (Document)

##### 6.1.3.3.1 Description

This resource represents an individual Mobile Terminated Short Message Information in IP-SM-GW.

This resource is modelled with the Document resource archetype (see clause C.1 of 3GPP TS 29.501 [5]).

##### 6.1.3.3.2 Resource Definition

Resource URI: **{apiRoot}/nipsmgw-smsevice/<apiVersion>/mt-sm-infos/{gpsi}**

This resource shall support the resource URI variables defined in table 6.1.3.3.2-1.

Table 6.1.3.3.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 6.1.1 |
| gpsi | gpsi | Represents the Generic Public Subscription Identifier with MSISDN (see 3GPP TS 23.501 [2] clause 5.9.8)  pattern: See pattern of type Gpsi in 3GPP TS 29.571 [15] |

##### 6.1.3.3.3 Resource Standard Methods

6.1.3.3.3.1 PUT

This method creates an individual resource of Mobile Terminated Short Message Information in the IP-SM-GW, or updates the indicated resource of Mobile Terminated Short Message Information in the IP-SM-GW.

This method shall support the URI query parameters specified in table 6.1.3.3.3.1-1.

Table 6.1.3.3.3.1-1: URI query parameters supported by the PUT method on this resource

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description | Applicability |
| n/a |  |  |  |  |  |

This method shall support the request data structures specified in table 6.1.3.3.3.1-2 and the response data structures and response codes specified in table 6.1.3.3.3.1-3.

Table 6.1.3.3.3.1-2: Data structures supported by the PUT Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| CreateRoutingData | M | 1 | Representation of the UE's Mobile Terminated Short Message Information to be created in the IP-SM-GW, or to be updated in the IP-SM-GW. |

Table 6.1.3.3.3.1-3: Data structures supported by the PUT Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| CreatedRoutingData | M | 1 | 201 Created | This case represents the successful creation of an UE's Mobile Terminated Short Message Information.  The HTTP response shall include a "Location" HTTP header that contains the resource URI of the created resource. |
| CreatedRoutingData | M | 1 | 200 OK | Upon success, a response body containing a representation of the updated UE's Mobile Terminated Short Message Information shall be returned. |
| n/a |  |  | 204 No Content | Upon success, an empty response body shall be returned |
| RedirectResponse | O | 0..1 | 307 Temporary Redirect | Temporary redirection.  (NOTE 2) |
| RedirectResponse | O | 0..1 | 308 Permanent Redirect | Permanent redirection.  (NOTE 2) |
| NOTE 1: The manadatory HTTP error status code for the PUT method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] also apply.  NOTE 2: RedirectResponse may be inserted by an SCP, see clause 6.10.9.1 of 3GPP TS 29.500 [4]. | | | | |

Table 6.1.3.3.3.1-4: Headers supported by the 201 response code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains the URI of the newly created resource, according to the structure: {apiRoot}/nipsmgw-smsevice/<apiVersion>/mt-sm-infos/{gpsi} |

Table 6.1.3.3.3.1-5: Headers supported by the 307 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | An alternative URI of the resource located on an alternative service instance within the same IP-SM-GW or IP-SM-GW (service) set.  For the case, when a request is redirected to the same target resource via a different SCP, see clause 6.10.9.1 in 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target NF (service) instance ID towards which the request is redirected |

Table 6.1.3.3.3.1-6: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | An alternative URI of the resource located on an alternative service instance within the same IP-SM-GW or IP-SM-GW (service) set.  For the case, when a request is redirected to the same target resource via a different SCP, see clause 6.10.9.1 in 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target NF (service) instance ID towards which the request is redirected |

##### 6.1.3.3.4 Resource Custom Operations

6.1.3.3.4.1 Overview

Table 6.1.3.3.4.1-1: Custom operations

|  |  |  |  |
| --- | --- | --- | --- |
| Operation name | Custom operaration URI | Mapped HTTP method | Description |
| sendsms | /mt-sm-infos/{gpsii}/sendsms | POST | Send MT SMS message or the related Delivery Report. |

6.1.3.3.4.2 Operation: sendsms

6.1.3.3.4.2.1 Description

This custom operation is used for NF Service Consumers to send SMS message in downlink direction.

6.1.3.3.4.2.2 Operation Definition

This custom operation is used to send a SMS payload to an UE's Mobile Terminated Short Message Information resource in the IP-SM-GW.

This operation shall support the request data structures specified in table 6.1.3.3.4.2.2-1 and the response data structure and response codes specified in table 6.1.3.3.4.2.2-2.

Table 6.1.3.3.4.2.2-1: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| SmsData | M | 1 | Representation of the MT SMS message to be sent. |

Table 6.1.3.3.4.2.2-2: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| SmsDeliveryData | M | 1 | 200 OK | This case represents the successful of sending SMS message in downlink direction, with necessary response data on the received delivery report. |
| RedirectResponse | O | 0..1 | 307 Temporary Redirect | Temporary redirection.  (NOTE 2) |
| RedirectResponse | O | 0..1 | 308 Permanent Redirect | Permanent redirection.  (NOTE 2) |
| ProblemDetails | O | 0..1 | 400 Bad Request | This case represents an unsuccessful delivery of SMS message.  The "cause" attribute may be used to indicate one of the following application errors:  - SMS\_PAYLOAD\_MISSING, if the expected SMS payload content is missing;  - SMS\_PAYLOAD\_ERROR, if error exists in the SMS payload content. |
| ProblemDetails | O | 0..1 | 404 Not Found | This case represents an unsuccessful delivery of SMS payload.  The "cause" attribute may be used to indicate one of the following application errors:  - ROUTING\_INFO\_NOT\_FOUND, if the routing information for SMS to be operated is invalid or not found in IP-SM-GW.  - USER\_NOT\_FOUND, if the UE identified by the GPSI is not found in the IP-SM-GW. |
| NOTE 1: The manadatory HTTP error status code for the POST method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] also apply.  NOTE 2: RedirectResponse may be inserted by an SCP, see clause 6.10.9.1 of 3GPP TS 29.500 [4]. | | | | |

Table 6.1.3.3.4.2.2-3: Headers supported by the 307 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | An alternative URI of the resource located on an alternative service instance within the same IP-SM-GW or IP-SM-GW (service) set.  For the case, when a request is redirected to the same target resource via a different SCP, see clause 6.10.9.1 in 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target NF (service) instance ID towards which the request is redirected |

Table 6.1.3.3.4.2.2-4: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | An alternative URI of the resource located on an alternative service instance within the same IP-SM-GW or IP-SM-GW (service) set.  For the case, when a request is redirected to the same target resource via a different SCP, see clause 6.10.9.1 in 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target NF (service) instance ID towards which the request is redirected |

### 6.1.4 Custom Operations without associated resources

In this release of this specification, no custom operations without associated resources are defined.

### 6.1.5 Notifications

In this release of this specification, no notification procedures are defined.

### 6.1.6 Data Model

#### 6.1.6.1 General

This clause specifies the application data model supported by the API.

Table 6.1.6.1-1 specifies the data types defined for the Nipsmgw\_SMService service based interface protocol.

Table 6.1.6.1-1: Nipsmgw\_SMService specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Clause defined | Description | Applicability |
| CreateRoutingData | 6.1.6.2.2 | Information used for creating or updating the routing information of the user. |  |
| CreatedRoutingData | 6.1.6.2.3 | Information used for receiving the MT SMS. |  |
| SmsData | 6.1.6.2.4 | Information within request message for delivering SMS. |  |
| SmsDeliveryData | 6.1.6.2.5 | Information within response message invoking MtForwardSm service operation, for delivering MT SMS Delivery Report. |  |

Table 6.1.6.1-2 specifies data types re-used by the Nipsmgw\_SMService service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nipsmgw\_SMService service based interface.

Table 6.1.6.1-2: Nipsmgw\_SMService re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| ProblemDetails | 3GPP TS 29.571 [15] | Common Data Type used in response bodies |  |
| RedirectResponse | 3GPP TS 29.571 [15] | Redirect Response |  |
| Gpsi | 3GPP TS 29.571 [15] | General Public Subscription Identifier |  |
| NfInstanceId | 3GPP TS 29.571 [15] | NF Instance ID |  |
| RefToBinaryData | 3GPP TS 29.571 [15] | Information for indicating the binary content of SMS payload. |  |
| Ipv4Addr | 3GPP TS 29.571 [15] | IPv4 address |  |
| Ipv6Addr | 3GPP TS 29.571 [15] | IPv6 address |  |
| SupportedFeatures | 3GPP TS 29.571 [15] | Supported Features |  |
| Fqdn | 3GPP TS 29.571 [15] | Fully Qualified Domain Name |  |
| Supi | 3GPP TS 29.571 [15] | Subscription Permanent Identifier |  |

#### 6.1.6.2 Structured data types

##### 6.1.6.2.1 Introduction

This clause defines the structures to be used in resource representations.

##### 6.1.6.2.2 Type: CreateRoutingData

Table 6.1.6.2.2-1: Definition of type CreateRoutingData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| smsfId | NfInstanceId | M | 1 | This IE shall be present, and it shall contain the NF instance ID of the SMSF to receive the downlink MT SM. |  |
| supi | Supi | O | 0..1 | SUPI |  |
| supportedFeatures | SupportedFeatures | C | 0..1 | This IE shall be present if at least one optional feature defined in clause 6.1.8 is supported. |  |

##### 6.1.6.2.3 Type: CreatedRoutingData

Table 6.1.6.2.3-1: Definition of type CreatedRoutingData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| ipsmgwIpv4 | Ipv4Addr | C | 0..1 | This IE shall be present if available.  When present, this IE indicates the IPv4 address of the IP-SM-GW to receive the downlink short message.  See NOTE |  |
| ipsmgwIpv6 | Ipv6Addr | C | 0..1 | This IE shall be present if available.  When present, this IE indicates the IPv6 address of the IP-SM-GW to receive the downlink short message.  See NOTE |  |
| ipsmgwFqdn | Fqdn | C | 0..1 | This IE shall be present if available.  When present, this IE indicates the FQDN of the IP-SM-GW to receive the downlink short message.  See NOTE |  |
| correlationId | string | O | 0..1 | Correlation ID |  |
| supportedFeatures | SupportedFeatures | C | 0..1 | This IE shall be present if at least one optional feature defined in clause 6.1.8 is supported. |  |
| NOTE: At least, one of IP-SM-GW addresses shall be included. | | | | | |

##### 6.1.6.2.4 Type: SmsData

Table 6.1.6.2.4-1: Definition of type SmsData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| smsPayload | RefToBinaryData | M | 1 | This IE shall be present, and it shall contain the reference to the SMS Payload Information binary data (see clause 6.1.6.5) |  |

##### 6.1.6.2.5 Type: SmsDeliveryData

Table 6.1.6.2.5-1: Definition of type SmsDeliveryData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| smsPayload | RefToBinaryData | M | 1 | This IE shall be present, and it shall contain the reference to the SMS Payload Information binary data (see clause 6.1.6.5) |  |

#### 6.1.6.3 Simple data types and enumerations

##### 6.1.6.3.1 Introduction

This clause defines simple data types and enumerations that can be referenced from data structures defined in the previous clauses.

##### 6.1.6.3.2 Simple data types

The simple data types defined in table 6.1.6.3.2-1 shall be supported.

Table 6.1.6.3.2-1: Simple data types

|  |  |  |  |
| --- | --- | --- | --- |
| Type Name | Type Definition | Description | Applicability |
|  |  |  |  |

#### 6.1.6.4 Data types describing alternative data types or combinations of data types

In this release of this specification, no alternative data types or combinations of data types are defined.

#### 6.1.6.5 Binary data

##### 6.1.6.5.1 Binary Data Types

Table 6.1.6.5.1-1: Binary Data Types

|  |  |  |
| --- | --- | --- |
| Name | Clause defined | Content type |
| SMS Payload Information | 6.1.6.5.2 | vnd.3gpp.sms |

##### 6.1.6.5.2 SMS Payload Information

SMS Payload Information shall encode a SMS payload as specified in 3GPP TS 23.040 [16] and 3GPP TS 24.011 [17], using the vnd.3gpp.sms content-type.

SMS Payload Information may encode e.g. the following content:

- CP-DATA, CP-ACK, CP-ERROR as specified in 3GPP TS 23.040 [16] and 3GPP TS 24.011 [17].

### 6.1.7 Error Handling

#### 6.1.7.1 General

For the Nipsmgw\_SMService API, HTTP error responses shall be supported as specified in clause 4.8 of 3GPP TS 29.501 [5]. Protocol errors and application errors specified in table 5.2.7.2-1 of 3GPP TS 29.500 [4] shall be supported for an HTTP method if the corresponding HTTP status codes are specified as mandatory for that HTTP method in table 5.2.7.1-1 of 3GPP TS 29.500 [4].

In addition, the requirements in the following clauses are applicable for the Nipsmgw\_SMService API.

#### 6.1.7.2 Protocol Errors

No specific procedures for the Nipsmgw\_SMService service are specified.

#### 6.1.7.3 Application Errors

The application errors defined for the Nipsmgw\_SMService service are listed in Table 6.1.7.3-1.

Table 6.1.7.3-1: Application errors

|  |  |  |
| --- | --- | --- |
| Application Error | HTTP status code | Description |
| SMS\_PAYLOAD\_MISSING | 400 Bad Request | The expected SMS payload content is missing. |
| SMS\_PAYLOAD\_ERROR | 400 Bad Request | Errors exist in the format of SMS payload. |
| USER\_NOT\_FOUND | 404 Not Found | The provided subscriber identifier is not found. |
| ROUTING\_INFO\_NOT\_FOUND | 404 Not Found | The routing information for SMS to be operated is invalid or not found in IP-SM-GW |

### 6.1.8 Feature negotiation

The optional features in table 6.1.8-1 are defined for the Nipsmgw\_SMService API. They shall be negotiated using the extensibility mechanism defined in clause 6.6 of 3GPP TS 29.500 [4].

Table 6.1.8-1: Supported Features

|  |  |  |
| --- | --- | --- |
| Feature number | Feature Name | Description |
|  |  |  |

### 6.1.9 Security

As indicated in 3GPP TS 33.501 [8] and 3GPP TS 29.500 [4], the access to the Nipsmgw\_SMService API may be authorized by means of the OAuth2 protocol (see IETF RFC 6749 [9]), based on local configuration, using the "Client Credentials" authorization grant, where the NRF (see 3GPP TS 29.510 [10]) plays the role of the authorization server.

If OAuth2 is used, an NF Service Consumer, prior to consuming services offered by the Nipsmgw\_SMService API, shall obtain a "token" from the authorization server, by invoking the Access Token Request service, as described in 3GPP TS 29.510 [10], clause 5.4.2.2.

NOTE: When multiple NRFs are deployed in a network, the NRF used as authorization server is the same NRF that the NF Service Consumer used for discovering the Nipsmgw\_SMService service.

The Nipsmgw\_SMService API defines the following scopes for Oauth2 authorization as specified in 3GPP TS 33.501 [8]:

Table 6.1.9-1: OAuth2 scopes defined in Nipsmgw\_SMService API

|  |  |
| --- | --- |
| Scope | Description |
| "nipsmgw\_smservice" | Access to the Nipsmgw\_SMService API. |
| "nipsmgw\_smservice:mtsminfos:write" | Access to write MT SM Infos |
| "nipsmgw\_smservice:sendsms:invoke" | Access to invoke Send SMS |

### 6.1.10 HTTP redirection

An HTTP request may be redirected to a different IP-SM-GW service instance, within the same IP-SM-GW or a different IP-SM-GW of an IP-SM-GW set, e.g. when an IP-SM-GW service instance is part of an IP-SM-GW (service) set or when using indirect communications (see 3GPP TS 29.500 [4]).

An SCP that reselects a different IP-SM-GW producer instance will return the NF Instance ID of the new IP-SM-GW producer instance in the 3gpp-Sbi-Producer-Id header, as specified in clause 6.10.3.4 of 3GPP TS 29.500 [4].

If an IP-SM-GW within an IP-SM-GW set redirects a service request to a different IP-SM-GW of the set using a 307 Temporary Redirect or 308 Permanent Redirect status code, the identity of the new IP-SM-GW towards which the service request is redirected shall be indicated in the 3gpp-Sbi-Target-Nf-Id header of the 307 Temporary Redirect or 308 Permanent Redirect response as specified in clause 6.10.9.1 of 3GPP TS 29.500 [4].

## 6.2 Nrouter\_SMService Service API

### 6.2.1 Introduction

The Nrouter\_SMService shall use the Nrouter\_SMService API.

The API URI of the Nrouter\_SMService API shall be:

**{apiRoot}/<apiName>/<apiVersion>**

The request URIs used in HTTP requests from the NF service consumer towards the NF service producer shall have the Resource URI structure defined in clause 4.4.1 of 3GPP TS 29.501 [5], i.e.:

**{apiRoot}/<apiName>/<apiVersion>/<apiSpecificResourceUriPart>**

with the following components:

- The {apiRoot} shall be set as described in 3GPP TS 29.501 [5].

- The <apiName>shall be "nrouter-smservice".

- The <apiVersion> shall be "v1".

- The <apiSpecificResourceUriPart> shall be set as described in clause 6.2.3.

### 6.2.2 Usage of HTTP

#### 6.2.2.1 General

HTTP/2, IETF RFC 9113 [11], shall be used as specified in clause 5 of 3GPP TS 29.500 [4].

HTTP/2 shall be transported as specified in clause 5.3 of 3GPP TS 29.500 [4].

The OpenAPI [6] specification of HTTP messages and content bodies for the Nrouter\_SMService API is contained in Annex A.

#### 6.2.2.2 HTTP standard headers

##### 6.2.2.2.1 General

See clause 5.2.2 of 3GPP TS 29.500 [4] for the usage of HTTP standard headers.

##### 6.2.2.2.2 Content type

JSON, IETF RFC 8259 [12], shall be used as content type of the HTTP bodies specified in the present specification as specified in clause 5.4 of 3GPP TS 29.500 [4]. The use of the JSON format shall be signalled by the content type "application/json".

"Problem Details" JSON object shall be used to indicate additional details of the error in a HTTP response body and shall be signalled by the content type "application/problem+json", as defined in IETF RFC 9457 [13].

Multipart messages shall also be supported (see clause 6.2.2.4) using the content type "multipart/related", comprising:

- one JSON body part with the "application/json" content type; and

- one binary body part with 3gpp vendor specific content subtypes.

The 3gpp vendor specific content subtypes defined in Table 6.2.2.2.2-1 shall be supported.

Table 6.2.2.2.2-1: 3GPP vendor specific content subtypes

|  |  |
| --- | --- |
| content subtype | Description |
| vnd.3gpp.sms | Binary encoded payload, encoding SMS payload, as specified in 3GPP TS 23.040 [16] and 3GPP TS 24.011 [17]. |
| NOTE: Using 3GPP vendor content subtypes allows to describe the nature of the opaque payload (e.g. SMS payload) without having to rely on metadata in the JSON payload. | |

See clause 6.2.2.4 for the binary payloads supported in the binary body part of multipart messages.

#### 6.2.2.3 HTTP custom headers

The mandatory HTTP custom header fields specified in clause 5.2.3.2 of 3GPP TS 29.500 [4] shall be supported, and the optional HTTP custom header fields specified in clause 5.2.3.3 of 3GPP TS 29.500 [4] may be supported.

#### 6.2.2.4 HTTP multipart messages

HTTP multipart messages shall be supported, to transfer opaque SMS payload (e.g. SMS message, CP Ack, etc.), in the following service operations (and HTTP messages):

- MtForwardSm service operation;

HTTP multipart messages shall include one JSON body part and one binary body part comprising content of SMS payload content (see clause 6.2.6.4).

The JSON body part shall be the "root" body part of the multipart message. It shall be encoded as the first body part of the multipart message. The "Start" parameter does not need to be included.

The multipart message shall include a "type" parameter (see IETF RFC 2387 [18]) specifying the media type of the root body part, i.e. "application/json".

NOTE: The "root" body part (or "root" object) is the first body part the application processes when receiving a multipart/related message, see IETF RFC 2387 [18]. The default root is the first body within the multipart/related message. The "Start" parameter indicates the root body part, e.g. when this is not the first body part in the message.

A binary body part shall include a Content-ID header (see IETF RFC 2045 [19]), and the JSON body part shall make a reference to the binary body part using the Content-ID header field.

Examples of multipart/related messages can be found in Annex B.

### 6.2.3 Resources

#### 6.2.3.1 Overview

This clause describes the structure for the Resource URIs and the resources and methods used for the service.

Figure 6.2.3.1-1 depicts the resource URIs structure for the Nrouter\_SMService API.



Figure 6.2.3.1-1: Resource URI structure of the Nrouter\_SMService API

Table 6.2.3.1-1 provides an overview of the resources and applicable HTTP methods.

Table 6.2.3.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource purpose/name | Resource URI (relative path after API URI) | HTTP method or custom operation | Description (service operation) |
| MtSmInfo  (Document) | /mt-sm-infos/{gpsi} | PUT | Create Routing Information for MT SMS. |
| /mt-sm-infos/{gpsi}/sendsms | sendsms  (POST) | It is used for the MtForwardSm service operation, to allow NF Service Consumer to send SMS payload in downlink direction. |

#### 6.2.3.2 Resource: MtSmInfos (Store)

##### 6.2.3.2.1 Description

This resource represents the collection of Mobile Terminated Short Message Information in SMS Router.

This resource is modelled with the Store resource archetype (see clause C.3 of 3GPP TS 29.501 [5]).

No HTTP method has been defined for this resource.

##### 6.2.3.2.2 Resource Definition

Resource URI: **{apiRoot}/nrouter-smsevice/<apiVersion>/mt-sm-infos**

This resource shall support the resource URI variables defined in table 6.2.3.2.2-1.

Table 6.2.3.2.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 6.2.1 |

##### 6.2.3.2.3 Resource Standard Methods

No HTTP method has been defined for the Mobile Terminated Short Message Information collection resource.

#### 6.2.3.3 Resource: MtSmInfo (Document)

##### 6.2.3.3.1 Description

This resource represents an individual Mobile Terminated Short Message Information in SMS Router.

This resource is modelled with the Document resource archetype (see clause C.1 of 3GPP TS 29.501 [5]).

##### 6.2.3.3.2 Resource Definition

Resource URI: **{apiRoot}/nrouter-smsevice/<apiVersion>/mt-sm-infos/{gpsi}**

This resource shall support the resource URI variables defined in table 6.2.3.3.2-1.

Table 6.2.3.3.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 6.2.1 |
| gpsi | gpsi | Represents the Generic Public Subscription Identifier with MSISDN (see 3GPP TS 23.501 [2] clause 5.9.8)  pattern: See pattern of type Gpsi in 3GPP TS 29.571 [15] |

##### 6.2.3.3.3 Resource Standard Methods

6.2.3.3.3.1 PUT

This method creates an individual resource of Mobile Terminated Short Message Information in the SMS Router, or updates the indicated resource of Mobile Terminated Short Message Information in the SMS Router.

This method shall support the URI query parameters specified in table 6.2.3.3.3.1-1.

Table 6.2.3.3.3.1-1: URI query parameters supported by the PUT method on this resource

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description | Applicability |
| n/a |  |  |  |  |  |

This method shall support the request data structures specified in table 6.2.3.3.3.1-2 and the response data structures and response codes specified in table 6.2.3.3.3.1-3.

Table 6.1.3.3.3.1-2: Data structures supported by the PUT Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| CreateRoutingData | M | 1 | Representation of the UE's Mobile Terminated Short Message Information to be created in the SMS Router, or to be updated in the SMS Router. |

Table 6.2.3.3.3.1-3: Data structures supported by the PUT Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| CreatedRoutingData | M | 1 | 201 Created | This case represents the successful creation of an UE's Mobile Terminated Short Message Information.  The HTTP response shall include a "Location" HTTP header that contains the resource URI of the created resource. |
| CreatedRoutingData | M | 1 | 200 OK | Upon success, a response body containing a representation of the updated UE's Mobile Terminated Short Message Information shall be returned. |
| n/a |  |  | 204 No Content | Upon success, an empty response body shall be returned |
| RedirectResponse | O | 0..1 | 307 Temporary Redirect | Temporary redirection.  (NOTE 2) |
| RedirectResponse | O | 0..1 | 308 Permanent Redirect | Permanent redirection.  (NOTE 2) |
| NOTE 1: The manadatory HTTP error status code for the PUT method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] also apply.  NOTE 2: RedirectResponse may be inserted by an SCP, see clause 6.10.9.1 of 3GPP TS 29.500 [4]. | | | | |

Table 6.2.3.3.3.1-4: Headers supported by the 201 response code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains the URI of the newly created resource, according to the structure: {apiRoot}/nrouter-smsevice/<apiVersion>/mt-sm-infos/{gpsi} |

Table 6.2.3.3.3.1-3: Headers supported by the 307 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | An alternative URI of the resource located on an alternative service instance within the same SMS Router or SMS Router (service) set.  For the case, when a request is redirected to the same target resource via a different SCP, see clause 6.10.9.1 in 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target NF (service) instance ID towards which the request is redirected |

Table 6.2.3.3.3.1-6: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | An alternative URI of the resource located on an alternative service instance within the same SMS Router or SMS Router (service) set.  For the case, when a request is redirected to the same target resource via a different SCP, see clause 6.10.9.1 in 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target NF (service) instance ID towards which the request is redirected |

##### 6.2.3.3.4 Resource Custom Operations

6.2.3.3.4.1 Overview

Table 6.2.3.3.4.1-1: Custom operations

|  |  |  |  |
| --- | --- | --- | --- |
| Operation name | Custom operaration URI | Mapped HTTP method | Description |
| sendsms | /mt-sm-infos/{gpsii}/sendsms | POST | Send MT SMS message or the related Delivery Report. |

6.2.3.3.4.2 Operation: sendsms

6.2.3.3.4.2.1 Description

This custom operation is used for NF Service Consumers to send SMS message in downlink direction.

6.2.3.3.4.2.2 Operation Definition

This custom operation is used to send a SMS payload to an UE's Mobile Terminated Short Message Information resource in the SMS Router.

This operation shall support the request data structures specified in table 6.2.3.3.4.2.2-1 and the response data structure and response codes specified in table 6.2.3.3.4.2.2-2.

Table 6.2.3.3.4.2.2-1: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| SmsData | M | 1 | Representation of the MT SMS message to be sent. |

Table 6.2.3.3.4.2.2-2: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response  codes | Description |
| SmsDeliveryData | M | 1 | 200 OK | This case represents the successful of sending SMS message in downlink direction, with necessary response data on the received delivery report. |
| RedirectResponse | O | 0..1 | 307 Temporary Redirect | Temporary redirection.  (NOTE 2) |
| RedirectResponse | O | 0..1 | 308 Permanent Redirect | Permanent redirection.  (NOTE 2) |
| ProblemDetails | O | 0..1 | 400 Bad Request | This case represents an unsuccessful delivery of SMS message.  The "cause" attribute may be used to indicate one of the following application errors:  - SMS\_PAYLOAD\_MISSING, if the expected SMS payload content is missing;  - SMS\_PAYLOAD\_ERROR, if error exists in the SMS payload content. |
| ProblemDetails | O | 0..1 | 404 Not Found | This case represents an unsuccessful delivery of SMS payload.  The "cause" attribute may be used to indicate one of the following application errors:  - ROUTING\_INFO\_NOT\_FOUND, if the routing information for SMS to be operated is invalid or not found in SMS Router.  - USER\_NOT\_FOUND, if the UE identified by the GPSI is not found in the SMS Router. |
| NOTE 1: The manadatory HTTP error status code for the POST method listed in Table 5.2.7.1-1 of 3GPP TS 29.500 [4] also apply.  NOTE 2: RedirectResponse may be inserted by an SCP, see clause 6.10.9.1 of 3GPP TS 29.500 [4]. | | | | |

Table 6.2.3.3.4.2.2-3: Headers supported by the 307 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | An alternative URI of the resource located on an alternative service instance within the same SMS Router or SMS Router (service) set.  For the case, when a request is redirected to the same target resource via a different SCP, see clause 6.10.9.1 in 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target NF (service) instance ID towards which the request is redirected |

Table 6.2.3.3.4.2.2-4: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | An alternative URI of the resource located on an alternative service instance within the same SMS Router or SMS Router (service) set.  For the case, when a request is redirected to the same target resource via a different SCP, see clause 6.10.9.1 in 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target NF (service) instance ID towards which the request is redirected |

### 6.2.4 Custom Operations without associated resources

In this release of this specification, no custom operations without associated resources are defined.

### 6.2.5 Notifications

In this release of this specification, no notification procedures are defined.

### 6.2.6 Data Model

#### 6.2.6.1 General

This clause specifies the application data model supported by the API.

Table 6.2.6.1-1 specifies the data types defined for the Nrouter\_SMService service based interface protocol.

Table 6.2.6.1-1: Nrouter\_SMService specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Clause defined | Description | Applicability |
| CreatedRoutingData | 6.2.6.2.2 | Information used for receiving the MT SMS. |  |

Table 6.2.6.1-2 specifies data types re-used by the Nrouter\_SMService service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nrouter\_SMService service based interface.

Table 6.2.6.1-2: Nrouter\_SMService re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| CreateRoutingData | 6.1.6.2.2 | Information used for creating or updating the routing information of the user. |  |
| SmsData | 6.1.6.2.4 | Information within request message invoking MtForwardSm service operation, for delivering MT SMS. |  |
| SmsDeliveryData | 6.1.6.2.5 | Information within response message invoking MtForwardSm service operation, for delivering MT SMS Delivery Report. |  |
| ProblemDetails | 3GPP TS 29.571 [15] | Common Data Type used in response bodies |  |
| RedirectResponse | 3GPP TS 29.571 [15] | Redirect Response |  |
| Gpsi | 3GPP TS 29.571 [15] | General Public Subscription Identifier |  |
| NfInstanceId | 3GPP TS 29.571 [15] | NF Instance ID |  |
| RefToBinaryData | 3GPP TS 29.571 [15] | Information for indicating the binary content of SMS payload. |  |
| Ipv4Addr | 3GPP TS 29.571 [15] | IPv4 address |  |
| Ipv6Addr | 3GPP TS 29.571 [15] | IPv6 address |  |
| SupportedFeatures | 3GPP TS 29.571 [15] | Supported Features |  |
| Fqdn | 3GPP TS 29.571 [15] | Fully Qualified Domain Name |  |

#### 6.2.6.2 Structured data types

##### 6.2.6.2.1 Introduction

This clause defines the structures to be used in resource representations.

##### 6.2.6.2.2 Type: CreatedRoutingData

Table 6.2.6.2.2-1: Definition of type CreatedRoutingData

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| routerIpv4 | Ipv4Addr | C | 0..1 | This IE shall be present if available.  When present, this IE indicates the IPv4 address of the SMS Router to receive the downlink short message.  See NOTE |  |
| routerIpv6 | Ipv6Addr | C | 0..1 | This IE shall be present if available.  When present, this IE indicates the IPv6 address of the SMS Router to receive the downlink short message.  See NOTE |  |
| routerFqdn | Fqdn | C | 0..1 | This IE shall be present if available.  When present, this IE indicates the FQDN of the SMS Router to receive the downlink short message.  See NOTE |  |
| supportedFeatures | SupportedFeatures | C | 0..1 | This IE shall be present if at least one optional feature defined in clause 6.1.8 is supported. |  |
| NOTE: At least, one of SMS Router addresses shall be included. | | | | | |

#### 6.2.6.3 Simple data types and enumerations

##### 6.2.6.3.1 Introduction

This clause defines simple data types and enumerations that can be referenced from data structures defined in the previous clauses.

##### 6.2.6.3.2 Simple data types

The simple data types defined in table 6.2.6.3.2-1 shall be supported.

Table 6.2.6.3.2-1: Simple data types

|  |  |  |  |
| --- | --- | --- | --- |
| Type Name | Type Definition | Description | Applicability |
|  |  |  |  |

##### 6.2.6.3.3 Enumeration: <EnumType1>

The enumeration <EnumType1> represents <something>. It shall comply with the provisions defined in table 6.1.6.3.3-1.

Table 6.2.6.3.3-1: Enumeration < EnumType1>

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
|  |  |  |

#### 6.2.6.4 Data types describing alternative data types or combinations of data types

In this release of this specification, no alternative data types or combinations of data types are defined.

#### 6.2.6.5 Binary data

See clause 6.1.6.5.

### 6.2.7 Error Handling

#### 6.2.7.1 General

For the Nrouter\_SMService API, HTTP error responses shall be supported as specified in clause 4.8 of 3GPP TS 29.501 [5]. Protocol errors and application errors specified in table 5.2.7.2-1 of 3GPP TS 29.500 [4] shall be supported for an HTTP method if the corresponding HTTP status codes are specified as mandatory for that HTTP method in table 5.2.7.1-1 of 3GPP TS 29.500 [4].

In addition, the requirements in the following clauses are applicable for the Nrouter\_SMService API.

#### 6.2.7.2 Protocol Errors

No specific procedures for the Nrouter\_SMService service are specified.

#### 6.2.7.3 Application Errors

The application errors defined for the Nrouter\_SMService service are listed in Table 6.2.7.3-1.

Table 6.2.7.3-1: Application errors

|  |  |  |
| --- | --- | --- |
| Application Error | HTTP status code | Description |
| SMS\_PAYLOAD\_MISSING | 400 Bad Request | The expected SMS payload content is missing. |
| SMS\_PAYLOAD\_ERROR | 400 Bad Request | Errors exist in the format of SMS payload. |
| USER\_NOT\_FOUND | 404 Not Found | The provided subscriber identifier is not found. |
| ROUTING\_INFO\_NOT\_FOUND | 404 Not Found | The routing information for SMS to be operated is invalid or not found in SMS Router |

### 6.2.8 Feature negotiation

The optional features in table 6.2.8-1 are defined for the Nrouter\_SMService API. They shall be negotiated using the extensibility mechanism defined in clause 6.6 of 3GPP TS 29.500 [4].

Table 6.2.8-1: Supported Features

|  |  |  |
| --- | --- | --- |
| Feature number | Feature Name | Description |
|  |  |  |

### 6.2.9 Security

As indicated in 3GPP TS 33.501 [8] and 3GPP TS 29.500 [4], the access to the Nrouter\_SMService API may be authorized by means of the OAuth2 protocol (see IETF RFC 6749 [9]), based on local configuration, using the "Client Credentials" authorization grant, where the NRF (see 3GPP TS 29.510 [10]) plays the role of the authorization server.

If OAuth2 is used, an NF Service Consumer, prior to consuming services offered by the Nrouter\_SMService API, shall obtain a "token" from the authorization server, by invoking the Access Token Request service, as described in 3GPP TS 29.510 [10], clause 5.4.2.2.

NOTE: When multiple NRFs are deployed in a network, the NRF used as authorization server is the same NRF that the NF Service Consumer used for discovering the Nrouter\_SMService service.

The Nrouter\_SMService API defines the following scopes for Oauth2 authorization as specified in 3GPP TS 33.501 [8]:

Table 6.2.9-1: OAuth2 scopes defined in Nrouter\_SMService API

|  |  |
| --- | --- |
| Scope | Description |
| "nrouter\_smservice" | Access to the Nrouter\_SMService API. |
| "nrouter\_smservice:mtsminfos:write" | Access to write MT SM Infos |
| "nrouter\_smservice:sendsms:invoke" | Access to invoke Send SMS |

### 6.2.10 HTTP redirection

An HTTP request may be redirected to a different SMS Router service instance, within the same SMS Router or a different SMS Router of an SMS Router set, e.g. when an SMS Router service instance is part of an SMS Router (service) set or when using indirect communications (see 3GPP TS 29.500 [4]).

An SCP that reselects a different SMS Router producer instance will return the NF Instance ID of the new SMS Router producer instance in the 3gpp-Sbi-Producer-Id header, as specified in clause 6.10.3.4 of 3GPP TS 29.500 [4].

If an SMS Router within an SMS Router set redirects a service request to a different SMS Router of the set using a 307 Temporary Redirect or 308 Permanent Redirect status code, the identity of the new SMS Router towards which the service request is redirected shall be indicated in the 3gpp-Sbi-Target-Nf-Id header of the 307 Temporary Redirect or 308 Permanent Redirect response as specified in clause 6.10.9.1 of 3GPP TS 29.500 [4].

Annex A (normative):  
OpenAPI specification

# A.1 General

This Annex specifies the formal definition of the API(s) defined in the present specification. It consists of OpenAPI specifications in YAML format.

This Annex takes precedence when being discrepant to other parts of the specification with respect to the encoding of information elements and methods within the API(s).

NOTE 1: The semantics and procedures, as well as conditions, e.g. for the applicability and allowed combinations of attributes or values, not expressed in the OpenAPI definitions but defined in other parts of the specification also apply.

Informative copies of the OpenAPI specification files contained in this 3GPP Technical Specification are available on a Git-based repository that uses the GitLab software version control system (see clause 5.3.1 of 3GPP TS 29.501 [5] and clause 5B of 3GPP TR 21.900 [7]).

# A.2 Nipsmgw\_SMService API

openapi: 3.0.0

info:

version: '1.1.0-alpha.2'

title: 'Nipsmgw\_SMService Service API'

description: |

IP-SM-GW SMService.

© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.577 V18.1.0; 5G System; IP Short Message Gateway and SMS Router For Short Message Services; Stage 3

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.577/'

security:

- oAuth2ClientCredentials:

- nipsmgw-smservice

- {}

servers:

- url: '{apiRoot}/nipsmgw-smservice/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501.

paths:

/mt-sm-infos/{gpsi}:

put:

summary: Create the routing information for a given UE

operationId: RoutingInfo

tags:

- Creation of Routing Info

security:

- {}

- oAuth2ClientCredentials:

- nipsmgw\_smservice

- oAuth2ClientCredentials:

- nipsmgw\_smservice

- nipsmgw\_smservice:mtsminfos:write

parameters:

- name: gpsi

in: path

required: true

description: Generic Public Subscription Identifier (GPSI)

schema:

type: string

requestBody:

content:

application/json:

schema:

$ref: '#/components/schemas/CreateRoutingData'

required: true

responses:

'201':

description: Routing Information is created in IP-SM-GW

content:

application/json:

schema:

$ref: '#/components/schemas/CreatedRoutingData'

headers:

Location:

description: >

'Contains the URI of the newly created resource, according to the structure:

{apiRoot}/nipsmgw-smservice/<apiVersion>/mt-sm-infos/{gpsi}'

required: true

schema:

type: string

'200':

description: Routing Information is updated in IP-SM-GW

content:

application/json:

schema:

$ref: '#/components/schemas/CreatedRoutingData'

'204':

description: Routing Information is updated in IP-SM-GW

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/mt-sm-infos/{gpsi}/sendsms:

post:

summary: Send SMS payload for a given UE

operationId: SendSMS

tags:

- Send MT SMS message and the delivery report

security:

- {}

- oAuth2ClientCredentials:

- nipsmgw\_smservice

- oAuth2ClientCredentials:

- nipsmgw\_smservice

- nipsmgw\_smservice:sendsms:invoke

parameters:

- name: gpsi

in: path

required: true

description: Generic Public Subscription Identifier (GPSI)

schema:

type: string

requestBody:

content:

multipart/related: # message with a binary body part

schema:

type: object

properties:

jsonData:

$ref: '#/components/schemas/SmsData'

binaryPayload:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryPayload:

contentType: application/vnd.3gpp.sms

headers:

Content-Id:

schema:

type: string

required: true

responses:

'200':

description: sending delivery report

content:

multipart/related: # message with a binary body part

schema:

type: object

properties:

jsonData:

$ref: '#/components/schemas/SmsDeliveryData'

binaryPayload:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryPayload:

contentType: application/vnd.3gpp.sms

headers:

Content-Id:

schema:

type: string

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

nipsmgw-smservice: Access to the nipsmgw-smservice API

nipsmgw-smservice:mtsminfos:write: Access to write MT SM Infos

nipsmgw-smservice:sendsms:invoke: Access to invoke Send SMS

schemas:

CreateRoutingData:

description: Information used for creating or updating the routing information of the user.

type: object

required:

- smsfId

properties:

smsfId:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

CreatedRoutingData:

description: Information used for receiving the MT SMS.

type: object

properties:

ipsmgwIpv4:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

ipsmgwIpv6:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

ipsmgwFqdn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Fqdn'

correlationId:

type: string

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

SmsData:

description: Information within request message for delivering SMS.

type: object

required:

- smsPayload

properties:

smsPayload:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

SmsDeliveryData:

description: >

Information within response message invoking MtForwardSm service operation, for delivering

MT SMS Delivery Report.

type: object

required:

- smsPayload

properties:

smsPayload:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/RefToBinaryData'

# A.3 Nrouter\_SMService API

openapi: 3.0.0

info:

version: '1.1.0-alpha.2'

title: 'Nrouter\_SMService Service API'

description: |

SMS Router SMService.

© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.577 V18.1.0; 5G System; IP Short Message Gateway and SMS Router For Short Message Services; Stage 3

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.577/'

security:

- oAuth2ClientCredentials:

- nrouter-smservice

- {}

servers:

- url: '{apiRoot}/nrouter-smservice/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501.

paths:

/mt-sm-infos/{gpsi}:

put:

summary: Create the routing information for a given UE

operationId: RoutingInfo

tags:

- Creation of Routing Info

security:

- {}

- oAuth2ClientCredentials:

- nrouter\_smservice

- oAuth2ClientCredentials:

- nrouter\_smservice

- nrouter\_smservice:mtsminfos:write

parameters:

- name: gpsi

in: path

required: true

description: Generic Public Subscription Identifier (GPSI)

schema:

type: string

requestBody:

content:

application/json:

schema:

$ref: 'TS29577\_Nipsmgw\_SMService.yaml#/components/schemas/CreateRoutingData'

required: true

responses:

'201':

description: Routing Information is created in SMS Router

content:

application/json:

schema:

$ref: '#/components/schemas/CreatedRoutingData'

headers:

Location:

description: >

'Contains the URI of the newly created resource, according to the structure:

{apiRoot}/nrouter-smservice/<apiVersion>/mt-sm-infos/{gpsi}'

required: true

schema:

type: string

'200':

description: Routing Information is updated in SMS Router

content:

application/json:

schema:

$ref: '#/components/schemas/CreatedRoutingData'

'204':

description: Routing Information is updated in SMS Router

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/mt-sm-infos/{gpsi}/sendsms:

post:

summary: Send SMS payload for a given UE

operationId: SendSMS

tags:

- Send MT SMS message and the delivery report

security:

- {}

- oAuth2ClientCredentials:

- nrouter\_smservice

- oAuth2ClientCredentials:

- nrouter\_smservice

- nrouter\_smservice:sendsms:invoke

parameters:

- name: gpsi

in: path

required: true

description: Generic Public Subscription Identifier (GPSI)

schema:

type: string

requestBody:

content:

multipart/related: # message with a binary body part

schema:

type: object

properties:

jsonData:

$ref: 'TS29577\_Nipsmgw\_SMService.yaml#/components/schemas/SmsData'

binaryPayload:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryPayload:

contentType: application/vnd.3gpp.sms

headers:

Content-Id:

schema:

type: string

required: true

responses:

'200':

description: sending delivery report

content:

multipart/related: # message with a binary body part

schema:

type: object

properties:

jsonData:

$ref: 'TS29577\_Nipsmgw\_SMService.yaml#/components/schemas/SmsDeliveryData'

binaryPayload:

type: string

format: binary

encoding:

jsonData:

contentType: application/json

binaryPayload:

contentType: application/vnd.3gpp.sms

headers:

Content-Id:

schema:

type: string

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

nrouter-smservice: Access to the nrouter-smservice API

nrouter-smservice:mtsminfos:write: Access to write MT SM Infos

nrouter-smservice:sendsms:invoke: Access to invoke Send SMS

schemas:

CreatedRoutingData:

description: Information used for receiving the MT SMS.

type: object

properties:

routerIpv4:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

routerIpv6:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

routerFqdn:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Fqdn'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

Annex B (Informative):  
HTTP Multipart Messages

# B.1 Example of HTTP multipart message

This Annex provides a (partial) example of HTTP multipart message. The example does not aim to be a complete representation of the HTTP message, e.g. additional information or headers can be included.

This Annex is informative and the normative descriptions in this specification prevail over the description in this Annex if there is any difference.

# B.2 Example HTTP multipart message with SMS binary data

Example HTTP multipart message with SMS binary data:

POST /example.com/nipsmgw-smservice/v1/mt-sm-infos/{gpsi}/sendsms HTTP/2

Content-Type: multipart/related; boundary=----Boundary

Content-Length: xyz

------Boundary

Content-Type: application/json

{

"smsPayload": {

"contentId": "sms"

},

}

------Boundary

Content-Type: application/vnd.3gpp.sms

Content-Id: sms

{ … SMS Message binary data …}

------Boundary

The JSON part of the HTTP POST message includes an attribute named "smsPayload" which refers to RefToBinaryData structure. The "contentId" of RefToBinaryData is encoded as a string and used to reference the value of the Content-ID header field of the binary body part.

Annex C (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2022-04 | CT4#109e | C4-222401 |  |  |  | TS skeleton | 0.0.0 |
| 2022-04 | CT4#109e | C4-222341 |  |  |  | Implementation of pCRs agreed at CT4#109e: C4-222279, C4-222280, C4-222283, C4-222398, C4-222399, C4-222402, C4-222403 | 0.1.0 |
| 2022-05 | CT4#110e | C4-223450 |  |  |  | Implementation of pCRs agreed at CT4#110e: C4-223220, C4-223222, C4-223353 | 0.2.0 |
| 2022-06 | CT#96 | CP-221078 |  |  |  | TS presented for information and approval | 1.0.0 |
| 2022-06 | CT#96 | CP-221078 |  |  |  | TS approved at CT#96 | 17.0.0 |
| 2022-09 | CT#97e | CP-222027 | 0001 | - | F | Alignment on the service name used with template | 17.1.0 |
| 2022-09 | CT#97e | CP-222027 | 0002 | - | F | Editorial corrections | 17.1.0 |
| 2022-09 | CT#97e | CP-222027 | 0003 | - | F | Update on the content type for OpenAPI | 17.1.0 |
| 2022-09 | CT#97e | CP-222058 | 0004 | - | F | 29.577 Rel-17 API version and External doc update | 17.1.0 |
| 2022-12 | CT#98e | CP-223028 | 0005 | 1 | F | Missing Mandatory Status Codes in OpenAPI | 18.0.0 |
| 2022-12 | CT#98e | CP-223033 | 0006 | - | F | 29.577 Rel-18 API version and External doc update | 18.0.0 |
| 2023-06 | CT#100 | CP-231026 | 0007 | 3 | F | Location header description | 18.1.0 |
| 2023-06 | CT#100 | CP-231026 | 0009 | - | B | OAuth2 scopes in the Nipsmgw\_SMService API | 18.1.0 |
| 2023-06 | CT#100 | CP-231028 | 0010 | 1 | B | OAuth2 scopes in the Nrouter\_SMService API | 18.1.0 |
| 2023-06 | CT#100 | CP-231070 | 0011 | - | F | 29.577 Rel-18 API version and External doc update | 18.1.0 |
| 2023-12 | CT#102 | CP-233027 | 0012 | - | F | HTTP RFCs obsoleted by IETF RFC 9113 | 18.2.0 |
| 2023-12 | CT#102 | CP-233030 | 0013 | - | F | ProblemDetails RFC 7807 obsoleted by 9457 | 18.2.0 |