3GPP TS 29.594 V18.3.0 (2023-12)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Core Network and Terminals;

5G System; Spending Limit Control Service;

Stage 3

(Release 18)

**



The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPP Organisational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPP only. The Organisational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organisational Partners' Publications Offices.

Keywords

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

<http://www.3gpp.org>

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 6

1 Scope 7

2 References 7

3 Definitions and abbreviations 8

3.1 Definitions 8

3.2 Abbreviations 8

4 Nchf\_SpendingLimitControl Service 9

4.1 Service Description 9

4.1.1 Overview 9

4.1.2 Service Architecture 9

4.1.3 Network Functions 10

4.1.3.1 Charging Function (CHF) 10

4.1.3.2 NF Service Consumers 10

4.2 Service Operations 10

4.2.1 Introduction 10

4.2.2 Nchf\_SpendingLimitControl\_Subscribe service operation 10

4.2.2.1 General 10

4.2.2.2 Initial spending limit retrieval 11

4.2.2.3 Intermediate spending limit report retrieval 12

4.2.3 Nchf\_SpendingLimitControl\_Unsubscribe service operation 14

4.2.3.1 General 14

4.2.3.2 Unsubscribe from spending limit reporting 14

4.2.4 Nchf\_SpendingLimitControl\_Notify service operation 15

4.2.4.1 General 15

4.2.4.2 Spending limit report 15

4.2.4.3 Subscription termination request by CHF 17

5 Nchf\_SpendingLimitControl Service API 18

5.1 Introduction 18

5.2 Usage of HTTP 18

5.2.1 General 18

5.2.2 HTTP standard headers 18

5.2.2.1 General 18

5.2.2.2 Content type 18

5.2.3 HTTP custom headers 19

5.2.3.1 General 19

5.3 Resources 19

5.3.1 Resource Structure 19

5.3.2 Resource: Spending Limit Retrieval Subscriptions (Collection) 19

5.3.2.1 Description 19

5.3.2.2 Resource definition 19

5.3.2.3 Resource Standard Methods 20

5.3.2.3.1 POST 20

5.3.2.4 Resource Custom Operations 20

5.3.3 Resource: Individual Spending Limit Retrieval Subscription (Document) 20

5.3.3.1 Description 20

5.3.3.2 Resource definition 21

5.3.3.3 Resource Standard Methods 21

5.3.3.3.1 PUT 21

5.3.3.3.2 DELETE 22

5.4 Custom Operations without associated resources 23

5.5 Notifications 23

5.5.1 General 23

5.5.2 Spending limit notification 24

5.5.2.1 Description 24

5.5.2.2 Target URI 24

5.5.2.3 Standard Methods 24

5.5.2.3.1 POST 24

5.5.3 Subscription Termination 25

5.5.3.1 Description 25

5.5.3.2 Target URI 25

5.5.3.3 Standard Methods 26

5.5.3.3.1 POST 26

5.6 Data Model 27

5.6.1 General 27

5.6.2 Structured data types 27

5.6.2.1 Introduction 27

5.6.2.2 Type SpendingLimitContext 28

5.6.2.3 Type SpendingLimitStatus 29

5.6.2.4 Type PolicyCounterInfo 30

5.6.2.5 Type PendingPolicyCounterStatus 30

5.6.2.6 Type SubscriptionTerminationInfo 30

5.6.3 Simple data types and enumerations 31

5.6.3.1 Introduction 31

5.6.3.2 Simple data types 31

5.6.3.3 Enumeration: TerminationCause 31

5.7 Error handling 31

5.7.1 General 31

5.7.2 Protocol Errors 31

5.7.3 Application Errors 31

5.8 Feature negotiation 32

5.9 Security 32

Annex A (normative): OpenAPI specification 33

A.1 General 33

A.2 Nchf\_SpendingLimitControl Service API 33

Annex B (normative): 5GC and EPC interworking scenario support 38

B.1 Scope 38

B.2 Nchf\_SpendingLimitControl Service 38

B.2.1 Service Description 38

B.2.1.1 Overview 38

B.2.1.2 Service Architecture 38

B.3 Service Operation 38

B.3.1 Introduction 38

B.3.2 Nchf\_SpendingLimitControl\_Subscribe Service Operation 38

B.3.3 Nchf\_SpendingLimitControl\_Unsubscribe Service Operation 39

B.3.4 Nchf\_SpendingLimitControl\_Notify Service Operation 39

Annex C (normative): Wireless and wireline convergence access support 39

C.1 Scope 39

C.2 Nchf\_SpendingLimitControl Service 39

C.2.1 Service Description 39

C.2.1.1 Overview 39

C.2.1.2 Service Architecture 39

C.3 Service Operation 39

C.3.1 Introduction 39

C.3.2 Nchf\_SpendingLimitControl\_Subscribe Service Operation 39

C.3.2.1 General 39

C.3.3 Nchf\_SpendingLimitControl\_Unsubscribe Service Operation 40

C.3.4 Nchf\_SpendingLimitControl\_Notify Service Operation 40

Annex D (informative): Change history 41

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present specification provides the stage 3 definition of the Spending Limit Control Service of the 5G System.

The 5G System Architecture is defined in 3GPP TS 23.501 [2]. The stage 2 definition and related procedures for the Spending Limit Control Service are specified in 3GPP TS 23.502 [3] and 3GPP TS 23.503 [6].

The 5G System stage 3 call flows are provided in 3GPP TS 29.513 [12].

The Technical Realization of the Service Based Architecture and the Principles and Guidelines for Services Definition are specified in 3GPP TS 29.500 [4] and 3GPP TS 29.501 [5].

The Spending Limit Control Service is provided by the Charging Function (CHF) and enables the NF service consumer to retrieve policy counter status information. The internal CHF functionality for policy counter management provisioning is specified in 3GPP TS 32.240 [7].

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[3] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[4] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[5] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[6] 3GPP TS 23.503: "Policy and Charging Control Framework for the 5G System; Stage 2".

[7] 3GPP TS 32.240: "Charging architecture and principles; Stage 2".

[8] IETF RFC 7540: "Hypertext Transfer Protocol Version 2 (HTTP/2)".

[9] OpenAPI: "OpenAPI Specification Version 3.0.0", <https://spec.openapis.org/oas/v3.0.0>.

[10] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format".

[11] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces".

[12] 3GPP TS 29.513: "5G System; Policy and Charging Control signalling flows and QoS parameter mapping; Stage 3".

[13] IETF RFC 9457: "Problem Details for HTTP APIs".

[14] 3GPP TS 33.501: "Security architecture and procedures for 5G system".

[15] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[16] 3GPP TS 29.510: "5G System; Network Function Repository Services; Stage 3".

[17] 3GPP TR 21.900: "Technical Specification Group working methods".

[18] 3GPP TS 29.512: "5G System; Session Management Policy Control Service; Stage 3".

[19] 3GPP TS 23.316: "Wireless and wireline convergence access support for the 5G System (5GS)".

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**Nchf:** Service-based interface exhibited by Charging Function.

**Policy counter:** A mechanism within the CHF to track spending applicable to a subscriber.

**Policy counter identifier:** A reference to a policy counter in the CHF for a subscriber.

**Policy counter status:** A label whose values are not standardized and that is associated with a policy counter's value relative to the spending limit(s) (the number of possible policy counter status values for a policy counter is one greater than the number of thresholds associated with that policy counter, i.e. policy counter status values describe the status around the thresholds). This is used to convey information relating to subscriber spending from CHF to PCF. Specific labels are configured jointly in CHF and PCF.

**Spending limit:** A spending limit is the usage limit of a policy counter (e.g. monetary, volume, duration) that a subscriber is allowed to consume.

**Spending limit report:** A notification, containing the current policy counter status generated from the CHF to the PCF.

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

5G-RG 5G Residential Gateway

CCS Converged Charging System

CHF Charging Function

CTS Charging Trigger Function

FN-RG Fixed Network Residential Gateway

GCI Global Cable Identifier

GLI Global Line Identifier

GPSI Generic Public Subscription Identifier

NF Network Function

NRF Network Repository Function

PCF Policy Control Function

SUPI Subscription Permanent Identifier

W-AGF Wireline Access Gateway Function

# 4 Nchf\_SpendingLimitControl Service

## 4.1 Service Description

### 4.1.1 Overview

The Nchf\_SpendingLimitControl service, as defined in 3GPP TS23.502 [3] and 3GPP TS23.503 [6], is provided by the Charging Function (CHF).

The Nchf\_SpendingLimitControl service enables the NF service consumer (e.g. PCF) to retrieve policy counter status information and spending limit reporting per UE from the CHF.

If the spending limit reporting is no more required, the Nchf\_SpendingLimitControl service enables the NF service consumer to unsubscribe from the reporting.

Nchf\_SpendingLimitControl Service applies to the cases where the PCF interacts with the CHF in the non-roaming scenario, and for roaming scenario the H-PCF for the PDU session interacts with the H-CHF in the home-routed scenario. Roaming scenarios are not supported for the PCF for the UE in this release of the specification.

### 4.1.2 Service Architecture

The Nchf\_SpendingLimitControl service is provided by the CHF and consumed by the NF service consumer (e.g. PCF), as shown in figure 4.1.2-1 for the SBI representation model and in figure 4.1.2-2 for the reference point representation model.



Figure 4.1.2-1: Nchf\_SpendingLimitControl service architecture, SBI representation



Figure 4.1.2-2: Nchf\_SpendingLimitControl service architecture, reference point representation

### 4.1.3 Network Functions

#### 4.1.3.1 Charging Function (CHF)

The Charging Function (CHF) is part of the Converged Charging System (CCS). The CHF provides the Nchf\_SpendingLimitControl service and is specified in 3GPP TS 32.240 [7].

#### 4.1.3.2 NF Service Consumers

The PCF is the known NF service consumer, as defined in 3GPP TS 23.502 [3]. The NF service consumer accesses policy counter status information relating to the subscriber spending from the CHF and uses the status of each relevant policy counter as input to its policy decision as required by the decision logic.

## 4.2 Service Operations

### 4.2.1 Introduction

The service operations defined for the Nchf\_SpendingLimitControl service are shown in table 4.2.1-1.

Table 4.2.1-1: Nchf\_SpendingLimitControl Service Operations

| **Service operation name** | **Description** | **Initiated by** |
| --- | --- | --- |
| Nchf\_SpendingLimitControl\_Subscribe | This service operation is used by NF service consumers to subscribe to notification of changes in the status of the policy counters available and retrieval of the status of the policy counters for which subscription is accepted. | NF service consumer (e.g. PCF) |
| Nchf\_SpendingLimitControl\_Unsubscribe | This service operation is used by NF service consumers to unsubscribe from notification of changes in the status of all policy counters. | NF service consumer (e.g. PCF) |
| Nchf\_SpendingLimitControl\_Notify | This service operation is used by the CHF to notify the NF service consumers about the change of the status of the subscribed policy counters. Alternatively, it can be used by the CHF to notify that the status for one or multiple subscribed policy counter will change in the future, indicating the time when this change shall be applied. Alternatively, it is also used to notify the NF service consumer of the removal of a subscriber from the CHF system for the purpose that the NF service consumer can terminate the subscriptions of all policy counters of the subscriber. | CHF |

### 4.2.2 Nchf\_SpendingLimitControl\_Subscribe service operation

#### 4.2.2.1 General

The Nchf\_SpendingLimitControl\_Subscribe service operation is used by the NF service consumer to subscribe to notification of changes in the status of the policy counters available and to retrieve the status of the policy counters for which the subscription is accepted. The following procedures are related to the subscribe service operation:

- initial spending limit retrieval; and

- intermediate spending limit report retrieval.

#### 4.2.2.2 Initial spending limit retrieval

Figure 4.2.2.2-1 shows the scenario where the NF service consumer sends a request to the CHF to retrieve the status of policy counters available at the CHF and to subscribe to spending limit reporting (see also 3GPP TS 23.502 [3], figure 4.16.8.2.1).



Figure 4.2.2.2-1: NF service consumer subscribes to retrieve policy counter status and spending limit reporting

The NF service consumer shall send an HTTP POST request to the resource "{apiRoot}/nchf-spendinglimitcontrol/v1/subscriptions" representing the "Spending Limit Retrieval Subscriptions", as shown in figure 4.2.2.2-1, step 1, to create a subscription for retrieval of the policy counter status and spending limit reporting.

The "SpendingLimitContext" data structure provided in the request body shall include:

- the Subscription Permanent Identifier (SUPI) encoded in the "supi" attribute;

- the notification correlation target address encoded in the "notifUri" attribute; and

- If the feature "NotificationCorrelation" is supported, a Notification Correlation Identifier assigned by the NF service consumer for the requested notifications encoded in the "notifId" attribute, if the "notifUri" does not encode within the provided URI the notification correlation Id.

NOTE: NF service consumer (e.g. PCF) ensures the combination of notifUri and notifId is unique per subscription in the whole network, including multiple network slices scenario.

The "SpendingLimitContext" data structure provided in the request body may include:

- the General Public Subscription Identifier (GPSI) encoded in the "gpsi" attribute;

- Event Filter information "list of policy counter identifier(s)" encoded in the "policyCounterIds" attribute. The "policyCounterIds" attribute shall contain the list of policy counter identifiers to be subscribed to. If the "policyCounterIds" attribute is omitted, the subscription is to all available policy counters; and

- when the feature "SubscriptionExpirationTimeControl" is supported by the NF service consumer, the NF service consumer may include an expiry time encoded in the "expiry" attribute, representing the time up to which the subscription is desired to be kept active. When the "expiry" attribute is omitted in the request, it represents the NF service consumer does not have any time constraint in the duration of the subscription.

If the CHF cannot successfully fulfil the received HTTP POST request due to an internal CHF error or due to the error in the HTTP POST request, the CHF shall send the HTTP error response as specified in clause 5.7.

If the subscriber specified in the request is unknown to the CHF, the CHF shall indicate in an HTTP "400 Bad Request" response the cause for the rejection with the "cause" attribute set to "USER\_UNKNOWN".

If the CHF has no available policy counters specified for the subscriber, the CHF shall indicate in an HTTP "400 Bad Request" response the cause for the rejection with the "cause" attribute set to "NO\_AVAILABLE\_POLICY\_COUNTERS ".

If one or more policy counters specified in the request in the "policyCounterIds" attribute are unknown to the CHF, and the CHF is configured to reject request, the CHF shall indicate in an HTTP "400 Bad Request" response the cause for the rejection with the "cause" attribute set to "UNKNOWN\_POLICY\_COUNTERS" and the unknown policy counter identifiers within the "invalidParams" attribute.

Otherwise, upon the reception of an HTTP POST request the CHF shall:

- create a new subscription resource, which contains the list of the policy counters included in the "policyCounterIds" attribute, or if the "policyCounterIds" attribute is omitted, all the policy counters of the subscriber;

- assign a subscriptionId; and

- store the subscription resource.

After the CHF created an "Individual Spending Limit Retrieval Subscription" resource, the CHF shall respond with "201 Created" response with a Location header field containing the URI of the created subscription resource and the message body containing a representation of the created subscription, as shown in figure 4.2.2.2-1, step 2.

The SpendingLimitStatus data structure provided in the response body shall include the status of the requested subscribed policy counters in the "statusInfos" map, where every PolicyCounterInfo entry shall contain:

- the policy counter identifier in the "policyCounterId" attribute; and

- the policy counter status in the "currentStatus" attribute.

When a requested policy counter identifier is known by the CHF, but it is not applicable to the subscriber (e.g. not provisioned), the CHF may include it in the "statusInfos" map, and set the "currentStatus" attribute to an operator configured policy counter status to indicate this to the NF service consumer.

When one or more policy counters specified in the request in the "policyCounterIds" attribute are unknown to the CHF, and the CHF is configured to accept the request, the CHF may include the unknown policy counters in the "statusInfos" map, and set the "currentStatus" attribute to an operator configured policy counter status to indicate this to the NF service consumer.

A PolicyCounterInfo data structure may include the list of the pending policy counter statuses and their activation times within the attribute "penPolCounterStatuses".

When the feature "SubscriptionExpirationTimeControl" is supported, the CHF may include the "expiry" attribute, representing the time up to which the subscription shall be kept active. If an expiry time was included in the subscription request, then the expiry time shall be returned in the response, and the value shall be less than or equal to the requested value. When the "expiry" attribute is omitted in the request and in the response, it represents neither the CHF or the NF service consumer have time constrains in the duration of the subscription and shall be kept active till the explicit subscription termination as described in clause 4.2.3.2 and clause 4.2.4.3.

NOTE 1: If the NF Service Consumer does not include a expiry time in the request, the CHF can include a expiry time in the response that represents the time after which the subscription becomes invalid.

NOTE 2: Once the subscription expires, if the NF service consumer wants to keep receiving notifications, it needs to create a new subscription in the CHF, as specified in this clause.

#### 4.2.2.3 Intermediate spending limit report retrieval

Figure 4.2.2.3-1 shows the scenario where the NF service consumer sends a request to the CHF to modify the existing subscription to the retrieval of spending limit reports (see also 3GPP TS 23.502 [3], figure 4.16.8.3.1). The NF service consumer can add or remove policy counters to retrieve the status of the counters.



Figure 4.2.2.3-1: NF service consumer modifies the subscription to retrieve policy counter status and spending limit reporting

The NF service consumer shall send an HTTP PUT request to the resource "{apiRoot}/nchf-spendinglimitcontrol/v1/subscriptions/{subscriptionId}" representing an existing "Individual Spending Limit Subscription" resource, as shown in figure 4.2.2.3-1, step 1, to modify the subscription for retrieval of the policy counter status and spending limit reporting.

The "SpendingLimitContext" data structure provided in the request body:

- shall include the Subscription Permanent Identifier (SUPI) encoded in the "supi" attribute;

- shall include the notification correlation target address encoded in the "notifUri" attribute;

- if the feature "NotificationCorrelation" is supported, a Notification Correlation Identifier assigned by the NF service consumer for the requested notifications encoded in the "notifId" attribute, if the "notifUri" does not encode within the provided URI the notification correlation Id.

NOTE 1: If the notification correlation target address is not changed the previously provided notification correlation target address is included in the "notifUri" attribute. If the Notification Correlation Id is not changed the previously provided Notification Correlation Id is included in the "notifId" attribute.

- if the General Public Subscription Identifier (GPSI) was provided within the initial spending limit retrieval procedure, described in clause 4.2.2.2, shall include the GPSI encoded in the "gpsi" attribute; and

- may include Event Filter information as a "list of policy counter identifier(s)" encoded in the "policyCounterIds" attribute. The "policyCounterIds" attribute shall contain the updated list of policy counter identifiers to be subscribed to. If the "policyCounterIds" attribute is omitted, the subscription is updated to all available policy counters; and

- when the feature "SubscriptionExpirationTimeControl" is supported, may include an updated expiry time encoded in the "expiry" attribute to update the duration of the subscription, representing the updated time up to which the subscription is desired to be kept active. When the "expiry" attribute is omitted in the request, it represents the NF service consumer update does not have any time constraint from this moment on in the duration of the subscription.

NOTE 2: The "notifUri" attribute within the SpendingLimitContext data structure can be modified to request that subsequent notifications are sent to a new NF service consumer.

When the "policyCounterIds" attribute is present in the subscription request, this list of policy counters overrides a previously provisioned list.

After the CHF modified an "Individual Spending Limit Retrieval Subscription" resource, the CHF shall respond with "200 OK" response with the message body containing a representation of the modified subscription, as shown in figure 4.2.2.3-1, step 2.

The SpendingLimitStatus data structure provided in the response body, when the feature "SubscriptionExpirationTimeControl" is not supported, shall include the status of the requested subscribed policy counters in the "statusInfos" map, where every PolicyCounterInfo entry shall contain:

- the policy counter identifier in the "policyCounterId" attribute; and

- the policy counter status in the "currentStatus" attribute.

When a requested policy counter identifier is known by the CHF, but it is not applicable to the subscriber (e.g. not provisioned), the CHF may include it in the "statusInfos" map, and set the "currentStatus" attribute to an operator configured policy counter status to indicate this to the NF service consumer.

When one or more policy counters specified in the request in the "policyCounterIds" attribute are unknown to the CHF, and the CHF is configured to accept the request, the CHF may include the unknown policy counters in the "statusInfos" map, and set the "currentStatus" attribute to an operator configured policy counter status to indicate this to the NF service consumer.

A PolicyCounterInfo data structure may include the list of the pending policy counter statuses and their activation times within the attribute "penPolCounterStatuses".

When the feature "SubscriptionExpirationTimeControl" is supported, the CHF may include the "expiry" attribute, representing the time up to which the subscription shall be kept active. If an expiry time was included in the subscription update request, then the expiry time shall be returned in the response, and the value returned should be less than or equal to the value in the request. When the "expiry" attribute is omitted in the request and in the response, it represents that the subscription shall be considered valid without an expiry time.

NOTE 3: When the NF service consumer does not include an expiry time in the request, the CHF can include an expiry time in the response that represents an update of the previously provided duration of the subscription.

NOTE 4: Once the subscription expires, if the NF service consumer wants to keep receiving notifications, it needs to create a new subscription in the CHF, as specified in clause 4.2.2.2.

If errors occur when processing the HTTP PUT request, the CHF shall send an HTTP error response as specified in clause 5.7.

If the feature "ES3XX" is supported, and the CHF determines the received HTTP PUT request needs to be redirected, the CHF shall send an HTTP redirect response as specified in clause 6.10.9 of 3GPP TS 29.500 [4].

If the CHF has no available policy counters specified for the subscriber, the CHF shall indicate in an HTTP "400 Bad Request" response the cause for the rejection with the "cause" attribute set to "NO\_AVAILABLE\_POLICY\_COUNTERS ".

If one or more policy counters specified in the PUT request in the "policyCounterIds" attribute are unknown to the CHF, and the CHF is configured to reject request, the CHF shall indicate in an HTTP "400 Bad Request" response the cause for the rejection with the "cause" attribute set to "UNKNOWN\_POLICY\_COUNTERS" and the unknown policy counter identifiers within the "invalidParams" attribute. The PUT request shall not take effect, and the CHF shall maintain the Individual Spending Limit Retrieval resource.

NOTE 5: In order to avoid misbehaviors due to the policy counters status maintained in the CHF and the NF service consumer, the NF service consumer can terminate the subscription invoking the Nchf\_SpendingLimitControl\_Unsubscribe service operation in clause 4.2.3.2.

NOTE 6: The NF service consumer can terminate the subscription invoking the Nchf\_SpendingLimitControl\_Unsubscribe service operation in clause 4.2.3.2, or maintain subscription assuming that further available policy counters will be notified.

### 4.2.3 Nchf\_SpendingLimitControl\_Unsubscribe service operation

#### 4.2.3.1 General

The Nchf\_SpendingLimitControl\_Unsubscribe service operation is used by the NF service consumer to cancel the subscription of status changes for all the policy counters available at the CHF. That means the complete cancellation of the spending limit reporting procedure.

#### 4.2.3.2 Unsubscribe from spending limit reporting

Figure 4.2.3.2-1 shows the scenario where the NF service consumer sends a request to the CHF to unsubscribe from spending limit reporting (see also 3GPP TS 23.502 [3] figure 4.16.8.4.1).



Figure 4.2.3.2-1: NF service consumer unsubscribes from spending limit reporting

The NF service consumer shall invoke the Nchf\_SpendingLimitControl\_Unsubscribe service operation to unsubscribe from the spending limit reporting (status change for all policy counters available is no more required). The NF service consumer shall send an HTTP DELETE request to the resource "{apiRoot}/nchf-spendinglimitcontrol/v1/subscriptions/{subscriptionId}", whereby the "{subscriptionId}" is the identification of the existing subscription to be deleted. Upon the reception of an HTTP DELETE request the CHF removes the corresponding subscription.

If the HTTP DELETE request is accepted by the CHF, it shall respond with "204 No Content" as shown in figure 4.2.3.2-1, step 2.

If the HTTP DELETE request is not accepted by the CHF (e.g. the HTTP DELETE request is for a non-existent subscription), it shall indicate the appropriate cause for the rejection in the HTTP response code or, if the feature "ES3XX" is supported, an HTTP redirect response to the NF service consumer.

### 4.2.4 Nchf\_SpendingLimitControl\_Notify service operation

#### 4.2.4.1 General

The Nchf\_SpendingLimitControl\_Notify service operation is used by the CHF:

- to notify the change of the status of the subscribed policy counters available at the CHF for that subscriber; and/or

- to provide one or more pending statuses for a subscribed policy counter together with the time they shall be applied; and/or

- to request the termination of the subscription of status changes for all policy counters for a subscriber (e.g. the subscriber is removed from the CHF system).

#### 4.2.4.2 Spending limit report

Figure 4.2.4.2-1 shows the scenario where the CHF sends a notification to the NF service consumer, when it detects that the status of a policy counter(s) has changed and the NF service consumer has subscribed to notifications of changes in the status of this policy counter(s). The CHF can also notify the NF service consumer that the status for one or multiple subscribed policy counter will change and indicate this by providing the time when this change shall be applied (see also 3GPP TS 23.502 [3], figure 4.16.8.5.1).



Figure 4.2.4.2-1: Spending limit reporting

The CHF shall send an HTTP POST request to the resource notification target address (notifUri) of the NF service consumer received in the subscription creation or modification, and shall append the "notify" segment path at the end of the URI, to indicate the NF service consumer the notification of a policy counter status change.

The SpendingLimitStatus data structure provided in the request body:

- shall include the Subscriber Identity in the "supi" attribute;

- shall include, if the feature "NotificationCorrelation" is supported, the notification correlation ID in the "notifId" attribute if received in the SpendingLimitContext data structure provided in the creation or update of the subscription;

- shall include, when the feature "SubscriptionExpirationTimeControl" is not supported, Policy counters status in the "statusInfos" map, where every PolicyCounterInfo entry shall include:

a. the "policyCounterId" attribute with the policy counter identifier; and

b. the "currentStatus" attribute with the new policy counter status when the notification is triggered by a change in the policy counter status, or the current policy counter status when the notification is triggered by a change in the pending policy counter status(es); and

- may include, when the feature "SubscriptionExpirationTimeControl" is supported, the Policy counters status in the "statusInfos" map if at this time there is change of policy counter status and/or the update of the expiry time in the "expiry".

NOTE 1: When the feature "SubscriptionExpirationTimeControl" is supported, and the CHF includes the update of the expiry time, if at this time there is no change of policy counter status, the CHF does not include the "statusInfos" attribute.

When a policy counter identifier is no longer applicable to the subscriber (e.g. becomes not provisioned), but still exists in the Individual Spending Control Retrieval resource, the CHF may include it in the "statusInfos" map, and set the "currentStatus" attribute to an operator configured policy counter status to indicate this to the NF service consumer.

A PolicyCounterInfo data structure may include the list of pending policy counter statuses and their activation times within the attribute "penPolCounterStatuses.

When the feature "SubscriptionExpirationTimeControl" is supported, the CHF may include the "expiry" attribute, representing an update in the time up to which the subscription shall be kept active. When the "expiry" attribute is omitted, it represents that the previously agreed duration of the subscription remains valid.

NOTE 2: Once the subscription expires, if the NF Service Consumer wants to keep receiving notifications, it needs to create a new subscription in the CHF, as specified in clause 4.2.2.2.

The CHF shall not send the policy counter status for the same policy counter until it received the response of the previous status report of the policy counter.

If the HTTP POST notification request message is accepted by the NF service consumer, it shall acknowledge the receipt of the event notification with a "204 No Content" response, as shown in figure 4.2.4.2-1, step 2.

If errors occur when processing the HTTP POST request, the NF service consumer shall send an HTTP error response as specified in clause 5.7.

If the feature "ES3XX" is supported, and the NF service consumer determines the received HTTP POST request needs to be redirected, the NF service consumer shall send an HTTP redirect response as specified in clause 6.10.9 of 3GPP TS 29.500 [4].

If the NF service consumer receives an HTTP POST notification request message for an intermediate spending limit report transaction from the CHF in which no pending policy counter statuses and their activation times are included for a policy counter, i.e., the "penPolCounterStatuses" attribute is not included, the NF service consumer shall cancel all previously provided pending policy counter statuses and their activation times for this policy counter. If the NF service consumer receives an HTTP POST notification request message for an intermediate spending limit report transaction from the CHF containing pending policy counter statuses and their activation times for a previously provided policy counter, the NF service consumer shall replace the existing pending policy counter statuses and their activation times if any.

If the NF service consumer receives an HTTP POST request for spending limit report initiated by the CHF while it has an ongoing intermediate spending limit report retrieval transaction with the CHF, the NF service consumer shall update the policy counter information based on the HTTP POST request for spending limit report. When the corresponding response for the ongoing intermediate spending limit report retrieval transaction is eventually received, the NF service consumer shall only update policy counter information for counters that were not provided in the previously received HTTP POST request for spending limit report.

#### 4.2.4.3 Subscription termination request by CHF

Figure 4.2.4.3-1 shows the scenario where the CHF sends a notification to the NF service consumer, when it requests the termination of the subscription of status changes for all policy counters for a subscriber.



Figure 4.2.4.3-1: Subscription termination request by CHF

The CHF shall send an HTTP POST request to the resource notification target address (notifUri) of the NF service consumer received in the subscription creation or modification and shall append the "terminate" segment path at the end of the URI, to indicate the subscription termination and the removal of the Individual Spending Limit Retrieval Subscription resource to the NF service consumer.

The SubscriptionTerminationInfo data structure provided in the request body shall include the subscriber identification encoded in the "supi" attribute, if the feature "NotificationCorrelation" is supported, the Notification Correlation Id in the "notifId" attribute if received and may include subscription termination information in the "termCause" attribute.

When the termination request is because the subscriber identified by the SUPI has been removed from the CHF, the CHF shall set the "termCause" attribute to "REMOVED\_SUBSCRIBER".

If the HTTP POST notification request message is accepted by the NF service consumer, it shall remove the subscription to notifications of all policy counters for a subscriber and shall acknowledge the receipt of the event notification with a "204 No Content" response, as shown in figure 4.2.4.3-1, step 2.

If errors occur when processing the HTTP POST request, the NF service consumer shall send an HTTP error response as specified in clause 5.7.

If the feature "ES3XX" is supported, and the NF service consumer determines the received HTTP POST request needs to be redirected, the NF service consumer shall send an HTTP redirect response as specified in clause 6.10.9 of 3GPP TS 29.500 [4].

# 5 Nchf\_SpendingLimitControl Service API

## 5.1 Introduction

The Nchf\_SpendingLimitControl service shall use the Nchf\_SpendingLimitControl API.

The API URI of the Nchf\_SpendingLimitControl API shall be:

**{apiRoot}/<apiName>/<apiVersion>**

The request URIs used in HTTP requests from the NF service consumer towards the CHF shall have the Resource URI structure defined in clause 4.4.1 of 3GPP TS 29.501 [5], i.e.:

**{apiRoot}/<apiName>/<apiVersion>/<apiSpecificResourceUriPart>**

with the following components:

- The {apiRoot} shall be set as described in 3GPP TS29.501 [5].

- The **<**apiName**>** shall be "nchf-spendinglimitcontrol".

- The **<**apiVersion**>** shall be "v1".

- The **<**apiSpecificResourceUriPart**>** shall be set as described in clause 5.3.

## 5.2 Usage of HTTP

### 5.2.1 General

HTTP/2, IETF RFC 7540 [8], shall be used as specified in clause 5.2 of 3GPP TS 29.500 [4].

HTTP/2 shall be transported as specified in clause 5.3 of 3GPP TS 29.500 [4].

The OpenAPI [9] specification of HTTP messages and content bodies for the Nchf\_SpendingLimitControl service is contained in Annex A.

### 5.2.2 HTTP standard headers

#### 5.2.2.1 General

See clause 5.2.2 of 3GPP TS 29.500 [4] for the usage of HTTP standard headers.

#### 5.2.2.2 Content type

JSON, IETF RFC 8259 [10], shall be used as content type of the HTTP bodies specified in the present specification, as specified in clause 5.4 of 3GPP TS 29.500 [4]. The use of the JSON format shall be signalled by the content type "application/json".

"Problem Details" JSON object shall be used to indicate additional details of the error in a HTTP response body and shall be signalled by the content type "application/problem+json", as defined in IETF RFC 9457 [13].

### 5.2.3 HTTP custom headers

#### 5.2.3.1 General

The Nchf\_SpendingLimitControl API shall support HTTP custom header fields specified in clause 5.2.3.2 of 3GPP TS 29.500 [4] and may support HTTP custom header fields specified in clause 5.2.3.3 of 3GPP TS 29.500 [4].

In this Release of the specification, no specific custom headers are defined for the Nchf\_SpendingLimitControl API.

## 5.3 Resources

### 5.3.1 Resource Structure

This clause describes the structure for the Resource URIs and the resources and methods used for the service.

Figure 5.3.1-1 shows the resource URI structure of the Nchf\_SpendingLimitControl API.



Figure 5.3.1-1: Resource URI structure of the Nchf\_SpendingLimitControl API

Table 5.3.1-1 provides an overview of the resources and applicable HTTP methods.

Table 5.3.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method or custom operation | Description |
| Spending Limit Retrieval Subscriptions | /subscriptions | POST | Creates a new individual spending limit retrieval subscription. |
| Individual Spending Limit Retrieval Subscription | /subscriptions/{subscriptionId} | PUT | Modifies an existing subscription (e.g. addition of additional policy counters). |
| DELETE | Deletes an individual subscription. |

### 5.3.2 Resource: Spending Limit Retrieval Subscriptions (Collection)

#### 5.3.2.1 Description

This resource represents the collection of Nchf\_SpendingLimitControl service subscriptions at a given CHF.

#### 5.3.2.2 Resource definition

Resource URI: **{apiRoot}/nchf-spendinglimitcontrol/v1/subscriptions**

This resource shall support the resource URI variables defined in table 5.3.2.2-1.

Table 5.3.2.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 5.1 |

#### 5.3.2.3 Resource Standard Methods

##### 5.3.2.3.1 POST

This method shall support the URI query parameters specified in table 5.3.2.3.1-1.

Table 5.3.2.3.1-1: URI query parameters supported by the POST method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| n/a |  |  |  |  |

This method shall support the request data structures specified in table 5.3.2.3.1-2 and the response data structures and response codes specified in table 5.3.2.3.1-3.

Table 5.3.2.3.1-2: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| SpendingLimitContext | M | 1 | Contains the information for the creation of a new individual spending limit retrieval subscription. |

Table 5.3.2.3.1-3: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response codes | Description |
| SpendingLimitStatus | M | 1 | 201 Created | The spending limit subscription was created and spending limit reports are provided. |
| ProblemDetails | O | 0..1 | 400 Bad Request | (NOTE 2) |
| NOTE 1: In addition, the HTTP status codes which are specified as mandatory in table 5.2.7.1-1 of 3GPP TS 29.500 [4] for the POST method shall also apply.  NOTE 2: In addition to protocol and application errors which are specified in clause 5.2.7.2 of 3GPP TS 29.500 [4], specific errors are described in clause 5.7. | | | | |

Table 5.3.2.3.1-4: Headers supported by the 201 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains the URI of the newly created resource, according to the structure: {apiRoot}/nchf-spendinglimitcontrol/v1/subscriptions/{subscriptionId} |

#### 5.3.2.4 Resource Custom Operations

None.

### 5.3.3 Resource: Individual Spending Limit Retrieval Subscription (Document)

#### 5.3.3.1 Description

This resource represents an individual Nchf\_SpendingLimitControl service subscription at a given CHF.

#### 5.3.3.2 Resource definition

Resource URI: **{apiRoot}/nchf-spendinglimitcontrol/v1/subscriptions/{subscriptionId}**

This resource shall support the resource URI variables defined in table 5.3.3.2-1.

Table 5.3.3.2-1: Resource URI variables for this resource

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| apiRoot | string | See clause 5.1 |
| subscriptionId | string | Identifies a subscription to the CHF spending limit control retrieval service. |

#### 5.3.3.3 Resource Standard Methods

##### 5.3.3.3.1 PUT

This method shall support the URI query parameters specified in table 5.3.3.3.1-1.

Table 5.3.3.3.1-1: URI query parameters supported by the PUT method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| n/a |  |  |  |  |

This method shall support the request data structures specified in table 5.3.3.3.1-2 and the response data structures and response codes specified in table 5.3.3.3.1-3.

Table 5.3.3.3.1-2: Data structures supported by the PUT Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| SpendingLimitContext | M | 1 | Modifies the existing individual spending limit retrieval subscription. |

Table 5.3.3.3.1-3: Data structures supported by the PUT Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response codes | Description |
| SpendingLimitStatus | M | 1 | 200 OK | Successful case: The individual spending limit subscription was modified and spending limit reports are provided. |
| RedirectResponse | O | 0..1 | 307 Temporary Redirect | Temporary redirection, during Individual Spending Limit Retrieval Subscription modification.  Applicable if the feature "ES3XX" is supported.  (NOTE 3) |
| RedirectResponse | O | 0..1 | 308 Permanent Redirect | Permanent redirection, during Individual Spending Limit Retrieval Subscription modification.  Applicable if the feature "ES3XX" is supported.  (NOTE 3) |
| ProblemDetails | O | 0..1 | 400 Bad Request | (NOTE 2) |
| NOTE 1: In addition, the HTTP status codes which are specified as mandatory in table 5.2.7.1-1 of 3GPP TS 29.500 [4] for the PUT method shall also apply.  NOTE 2: In addition to protocol and application errors which are specified in clause 5.2.7.2 of 3GPP TS 29.500 [4], specific errors are described in clause 5.7.  NOTE 3: The RedirectResponse data structure may be provided by an SCP (refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]). | | | | |

Table 5.3.3.3.1-4: Headers supported by the 307 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI of the resource located in an alternative CHF (service) instance towards which the request is redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target CHF (service) instance towards which the request is redirected. |

Table 5.3.3.3.1-5: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI of the resource located in an alternative CHF (service) instance instance towards which the request is redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target CHF (service) instance towards which the request is redirected. |

##### 5.3.3.3.2 DELETE

This method shall support the URI query parameters specified in table 5.3.3.3.2-1.

Table 5.3.3.3.3-1: URI query parameters supported by the DELETE method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| n/a |  |  |  |  |

This method shall support the request data structures specified in table 5.3.3.3.2-2 and the response data structures and response codes specified in table 5.3.3.3.2-3.

Table 5.3.3.3.2-2: Data structures supported by the DELETE Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| n/a |  |  |  |

Table 5.3.3.3.2-3: Data structures supported by the DELETE Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response codes | Description |
| n/a |  |  | 204 No Content | Successful case: The individual spending limit subscription matching the subscriptionId was deleted. |
| RedirectResponse | O | 0..1 | 307 Temporary Redirect | Temporary redirection, during Individual Spending Limit Retrieval Subscription deletion.  Applicable if the feature "ES3XX" is supported.  (NOTE 2) |
| RedirectResponse | O | 0..1 | 308 Permanent Redirect | Permanent redirection, during Individual Spending Limit Retrieval Subscription deletion.  Applicable if the feature "ES3XX" is supported.  (NOTE 2) |
| NOTE 1: In addition, the HTTP status codes which are specified as mandatory in table 5.2.7.1-1 of 3GPP TS 29.500 [4] for the DELETE method shall also apply.  NOTE 2: The RedirectResponse data structure may be provided by an SCP (refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]). | | | | |

Table 5.3.3.3.2-4: Headers supported by the 307 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI of the resource located in an alternative CHF (service) instance instance towards which the request is redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target CHF (service) instance towards which the request is redirected. |

Table 5.3.3.3.2-5: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI of the resource located in an alternative CHF (service) instance instance towards which the request is redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target CHF (service) instance towards which the request is redirected. |

## 5.4 Custom Operations without associated resources

None.

## 5.5 Notifications

### 5.5.1 General

Notification shall comply with clause 6.2 of 3GPP TS 29.500 [4] and clause 4.6.2.3 of 3GPP TS 29.501 [5].

Table 5.5.1-1: Notifications overview

|  |  |  |  |
| --- | --- | --- | --- |
| Notification | Callback URI | HTTP method or custom operation | Description (service operation) |
| Spending limit notification | {notifUri}/notify | notify (POST) | Counter Status changes notification. |
| Subscription Termination | {notifUri}/terminate | terminate (POST) | Indication of subscription termination. |

### 5.5.2 Spending limit notification

#### 5.5.2.1 Description

The spending limit notification is used by the CHF to notify the change of the status of the subscribed policy counters for a subscriber and/or to provide one or more pending statuses for a subscribed policy counter together with the time they shall be applied.

#### 5.5.2.2 Target URI

The Callback URI **{notifUri}/notify** shall be used with the callback URI variables defined in table 5.5.2.2-1.

Table 5.5.2.2-1: Callback URI variables

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| notifUri | Uri | The Notification Uri as assigned by the NF service consumer during the subscription service operation and described within the SpendingLimitContext data type (see table 5.6.2.2-1). |

#### 5.5.2.3 Standard Methods

##### 5.5.2.3.1 POST

This method shall support the URI query parameters specified in table 5.5.2.3.1-1.

Table 5.5.2.3.1-1: URI query parameters supported by the POST method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| n/a |  |  |  |  |

This method shall support the request data structures specified in table 5.5.2.3.1-2 and the response data structures and response codes specified in table 5.5.2.3.1-3.

Table 5.5.2.3.1-2: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| SpendingLimitStatus | M | 1 | Provides information about the statuses of policy counters. |

Table 5.5.2.3.1-3: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response codes | Description |
| n/a |  |  | 204 No Content | The receipt of the notification is acknowledged. |
| RedirectResponse | O | 0..1 | 307 Temporary Redirect | Temporary redirection, during Spending limit report.  Applicable if the feature "ES3XX" is supported.  (NOTE 2) |
| RedirectResponse | O | 0..1 | 308 Permanent Redirect | Permanent redirection, during Spending limit report.  Applicable if the feature "ES3XX" is supported.  (NOTE 2) |
| NOTE 1: In addition, the HTTP status codes which are specified as mandatory in table 5.2.7.1-1 of 3GPP TS 29.500 [4] for the POST method shall also apply.  NOTE 2: The RedirectResponse data structure may be provided by an SCP (refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]). | | | | |

Table 5.3.3.3.2-4: Headers supported by the 307 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contians an alternative URI representing the end point of an alternative NF consumer (service) instance towards which the notification should be redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target NF (service) instance towards which the notification request is redirected. |

Table 5.3.3.3.2-5: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI representing the end point of an alternative NF consumer (service) instance towards which the notification should be redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target NF (service) instance towards which the notification request is redirected. |

### 5.5.3 Subscription Termination

#### 5.5.3.1 Description

The Subscription Termination request is used by the CHF to request the NF service consumer the termination of the subscription to policy counter status changes.

#### 5.5.3.2 Target URI

The Callback URI **{notifUri}/terminate** shall be used with the callback URI variables defined in table 5.5.3.2-1.

Table 5.5.3.2-1: Callback URI variables

|  |  |  |
| --- | --- | --- |
| Name | Data type | Definition |
| notifUri | Uri | The Notification Uri as assigned by the NF service consumer during the subscription service operation and described within the SpendingLimitContext data type (see table 5.6.2.2-1). |

#### 5.5.3.3 Standard Methods

##### 5.5.3.3.1 POST

This method shall support the URI query parameters specified in table 5.5.3.3.1-1.

Table 5.5.3.3.1-1: URI query parameters supported by the POST method on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| n/a |  |  |  |  |

This method shall support the request data structures specified in table 5.5.3.3.1-2 and the response data structures and response codes specified in table 5.5.3.3.1-3.

Table 5.5.3.3.1-2: Data structures supported by the POST Request Body on this resource

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | P | Cardinality | Description |
| SubscriptionTerminationInfo | M | 1 | Provides information about the deletion of the resource. |

Table 5.5.3.3.1-3: Data structures supported by the POST Response Body on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Data type | P | Cardinality | Response codes | Description |
| n/a |  |  | 204 No Content | The receipt of the Notification is acknowledged. |
| RedirectResponse | O | 0..1 | 307 Temporary Redirect | Temporary redirection, during subscription termination.  Applicable if the feature "ES3XX" is supported.  (NOTE 2) |
| RedirectResponse | O | 0..1 | 308 Permanent Redirect | Permanent redirection, during subscription termination.  Applicable if the feature "ES3XX" is supported.  (NOTE 2) |
| NOTE 1: In addition, the HTTP status codes which are specified as mandatory in table 5.2.7.1-1 of 3GPP TS 29.500 [4] for the POST method shall also apply.  NOTE 2: The RedirectResponse data structure may be provided by an SCP (refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]). | | | | |

Table 5.5.3.3.1-4: Headers supported by the 307 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contians an alternative URI representing the end point of an alternative NF consumer (service) instance towards which the notification should be redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target NF (service) instance towards which the notification request is redirected. |

Table 5.5.3.3.1-5: Headers supported by the 308 Response Code on this resource

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Name | Data type | P | Cardinality | Description |
| Location | string | M | 1 | Contains an alternative URI representing the end point of an alternative NF consumer (service) instance towards which the notification should be redirected.  For the case where the request is redirected to the same target via a different SCP, refer to clause 6.10.9.1 of 3GPP TS 29.500 [4]. |
| 3gpp-Sbi-Target-Nf-Id | string | O | 0..1 | Identifier of the target NF (service) instance towards which the notification request is redirected. |

## 5.6 Data Model

### 5.6.1 General

This clause specifies the application data model supported by the API.

Table 5.6.1-1 specifies the data types defined for the Nchf\_SpendingLimitControl service based interface protocol.

Table 5.6.1-1: Nchf\_SpendingLimitControl specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Section defined | Description | Applicability |
| SpendingLimitContext | 5.6.2.2 | Describes the subscription data structure required for an individual CHF spending limit subscription. |  |
| SpendingLimitStatus | 5.6.2.3 | Describes the data structure presenting the statuses of policy counters. |  |
| PolicyCounterInfo | 5.6.2.4 | Describes the data structure presenting the policy counter status. |  |
| PendingPolicyCounterStatus | 5.6.2.5 | Describes the data structure presenting the pending policy counter status. |  |
| PolicyCounterId | 5.6.3.2 | Identifies a policy counter. |  |
| SubscriptionTerminationInfo | 5.6.2.6 | Describes the data structure presenting the indication of the termination of the subscription. |  |
| TerminationCause | 5.6.3.3 | Represents the types of causes for requesting the termination of the subscription. |  |

Table 5.6.1-2 specifies data types re-used by the Nchf\_SpendingLimitControl service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nchf\_SpendingLimitControl service based interface.

Table 5.6.1-2: Nchf\_SpendingLimitControl re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| DateTime | 3GPP TS 29.571 [11] | String with format "date-time" as defined in OpenAPI Specification [9]. |  |
| Uri | 3GPP TS 29.571 [11] |  |  |
| Supi | 3GPP TS 29.571 [11] |  |  |
| Gpsi | 3GPP TS 29.571 [11] |  |  |
| RedirectResponse | 3GPP TS 29.571 [11] | Contains redirection related information. | ES3XX |
| SupportedFeatures | 3GPP TS 29.571 [11] | Used to negotiate the applicability of the optional features defined in table 5.8-1. |  |

### 5.6.2 Structured data types

#### 5.6.2.1 Introduction

This clause defines the structures to be used in resource representations.

#### 5.6.2.2 Type SpendingLimitContext

Table 5.6.2.2-1: Definition of type SpendingLimitContext

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Attribute name | | Data type | | | P | Cardinality | | Description | | Applicability | |
| supi | | Supi | | | C | 0..1 | | The Subscription Permanent Identifier (Supi) shall be present within the initial spending limit retrieval procedure (creation of a new individual subscription) and intermediate spending limit retrieval procedure (modification of an existing subscription). | |  | |
| gpsi | | Gpsi | | | O | 0..1 | | The Generic Public Subscription Identifier (Gpsi) shall contain either an External Id or an MSISDN. It may be present within the initial spending limit retrieval procedure (creation of a new individual subscription) and intermediate spending limit retrieval procedure (modification of an existing subscription). | |  | |
| policyCounterIds | | array(PolicyCounterId) | | | O | 1..N | | This is a list of policy counter identifier(s), which identifies policy counters maintained per subscriber within the CHF. | |  | |
| notifUri | | Uri | | | C | 0..1 | | This attribute identifies the recipient of spending limit notifications sent to the NF service consumer by the CHF. The notifUri shall be present within the initial spending limit retrieval procedure (creation of a new individual subscription and within the intermediate spending limit retrieval procedure (modification of an existing subscription). | |  | |
| notifId | | string | | C | 0..1 | | | Notification Correlation ID assigned by the NF service consumer. It shall be included if the NotificationCorrelation feature is supported, the notifUri does not encode the notification correlation Id, and the NF service consumers require multiple subscriptions for the same SUPI, e.g. UE accesses multiple network slices. | | NotificationCorrelation | |
| expiry | | DateTime | | | O | 0..1 | | The expiry time may be included in a subscription request. When present, this IE shall represent the longest duration time after which the subscription shall become invalid. | | SubscriptionExpirationTimeControl | |
| supportedFeatures | | SupportedFeatures | | | C | 0..1 | | The list of supported features as described in clause 5.8 shall be supplied by the NF service consumer in the POST request that request the creation of a spending limit report resource and intermediate spending limit retrieval procedure (modification of an existing subscription). | |  | |

#### 5.6.2.3 Type SpendingLimitStatus

Table 5.6.2.3-1: Definition of type SpendingLimitStatus

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Attribute name | | Data type | | | P | Cardinality | | Description | | Applicability | |
| supi | | Supi | | | O | 0..1 | | The Subscription Permanent Identifier (Supi) shall be present within the callback notify service operation (notification of the status of subscribed policy counters). | |  | |
| notifId | | string | | C | 0..1 | | | Notification Correlation ID assigned by the NF service consumer. It shall be included if provided during the subscription within the SpendingLimitContext data type. | | NotificationCorrelation | |
| statusInfos | | map(PolicyCounterInfo) | | | C | 1..N | | Status of the requested policy counters. The key of the map is the attribute "policyCounterId".  It may be omitted when the feature SubscriptionExpirationTimeControl is supported and the CHF only requires to update the "expiry" attribute. | |  | |
| expiry | | DateTime | | | C | 0..1 | | This expiry time shall be included in a subscription response, if the expiry time was included in the request.  It may be included in a subscription response and notification request based on operator policies for the control in the CHF of the subscription duration. | | SubscriptionExpirationTimeControl | |
| supportedFeatures | | SupportedFeatures | | | C | 0..1 | | If the supportedFeatures is included in the request by the NF service consumer, it shall be supplied in the reply of the corresponding request by the CHF. | |  | |

#### 5.6.2.4 Type PolicyCounterInfo

Table 5.6.2.4-1: Definition of type PolicyCounterInfo

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| policyCounterId | PolicyCounterId | M | 1 | Identifies the requested policy counter. |  |
| currentStatus | string | M | 1 | Identifies the policy counter status applicable for a specific policy counter identified by the policyCounterId. The values (e.g. valid, invalid or any other status) are not specified. The interpretation and actions related to the defined values are out of scope of 3GPP. |  |
| penPolCounterStatuses | array(PendingPolicyCounterStatus) | O | 1..N | Provides the pending policy counter status. |  |

#### 5.6.2.5 Type PendingPolicyCounterStatus

Table 5.6.2.5-1: Definition of type PendingPolicyCounterStatus

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| policyCounterStatus | string | M | 1 | Identifies the policy counter status applicable for a specific policy counter identified by the PolicyCounterId. The values (e.g. valid, invalid or any other status) are not specified. The interpretation and actions related to the defined values are out of scope of 3GPP. |  |
| activationTime | DateTime | M | 1 | Indicates the time at which the pending policy counter status becomes the current status of a policy counter. |  |

#### 5.6.2.6 Type SubscriptionTerminationInfo

Table 5.6.2.6-1: Definition of type SubscriptionTerminationInfo

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| supi | Supi | M | 1 | Subscription Permanent Identifier. |  |
| notifId | string | C | 0..1 | Notification Correlation ID assigned by the NF service consumer. It shall be included if provided during the subscription within the SpendingLimitContext data type. | NotificationCorrelation |
| termCause | TerminationCause | O | 0..1 | Indicates the cause for requesting the termination of the subscription to policy counter status changes. |  |

### 5.6.3 Simple data types and enumerations

#### 5.6.3.1 Introduction

This clause defines simple data types and enumerations that can be referenced from data structures defined in the previous clauses.

#### 5.6.3.2 Simple data types

The simple data types defined in table 5.6.3.2-1 shall be supported.

Table 5.6.3.2-1: Simple data types

|  |  |  |  |
| --- | --- | --- | --- |
| Type Name | Type Definition | Description | Applicability |
| PolicyCounterId | string | Identifies a policy counter. |  |

#### 5.6.3.3 Enumeration: TerminationCause

The enumeration "TerminationCause" represents the types of causes the CHF can report when requesting the termination of the subscription.

Table 5.6.3.3-1: Enumeration TerminationCause

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| REMOVED\_SUBSCRIBER | The subscriber identified by the SUPI has been removed from the CHF. |  |

## 5.7 Error handling

### 5.7.1 General

HTTP error handling shall be supported as specified in clause 5.2.4 of 3GPP TS 29.500 [4].

For the Nchf\_SpendingLimitControl service API, HTTP error responses shall be supported as specified in clause 4.8 of 3GPP TS 29.501 [5].

Protocol errors and application errors specified in table 5.2.7.2-1 of 3GPP TS 29.500 [4] shall be supported for an HTTP method if the corresponding HTTP status codes are specified as mandatory for that HTTP method in table 5.2.7.1-1 of 3GPP TS 29.500 [4].

In addition, the requirements in the following clauses shall apply.

### 5.7.2 Protocol Errors

In this Release of the specification, there are no additional protocol errors applicable for the Nchf\_SpendingLimitControl service API.

### 5.7.3 Application Errors

The application errors defined for the Nchf\_SpendingLimitControl service API are listed in table 5.7.3-1.

Table 5.7.3-1: Application errors

|  |  |  |
| --- | --- | --- |
| Application Error | HTTP status code | Description |
| USER\_UNKNOWN | 400 Bad Request | The subscriber specified in the request is not known at the CHF and the subscription cannot be created. |
| NO\_AVAILABLE\_POLICY\_COUNTERS | 400 Bad Request | There are no policy counters available for the subscriber at the CHF |
| UNKNOWN\_POLICY\_COUNTERS | 400 Bad Request | The policy counter identifiers in the request are not known at the CHF. |
| NOTE: Including a "ProblemDetails" data structure with the "cause" attribute in the HTTP response is optional unless explicitly mandated in the service operation clauses. | | |

## 5.8 Feature negotiation

The optional features in table 5.8-1 are defined for the Nchf\_SpendingLimitControl Service API. They shall be negotiated using the extensibility mechanism defined in clause 6.6.2 of 3GPP TS 29.500 [4].

Table 5.8-1: Supported Features

|  |  |  |
| --- | --- | --- |
| Feature number | Feature Name | Description |
| 1 | SubscriptionExpirationTimeControl | Indicates the support of a expiry time to control the time duration of the subscription to changes of policy counters status. |
| 2 | NotifiationCorrelation | Indicates the support of the explicit indication of the notification correlation id |
| 3 | ES3XX | Extended Support for 3xx redirections. This feature indicates the support of redirection for any service operation, according to Stateless NF procedures as specified in clauses 6.5.3.2 and 6.5.3.3 of 3GPP TS 29.500 [4] and according to HTTP redirection principles for indirect communication, as specified in clause 6.10.9 of 3GPP TS 29.500 [4]. |

## 5.9 Security

As indicated in 3GPP TS 33.501 [14] and 3GPP TS 29.500 [4], the access to the Nchf\_SpendingLimitControl API, based on local configuration, may be authorized by means of the OAuth2 protocol (see IETF RFC 6749 [15]), using the "Client Credentials" authorization grant, where the NRF (see 3GPP TS 29.510 [16]) plays the role of the authorization server.

If OAuth2 is used, an NF service consumer, prior to consuming services offered by the Nchf\_SpendingLimitControl API, shall obtain a "token" from the authorization server, by invoking the Access Token Request service, as described in 3GPP TS 29.510 [16], clause 5.4.2.2.

NOTE: When multiple NRFs are deployed in a network, the NRF used as authorization server is the same NRF that the NF service consumer used for discovering the Nchf\_SpendingLimitControl service.

The Nchf\_SpendingLimitControl API defines a single scope "nchf-spendinglimitcontrol" for OAuth2 authorization (as specified in 3GPP TS 33.501 [14]) for the entire API, and it does not define any additional scopes at resource or operation level.

Annex A (normative):   
OpenAPI specification

# A.1 General

The present Annex contains an OpenAPI [9] specification of HTTP messages and content bodies used by the Nchf\_SpendingLimitControl Service API.

This Annex shall take precedence when being discrepant to other parts of the specification with respect to the encoding of information elements and methods within the API.

NOTE: The semantics and procedures, as well as conditions, e.g. for the applicability and allowed combinations of attributes or values, not expressed in the OpenAPI definitions but defined in other parts of the specification also apply.

Informative copies of the OpenAPI specification file contained in this 3GPP Technical Specification are available on a Git-based repository that uses the GitLab software version control system (see clause 5B of the 3GPP TR 21.900 [17] and clause 5.3.1 of the 3GPP TS 29.501 [5] for further information).

# A.2 Nchf\_SpendingLimitControl Service API

openapi: 3.0.0

info:

version: 1.3.0-alpha.2

title: Nchf\_SpendingLimitControl

description: |

Nchf Spending Limit Control Service.

© 2023, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

externalDocs:

description: 3GPP TS 29.594 V18.3.0; 5G System; Spending Limit Control Service.

url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.594/'

servers:

- url: '{apiRoot}/nchf-spendinglimitcontrol/v1'

variables:

apiRoot:

default: https://example.com

description: apiRoot as defined in clause 4.4 of 3GPP TS 29.501

security:

- {}

- oAuth2ClientCredentials:

- nchf-spendinglimitcontrol

paths:

/subscriptions:

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/SpendingLimitContext'

responses:

'201':

description: Success

content:

application/json:

schema:

$ref: '#/components/schemas/SpendingLimitStatus'

headers:

Location:

description: >

Contains the URI of the created individual spending limit resource,

according to the structure

{apiRoot}/nchf-spendinglimitcontrol/v1/subscriptions/{subscriptionId}

required: true

schema:

type: string

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

callbacks:

statusNotification:

'{$request.body#/notifUri}/notify':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/SpendingLimitStatus'

responses:

'204':

description: No Content, Notification was succesfull

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

subscriptionTermination:

'{$request.body#/notifUri}/terminate':

post:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/SubscriptionTerminationInfo'

responses:

'204':

description: No Content, Notification was succesfull

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

/subscriptions/{subscriptionId}:

parameters:

- in: path

name: subscriptionId

description: Identifies an individual spending limit retrieval subscription.

required: true

schema:

type: string

put:

requestBody:

required: true

content:

application/json:

schema:

$ref: '#/components/schemas/SpendingLimitContext'

responses:

'200':

description: OK. Resource was succesfully modified and representation is returned

content:

application/json:

schema:

$ref: '#/components/schemas/SpendingLimitStatus'

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'411':

$ref: 'TS29571\_CommonData.yaml#/components/responses/411'

'413':

$ref: 'TS29571\_CommonData.yaml#/components/responses/413'

'415':

$ref: 'TS29571\_CommonData.yaml#/components/responses/415'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

delete:

responses:

'204':

description: No Content. Resource was succesfully deleted

'307':

$ref: 'TS29571\_CommonData.yaml#/components/responses/307'

'308':

$ref: 'TS29571\_CommonData.yaml#/components/responses/308'

'400':

$ref: 'TS29571\_CommonData.yaml#/components/responses/400'

'401':

$ref: 'TS29571\_CommonData.yaml#/components/responses/401'

'403':

$ref: 'TS29571\_CommonData.yaml#/components/responses/403'

'404':

$ref: 'TS29571\_CommonData.yaml#/components/responses/404'

'429':

$ref: 'TS29571\_CommonData.yaml#/components/responses/429'

'500':

$ref: 'TS29571\_CommonData.yaml#/components/responses/500'

'502':

$ref: 'TS29571\_CommonData.yaml#/components/responses/502'

'503':

$ref: 'TS29571\_CommonData.yaml#/components/responses/503'

default:

$ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

nchf-spendinglimitcontrol: Access to the Nchf\_SpendingLimitControl API

schemas:

SpendingLimitContext:

description: >

Represents the subscription data structure required for an individual CHF spending limit

subscription.

type: object

properties:

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

gpsi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

policyCounterIds:

type: array

items:

$ref: '#/components/schemas/PolicyCounterId'

minItems: 1

description: >

This is a list of policy counter identifier(s), which identifies policy counters

maintained per subscriber within the CHF.

notifUri:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

expiry:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

notifId:

type: string

SpendingLimitStatus:

description: >

Represents the data structure presenting the statuses of policy counters.

type: object

properties:

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

notifId:

type: string

statusInfos:

type: object

additionalProperties:

$ref: '#/components/schemas/PolicyCounterInfo'

minProperties: 1

description: >

Status of the requested policy counters. The key of the map is the attribute

"policyCounterId".

expiry:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

supportedFeatures:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

PolicyCounterInfo:

description: Represents the data structure presenting the policy counter status.

type: object

properties:

policyCounterId:

$ref: '#/components/schemas/PolicyCounterId'

currentStatus:

type: string

description: >

Identifies the policy counter status applicable for a specific policy counter identified

by the policyCounterId. The values (e.g. valid, invalid or any other status) are not

specified. The interpretation and actions related to the defined values are out of scope

of 3GPP.

penPolCounterStatuses:

type: array

items:

$ref: '#/components/schemas/PendingPolicyCounterStatus'

minItems: 1

description: Provides the pending policy counter status.

required:

- policyCounterId

- currentStatus

PendingPolicyCounterStatus:

description: >

Represents the data structure presenting the pending policy counter status.

type: object

properties:

policyCounterStatus:

type: string

description: >

Identifies the policy counter status applicable for a specific policy counter identified

by the policyCounterId. The values (e.g. valid, invalid or any other status) are not

specified. The interpretation and actions related to the defined values are out of scope

of 3GPP.

activationTime:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

required:

- policyCounterStatus

- activationTime

PolicyCounterId:

type: string

description: Identifies a policy counter.

SubscriptionTerminationInfo:

description: >

Represents the data structure presenting the indication of the termination of the

subscription.

type: object

properties:

supi:

$ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

notifId:

type: string

termCause:

$ref: '#/components/schemas/TerminationCause'

required:

- supi

# Simple data types and Enumerations

TerminationCause:

anyOf:

- type: string

enum:

- REMOVED\_SUBSCRIBER

- type: string

description: >

This string provides forward-compatibility with future extensions to the enumeration

and is not used to encode content defined in the present version of this API.

description: |

Represents the cause for requesting the termination of the subscription to policy counter

status changes.

Possible values are:

- REMOVED\_SUBSCRIBER: The subscriber identified by the SUPI has been removed from the CHF.

Annex B (normative):   
5GC and EPC interworking scenario support

# B.1 Scope

This annex defines procedures for the Nchf\_SpendingLimitControl service for 5GC and EPC interworking scenarios specified in clause B.1 of 3GPP TS 29.512 [18].

# B.2 Nchf\_SpendingLimitControl Service

## B.2.1 Service Description

### B.2.1.1 Overview

The overview in clause 4.1.1 applies.

### B.2.1.2 Service Architecture

The architecture in clause 4.1.2 applies.

# B.3 Service Operation

## B.3.1 Introduction

The service operations defined in clause 4.2 shall be applicable.

## B.3.2 Nchf\_SpendingLimitControl\_Subscribe Service Operation

Clause 4.2.2.2 and clause 4.2.2.3 are applied with the differences that the NF service consumers (e.g. PCF) shall include (if available) in SpendingLimitContext data structure:

- the IMSI of the user within the "supi" attribute;

- the MSISDN of the user within the "gpsi" attribute;

## B.3.3 Nchf\_SpendingLimitControl\_Unsubscribe Service Operation

Clause 4.2.3 applies.

## B.3.4 Nchf\_SpendingLimitControl\_Notify Service Operation

Clause 4.2.4 applies.

Annex C (normative):  
Wireless and wireline convergence access support

# C.1 Scope

This annex defines procedures for wireless and wireline convergence access support for 5GS. The specific stage 2 definition and related procedures are contained in 3GPP TS 23.316 [19]. The System Architecture for wireless and wireline convergence access is defined in 3GPP TS 23.501 [2].

# C.2 Nchf\_SpendingLimitControl Service

## C.2.1 Service Description

### C.2.1.1 Overview

Clause 4.1.1 applies with the following exceptions:

- the UE is replaced by the 5G-RG and the W-AGF, which is acting as a UE towards the 5GC on behalf of the FN-RG; and

- roaming is only applicable to a 5G-RG connecting to the 5GC via NG RAN, i.e., the H-PCF interaction with the H-CHF for the home-routed scenario only applies to a 5G-RG connecting to the 5GC via NG RAN.

### C.2.1.2 Service Architecture

The architecture in clause 4.1.2 applies.

# C.3 Service Operation

## C.3.1 Introduction

The service operations defined in clause 4.2.1 apply.

## C.3.2 Nchf\_SpendingLimitControl\_Subscribe Service Operation

### C.3.2.1 General

Clauses 4.2.2.2 and 4.2.2.3 are applied with the differences that the NF service consumer shall include (if available) in SpendingLimitContext data structure:

- a IMSI or a Global Cable Identifier (GCI) or a Global Line Identifier (GLI) as specified in 3GPP TS 23.316 [19] clause 4.7, encoded as specified in 3GPP TS 29.571[11], clause 5.3.2, within the "supi" attribute.

## C.3.3 Nchf\_SpendingLimitControl\_Unsubscribe Service Operation

Clause 4.2.3 applies.

## C.3.4 Nchf\_SpendingLimitControl\_Notify Service Operation

Clause 4.2.4 applies.

Annex D (informative):   
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Date** | **TSG #** | **TSG Doc.** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New** |
| 2018-04 |  |  |  |  |  | TS skeleton of Spending Limit Control Service specification | 0.0.0 |
| 2018-04 | CT3#96 |  |  |  |  | Inclusion of documents agreed in CT3#96: C3-182160, C3-182161, C3-182167, C3-182432, C3-182433, C3-182434, C3-182435, C3-182436, C3-182437, C3-182479 | 0.1.0 |
| 2018-05 | CT3#97 |  |  |  |  | Inclusion of documents agreed in CT3#97: C3-183138, C3-183288, C3-183538, C3-183539, C3-183541, C3-183543, C3-183544, C3-183545, C3-183546, C3-183547, C3-183548, C3-183550, C3-183552, C3-183780, C3-183782, C3-183830, C3-183831 | 0.2.0 |
| 2018-06 | CT#80 | CP-181026 |  |  |  | TS sent for approval to TSG | 1.0.0 |
| 2018-06 | CT#80 | CP-181026 |  |  |  | TS approved by plenary | 15.0.0 |
| 2018-09 | CT#81 | CP-182015 | 0001 | 1 | F | Removal of possibility of confusion related to 3GPP TS 29.513, custom headers, verbal forms and OpenAPI corrections | 15.1.0 |
| 2018-09 | CT#81 | CP-182221 | 0002 | 4 | F | Introduction of the simple data type "policyCounterId" | 15.1.0 |
| 2018-09 | CT#81 | CP-182098 | 0003 | 3 | F | Update and corrections of the data model | 15.1.0 |
| 2018-09 | CT#81 | CP-182015 | 0004 | 2 | F | Integration of error handling | 15.1.0 |
| 2018-09 | CT#81 | CP-182015 | 0007 | - | F | ED – Continuous reporting and policy counter status change | 15.1.0 |
| 2018-09 | CT#81 | CP-182099 | 0008 | 3 | F | Termination of the subscription of status changes for all policy counters by CHF | 15.1.0 |
| 2018-12 | CT#82 | CP-183205 | 0009 | - | F | Application of resource illustration rule | 15.2.0 |
| 2018-12 | CT#82 | CP-183205 | 0010 | - | F | Consolidation of the term "notificationUri" | 15.2.0 |
| 2018-12 | CT#82 | CP-183205 | 0011 | - | F | Clarification of "intermediate spending limit report retrieval" usage | 15.2.0 |
| 2018-12 | CT#82 | CP-183205 | 0012 | - | F | Correction of wrong reference for supi in OpenAPI doc | 15.2.0 |
| 2018-12 | CT#82 | CP-183205 | 0013 | - | F | Correction of the originator for application error responses | 15.2.0 |
| 2018-12 | CT#82 | CP-183205 | 0014 | 1 | F | Application of externalDocs field in OpenAPI doc | 15.2.0 |
| 2018-12 | CT#82 | CP-183205 | 0015 | 1 | F | Application of version pattern rule in OpenAPI doc | 15.2.0 |
| 2018-12 | CT#82 | CP-183205 | 0016 | 1 | F | Corrections to OpenAPI file | 15.2.0 |
| 2018-12 | CT#82 | CP-183205 | 0017 | - | F | Default value for apiRoot | 15.2.0 |
| 2018-12 | CT#82 | CP-183205 | 0018 | - | F | Cardinality | 15.2.0 |
| 2018-12 | CT#82 | CP-183205 | 0019 | 2 | F | Sending of GPSI (MSISDN) in Initial Spenidng Limit retrieval | 15.2.0 |
| 2018-12 | CT#82 | CP-183205 | 0020 | 1 | F | Update of content types | 15.2.0 |
| 2018-12 | CT#82 | CP-183205 | 0021 | 1 | F | Authorization of NF service access by OAuth 2.0 | 15.2.0 |
| 2018-12 | CT#82 | CP-183205 | 0022 | 1 | F | Introduction of status code 404 Not Found as mandatory status code and missing ones | 15.2.0 |
| 2018-12 | CT#82 | CP-183205 | 0023 | 1 | F | Location Header | 15.2.0 |
| 2018-12 | CT#82 | CP-183205 | 0024 | 2 | F | Correcting application error | 15.2.0 |
| 2019-03 | CT#83 | CP-190113 | 0025 | 1 | F | Correction of Resource URI | 15.3.0 |
| 2019-03 | CT#83 | CP-190113 | 0026 | 1 | F | Correction relating to the introduction of the General Public Subscription Identifier | 15.3.0 |
| 2019-03 | CT#83 | CP-190068 | 0027 | 2 | F | OpenAPI info version update | 15.3.0 |
| 2019-03 | CT#83 | CP-190067 | 0028 | - | F | Correction of wrong usage of key word "items" | 15.3.0 |
| 2019-06 | CT#84 | CP-191189 | 0030 | 3 | F | Precedence of OpenAPI file | 15.4.0 |
| 2019-06 | CT#84 | CP-191189 | 0031 | 1 | F | Copyright Note in YAML file | 15.4.0 |
| 2019-06 | CT#84 | CP-191189 | 0033 | - | F | OpenAPI version number update | 15.4.0 |
| 2019-06 | CT#84 | CP-191089 | 0032 | 1 | B | Race Condition handling | 16.0.0 |
| 2019-09 | CT#85 | CP-192151 | 0035 | - | A | NF service consumer pending policy counter handling | 16.1.0 |
| 2019-09 | CT#85 | CP-192156 | 0036 | 1 | B | Support of Expiry Time | 16.1.0 |
| 2019-09 | CT#85 | CP-192151 | 0038 | - | A | Correction to Subscription Termination service operation | 16.1.0 |
| 2019-09 | CT#85 | CP-192151 | 0040 | - | A | Correction to subscription creation/update response | 16.1.0 |
| 2019-09 | CT#85 | CP-192151 | 0042 | - | A | Corrections to subscription request descriptions | 16.1.0 |
| 2019-09 | CT#85 | CP-192151 | 0044 | - | A | Handling of unknown policy counters | 16.1.0 |
| 2019-09 | CT#85 | CP-192173 | 0045 | - | F | OpenAPI version update for TS 29.594 Rel-16 | 16.1.0 |
| 2020-06 | CT#88e | CP-201233 | 0046 | - | F | Description of "activationTime" attribute | 16.2.0 |
| 2020-06 | CT#88e | CP-201233 | 0047 | - | F | Miscellaneous corrections | 16.2.0 |
| 2020-06 | CT#88e | CP-201244 | 0048 | 1 | F | Storage of YAML files in ETSI Forge | 16.2.0 |
| 2020-06 | CT#88e | CP-201256 | 0049 | 1 | F | URI of the Nchf\_SpendingLimitControl service | 16.2.0 |
| 2020-06 | CT#88e | CP-201244 | 0050 | 1 | F | Optionality of ProblemDetails | 16.2.0 |
| 2020-06 | CT#88e | CP-201244 | 0052 | 1 | F | Supported headers, Resource Data type | 16.2.0 |
| 2020-06 | CT#88e | CP-201255 | 0053 | - | F | Update of OpenAPI version and TS version in externalDocs field | 16.2.0 |
| 2020-09 | CT#89e | CP-202058 | 0056 | 1 | A | Correction to spending limit subscribe and unsubscribe procedures | 16.3.0 |
| 2020-09 | CT#89e | CP-202058 | 0058 | 1 | A | Nchf\_SpendingLimitControl Service support of interworking | 16.3.0 |
| 2020-12 | CT#90e | CP-203139 | 0061 | 1 | F | Essential corrections and alignments | 16.4.0 |
| 2020-12 | CT#90e | CP-203139 | 0062 | 1 | F | Storage of YAML files in 3GPP Forge | 16.4.0 |
| 2020-12 | CT#90e | CP-203122 | 0064 | 1 | A | Correction to Intermediate spending limit report retrieval | 16.4.0 |
| 2020-12 | CT#90e | CP-203128 | 0065 | - | F | Correction to subscription's expiry time | 16.4.0 |
| 2020-12 | CT#90e | CP-203128 | 0066 | 1 | F | Correction to subscription create service operation | 16.4.0 |
| 2020-12 | CT#90e | CP-203152 | 0068 | - | F | Update of OpenAPI version and TS version in externalDocs field | 16.4.0 |
| 2021-03 | CT#91e | CP-210191 | 0070 | 2 | F | Support of stateless NFs | 16.5.0 |
| 2021-03 | CT#91e | CP-210202 | 0071 | 2 | F | Correction to Wireline Access information | 16.5.0 |
| 2021-03 | CT#91e | CP-210226 | 0072 | 1 | F | Definition addition to TS29.594 | 17.0.0 |
| 2021-03 | CT#91e | CP-210219 | 0073 | 1 | F | Optional header clearification | 17.0.0 |
| 2021-03 | CT#91e | CP-210221 | 0075 | 1 | F | Adding some missing description fields to data type definitions in OpenAPI | 17.0.0 |
| 2021-03 | CT#91e | CP-210221 | 0076 | 1 | F | Ambiguous concept of NF service consumer terminology | 17.0.0 |
| 2021-03 | CT#91e | CP-210220 | 0077 | - | F | OpenAPI reference | 17.0.0 |
| 2021-03 | CT#91e | CP-210240 | 0079 | - | F | Update of OpenAPI version and TS version in externalDocs field | 17.0.0 |
| 2021-06 | CT#92e | CP-211210 | 0082 | 1 | A | Correction to policyCounterId | 17.1.0 |
| 2021-06 | CT#92e | CP-211219 | 0084 | 1 | A | Correction to expiry time | 17.1.0 |
| 2021-06 | CT#92e | CP-211219 | 0086 | 1 | A | Correction to notification correlation id | 17.1.0 |
| 2021-06 | CT#92e | CP-211219 | 0090 | 1 | A | Correction to the termination procedure | 17.1.0 |
| 2021-06 | CT#92e | CP-211200 | 0092 | 1 | A | Temporary and Permanent Redirection | 17.1.0 |
| 2021-06 | CT#92e | CP-211265 | 0094 | - | F | Update of OpenAPI version and TS version in externalDocs field | 17.1.0 |
| 2021-09 | CT#93e | CP-212220 | 0095 | 1 | F | Correction of URI structure | 17.2.0 |
| 2022-03 | CT#95e | CP-220176 | 0096 | 2 | A | Alignment of "Application Errors" clause with SBI TS template | 17.3.0 |
| 2022-06 | CT#96 | CP-221154 | 0098 | 1 | F | Formatting of description fields | 17.4.0 |
| 2022-06 | CT#96 | CP-221152 | 0099 | - | F | Update of info and externalDocs fields | 17.4.0 |
| 2022-09 | CT#97e | CP-222123 | 0100 | - | F | Alignment with the SBI template | 17.5.0 |
| 2022-12 | CT#98e | CP-223191 | 0101 | - | F | Adding the mandatory error code 502 Bad Gateway | 18.0.0 |
| 2022-12 | CT#98e | CP-223192 | 0102 | 1 | F | TerminationCause enumeration definition in the OpenAPI file | 18.0.0 |
| 2022-12 | CT#98e | CP-223190 | 0103 | - | F | Update of info and externalDocs fields | 18.0.0 |
| 2023-06 | CT#100 | CP-231132 | 0104 | 1 | F | HTTP redirection clause correction | 18.1.0 |
| 2023-09 | CT#101 | CP-232099 | 0105 | 1 | B | Clarification on Spending Limit Control Service | 18.2.0 |
| 2023-12 | CT#102 | CP-233230 | 0108 | 1 | F | Update HTTP RFC 7807 obsoleted by IETF RFC 9457 | 18.3.0 |
| 2023-12 | CT#102 | CP-233230 | 0109 | 1 | F | Corrections to the description fields of the enumerations | 18.3.0 |
| 2023-12 | CT#102 | CP-233238 | 0110 | - | F | Update of info and externalDocs fields | 18.3.0 |